<div align=center>
<img src="https://github.com/BestModules-Libraries/img/blob/main/BMV31T001_V1.0.png" width="320" height="240"> 
</div> 

BMV31T001
===========================================================

The BMV31T001 is a voice playback shield from Best Modules, which uses the one-wire communication to implement the playback control. This document provides the description of the BMV31T001 Arduino Lib functions and how to install the Arduino Lib. The example demonstrates the online voice source update and voice play operation.

This library can be installed via the Arduino Library manager. Search for **BMV31T001**. 

Repository Contents
-------------------

* **/examples** - Example sketches for the library (.ino). Run these from the Arduino IDE. 
* **/src** - Source files for the library (.cpp, .h).
* **keywords.txt** - Keywords from this library that will be highlighted in the Arduino IDE. 
* **library.properties** - General library properties for the Arduino package manager. 

Documentation 
-------------------

* **[BMV31T001 Arduino Library V1.0.1 Description v100]( https://www.bestmodulescorp.com/bmv31t001.html#tab-product2 )** - Arduino Library Description.

Version History  
-------------------

* **V1.0.1** - Initial public release.

License Information
-------------------

This product is _**open source**_! 

Please review the LICENSE.md file for license information. 

If you have any questions or concerns on licensing, please contact technical support on our BESTMODULES Email:service@bestmodulescorp.com

Distributed as-is; no warranty is given.

BESTMODULES
