<div align=center>
<img src="https://github.com/BestModules-Libraries/img/blob/main/BMV51T001_V1.0.png" width="320" height="240"> 
</div> 


BMV51T001
===========================================================

The BMV51T001 is a MIDI tone library shield with wavetable synthesis from Best Modules, which uses the UART communication method to transmit and receive commands. This document provides the description of the BMV51T001 Arduino Lib functions and how to install the Arduino Lib. The example demonstrates the keyboard and hit functions, as well as MIDI audio play function.

This library can be installed via the Arduino Library manager. Search for **BMV51T001**. 

Repository Contents
-------------------

* **/examples** - Example sketches for the library (.ino). Run these from the Arduino IDE. 
* **/src** - Source files for the library (.cpp, .h).
* **keywords.txt** - Keywords from this library that will be highlighted in the Arduino IDE. 
* **library.properties** - General library properties for the Arduino package manager. 

Documentation 
-------------------

* **[BMV51T001 Arduino Library]( https://www.bestmodulescorp.com/bmv51t001.html#tab-product2 )** - Arduino Library Description.

Version History  
-------------------

* **V1.0.1**  
&emsp;&emsp;- Initial public release.  
* **V1.0.2**   
&emsp;&emsp;- Perfect some function header comments.

License Information
-------------------

This product is _**open source**_! 

Please review the LICENSE.md file for license information. 

If you have any questions or concerns on licensing, please contact technical support on our BEST MODULES CORP. Email:service@bestmodulescorp.com

Distributed as-is; no warranty is given.

BEST MODULES CORP.
