# Arduino Library for Bridgetek FT800 and FT801

[Back](../README.md)

This library is to provide an API to control the Bridgetek FT800 and FT801 devices. It implements EVE API 1.

The class name of the library is "Bridgetek_EVE1".

The library provides an Arduino IDE interface to the EVE embedded development library [EVE-MCU-Dev](https://github.com/Bridgetek/Eve-MCU-Dev).
It is programmed in the same way with minor changes and ensures that code is easily transferrable.

The example code is set to the WQVGA display resolution.

## Contents

- [Hardware](#hardware)
- [Using the Library](#using-the-library)
- [Programming Guide](#programming-guide)
  - [Library API](#library-api)
  - [Library Constants](#library-constants)
- [Examples](#examples)
  - [Arduino IDE Examples](#arduino-ide-examples)
- [Module Connections](#module-connections)
  - [Through-Board 2x8 Pins](#through-board-2x8-pins)
  - [Header 1x10 Pins](#header-1x10-pins)
  - [Arduino Connection](#arduino-connection)

## Hardware

The Arduino port was developed using an Arduino Zero and Arduino Leonardo. The Arduino module can be connected via short wires to the corresponding signals of an EVE module. Please reference the Arduino Datasheet for more information.

| Arduino Name | Arduino Pin | EVE Signal |
| --- | --- | --- |
| SCLK | ISCP 3 | SCK |
| COPI | ISCP 4 | MOSI |
| CIPO | ISCP 1 | MISO |
| D10 | PB6 | CS# |
| D9 | PB5 | PD# |
| - | ISCP 2 | 5V |
| - | ISCP 6 / GND | GND |

If using the 5V power from the Arduino ensure that the power supply from the Arduino module
is capable of also powering the EVE board. If using third-party modules which may consume
more current, a separate power connection to the EVE module could be used, with the grounds
of the Arduino and EVE modules common to both power sources.

## Using the Library

The library can be added to a sketch by including the lines in the example below. This example
is for the API 1 library for FT800 and FT801,
the number corresponds to the API.

The sketch must include the following code:

```
#include <BridgetekEVE1.h>

Bridgetek_EVE1 eve;

void setup(){
  eve.setup(WVGA);
  eve.Init()
}
```

The `#include <BridgetekEVE1.h>` line will add in the header for this
library and the declarations and constants included in the library API.

The `Bridgetek_EVE1 eve` creates a class for the library which is required to direct
accesses to the EVE device to the library.

The `eve.setup(WVGA)` command initialises the library to use a WVGA display which is
800 by 480 pixels.

Finally, `eve.Init()` calls the library and initialises the SPI interface to the EVE
device and then configures the EVE device for use. Once this command is complete the
EVE device is usable for creating displays using co-processor commands via the library's
API.

Display lists can be generated through the co-processor in the same way as they are in
[EVE-MCU-Dev](https://github.com/Bridgetek/Eve-MCU-Dev), the display list entries and
  co-processor commands are added using calls to the library API.

## Programming Guide

The latest Programming Guide for the FT800 and FT801 can be found on the
[Bridgetek Programming Guides](https://brtchip.com/document/programming-guides/) page.

This covers the command set implemented by the device and methods for acheiving the
desired output on the screen.

### Co-Processor Helpers

These functions perform the necessary tasks to begin and execute co-processor lists.

`void LIB_BeginCoProList(void)`

Puts Chip Select low and sends the starting address of the RAM_CMD location where the
commands will be written. Chip Select remains low.

`void LIB_EndCoProList(void)`

Brings Chip Select high to end the burst and ensures that the co-processor will execute
the newly added commands.

`void LIB_AwaitCoProEmpty(void)`

Waits for the completion of the current commands sent to the co-processor.

### Creating screens and executing commands

The API Layer provides functions to begin and end lists of co-processor commands. The co-processor
commands must be preceeded and followed by co-processor management functions.

#### Writing DL Instructions and Co-Processor Commands

Using EVE commands via the co-processor requires some data formatting to convert the parameters of the
command into the correct hex values to be sent as well as keeping track of the number of bytes sent to
update the write pointer correctly. Some commands also require padding to make their total size including
parameters a multiple of 4 bytes. The functions in the library hide this from the main application.

#### Beginning and Ending Co-Processor Lists

All co-processor lists must begin with a call to `LIB_BeginCoProList()`.
If any display list items or co-processor commands which use the display list are to be added then a
call to `CMD_DLSTART()` is required immediately after this.

For the avoidance of doubt, commands that only read or write registers, read or write memory, access
flash or access the SD card do not require the `CMD_DLSTART()` call.

All co-processor lists displaying graphics would be preceeded by:
```
    eve.LIB_BeginCoProList(); // CS low and send address in RAM_CMD
    eve.CMD_DLSTART(); // When executed, EVE will begin a new DL
```
And followed by:
```
    eve.LIB_EndCoProList(); // CS high
    eve.LIB_AwaitCoProEmpty(); // Wait for FIFO to be finish
```
A call to `LIB_AwaitCoProEmpty()` is implied in the call to `LIB_BeginCoProList()`. Therefore
it is not necessary to wait at the end of the co-processor
list for the completion of the commands allowing program to perform other tasks not related to
programming the EVE device.

#### Simple Co-Pocessor List

The following is a simple list to write text on the screen in white letters:

```
    eve.LIB_BeginCoProList(); // CS low and send address in RAM_CMD
    eve.CMD_DLSTART(); // When executed, EVE will begin a new DL

    eve.CLEAR_COLOR_RGB(0, 0, 0); // Select colour to clear screen to
    eve.CLEAR(1,1,1); // Clear screen

    eve.COLOR_RGB(255, 255, 255);
    eve.CMD_TEXT(100, 100, 28, eve.OPT_CENTERX | eve.OPT_CENTERY, "Hello");

    eve.DISPLAY(); // Tells EVE that this is the end
    eve.CMD_SWAP(); // Swaps new list into foreground buffer
    eve.LIB_EndCoProList(); // CS high and end list
    eve.LIB_AwaitCoProEmpty(); // Wait for FIFO to be empty
    // (commands executed)
```

#### Executing a Single Co-Processor Command

When just executing a co-processor command (for example calling CMD_SETROTATE during set-up
of the application to set the screen orientation) then the following can be used:

```
    eve.LIB_BeginCoProList(); // CS low and send address in RAM_CMD
    eve.CMD_DLSTART(); // When executed, EVE will begin a new DL

    eve.CMD_SETROTATE(2);

    eve.LIB_EndCoProList(); // CS high
    eve.LIB_AwaitCoProEmpty(); // Wait for FIFO to be finish
```

### Library API

This library functions provide an API for sending commands to the device and receiving results and
status from a sketch.

API calls in a sketch to this library call an equivalent function in the [EVE-MCU-Dev](https://github.com/Bridgetek/Eve-MCU-Dev) API.
Each API function in this library maps to a function with a prefix `EVE_` in the EVE-MCU-Dev library.
Therefore, taking `eve` as the name of the library class in a sketch, calling the function
`eve.CMD_SWAP()` will call the function `EVE_CMD_SWAP()` in EVE-MCU-Dev.

The full API available to the Arduino IDE is as follows:

```
int LIB_AwaitCoProEmpty(void)
uint16_t LIB_MemRead16(uint32_t address)
uint16_t LIB_SendString(const char* string)
uint32_t LIB_GetResult(int offset)
uint32_t LIB_MemRead32(uint32_t address)
uint8_t LIB_MemRead8(uint32_t address)
void LIB_BeginCoProList(void)
void LIB_EndCoProList(void)
void LIB_GetMatrix(uint32_t *a,  uint32_t *b,  uint32_t *c,  uint32_t *d,  uint32_t *e,  uint32_t *f)
void LIB_GetProps(uint32_t *addr,  uint32_t *width,  uint32_t *height)
void LIB_GetPtr(uint32_t *addr)
void LIB_MemCrc(uint32_t ptr,  uint32_t num,  uint32_t *result)
void LIB_MemWrite16(uint32_t addr,  uint16_t value)
void LIB_MemWrite32(uint32_t addr,  uint32_t value)
void LIB_MemWrite8(uint32_t addr,  uint8_t value)
void LIB_ReadDataFromRAMG(uint8_t *ImgData,  uint32_t DataSize,  uint32_t SrcAddress)
void LIB_WriteDataToCMD(const uint8_t *ImgData,  uint32_t DataSize)
void LIB_WriteDataToRAMG(const uint8_t *ImgData,  uint32_t DataSize,  uint32_t DestAddress)

void CMD_APPEND(uint32_t ptr,  uint32_t num)
void CMD_BGCOLOR(uint32_t c)
void CMD_BITMAP_TRANSFORM(int32_t x0,  int32_t y0,  int32_t x1,  int32_t y1,  int32_t x2,  int32_t y2,  int32_t tx0,  int32_t ty0,  int32_t tx1,  int32_t ty1,  int32_t tx2,  int32_t ty2,  uint16_t result)
void CMD_BUTTON(int16_t x,  int16_t y,  int16_t w,  int16_t h,  int16_t font,  uint16_t options,  const char* string, ...)
void CMD_CALIBRATE(uint32_t result)
void CMD_CLOCK(int16_t x,  int16_t y,  int16_t r,  uint16_t options,  uint16_t h,  uint16_t m,  uint16_t s,  uint16_t ms)
void CMD_COLDSTART(void)
void CMD_DIAL(int16_t x,  int16_t y,  int16_t r,  uint16_t options,  uint16_t val)
void CMD_DLSTART(void)
void CMD_FGCOLOR(uint32_t c)
void CMD_GAUGE(int16_t x,  int16_t y,  int16_t r,  uint16_t options,  uint16_t major,  uint16_t minor,  uint16_t val,  uint16_t range)
void CMD_GETMATRIX(int32_t a,  int32_t b,  int32_t c,  int32_t d,  int32_t e,  int32_t f)
void CMD_GETPROPS(uint32_t ptr,  uint32_t w,  uint32_t h)
void CMD_GETPTR(uint32_t result)
void CMD_GRADCOLOR(uint32_t c)
void CMD_GRADIENT(int16_t x0,  int16_t y0,  uint32_t rgb0,  int16_t x1,  int16_t y1,  uint32_t rgb1)
void CMD_INFLATE(uint32_t ptr)
void CMD_INTERRUPT(uint32_t ms)
void CMD_KEYS(int16_t x,  int16_t y,  int16_t w,  int16_t h,  int16_t font,  uint16_t options,  const char* string)
void CMD_LOADIDENTITY(void)
void CMD_LOADIMAGE(uint32_t ptr,  uint32_t options)
void CMD_LOGO(void)
void CMD_MEMCPY(uint32_t dest,  uint32_t src,  uint32_t num)
void CMD_MEMCRC(uint32_t ptr,  uint32_t num,  uint32_t result)
void CMD_MEMSET(uint32_t ptr,  uint32_t value,  uint32_t num)
void CMD_MEMWRITE(uint32_t ptr,  uint32_t num)
void CMD_MEMZERO(uint32_t ptr,  uint32_t num)
void CMD_NUMBER(int16_t x,  int16_t y,  int16_t font,  uint16_t options,  int32_t n)
void CMD_PROGRESS(int16_t x,  int16_t y,  int16_t w,  int16_t h,  uint16_t options,  uint16_t val,  uint16_t range)
void CMD_REGREAD(uint32_t ptr,  uint32_t result)
void CMD_ROTATE(int32_t a)
void CMD_SCALE(int32_t sx,  int32_t sy)
void CMD_SCREENSAVER(void)
void CMD_SCROLLBAR(int16_t x,  int16_t y,  int16_t w,  int16_t h,  uint16_t options,  uint16_t val,  uint16_t size,  uint16_t range)
void CMD_SETFONT(uint32_t font,  uint32_t ptr)
void CMD_SETMATRIX(void)
void CMD_SKETCH(int16_t x,  int16_t y,  uint16_t w,  uint16_t h,  uint32_t ptr,  uint16_t format)
void CMD_SLIDER(int16_t x,  int16_t y,  int16_t w,  int16_t h,  uint16_t options,  uint16_t val,  uint16_t range)
void CMD_SNAPSHOT(uint32_t ptr)
void CMD_SPINNER(int16_t x,  int16_t y,  uint16_t style,  uint16_t scale)
void CMD_STOP(void)
void CMD_SWAP(void)
void CMD_TEXT(int16_t x,  int16_t y,  int16_t font,  uint16_t options,  const char* string, ...)
void CMD_TOGGLE(int16_t x,  int16_t y,  int16_t w,  int16_t font,  uint16_t options,  uint16_t state,  const char* string, ...)
void CMD_TRACK(int16_t x,  int16_t y,  int16_t w,  int16_t h,  int16_t tag)
void CMD_TRANSLATE(int32_t tx,  int32_t ty)


void ALPHA_FUNC(uint8_t func,  uint8_t ref)
void BEGIN(uint8_t prim)
void BITMAP_HANDLE(uint8_t handle)
void BITMAP_LAYOUT(uint8_t format,  uint16_t linestride,  uint16_t height)
void BITMAP_SIZE(uint8_t filter,  uint8_t wrapx,  uint8_t wrapy,  uint16_t width,  uint16_t height)
void BITMAP_SOURCE(int32_t addr)
void BITMAP_TRANSFORM_A(long a)
void BITMAP_TRANSFORM_B(long b)
void BITMAP_TRANSFORM_C(long c)
void BITMAP_TRANSFORM_D(long d)
void BITMAP_TRANSFORM_E(long e)
void BITMAP_TRANSFORM_F(long f)
void BLEND_FUNC(uint8_t src,  uint8_t dst)
void CALL(uint16_t dest)
void CELL(uint8_t cell)
void CLEAR(uint8_t c,  uint8_t s,  uint8_t t)
void CLEAR_COLOR(uint32_t c)
void CLEAR_COLOR_A(uint8_t alpha)
void CLEAR_COLOR_RGB(uint8_t r,  uint8_t g,  uint8_t b)
void CLEAR_STENCIL(uint8_t s)
void CLEAR_TAG(uint8_t s)
void CMD(uint32_t c)
void COLOR(uint32_t c)
void COLOR_A(uint8_t alpha)
void COLOR_MASK(uint8_t r,  uint8_t g,  uint8_t b,  uint8_t a)
void COLOR_RGB(uint8_t r,  uint8_t g,  uint8_t b)
void DISPLAY(void)
void END(void)
void Init(void)
void JUMP(uint16_t dest)
void LINE_WIDTH(uint16_t width)
void MACRO(uint8_t m)
void POINT_SIZE(uint16_t size)
void RESTORE_CONTEXT(void)
void RETURN(void)
void SAVE_CONTEXT(void)
void SCISSOR_SIZE(uint16_t width,  uint16_t height)
void SCISSOR_XY(uint16_t x,  uint16_t y)
void STENCIL_FUNC(uint8_t func,  uint8_t ref,  uint8_t mask)
void STENCIL_MASK(uint8_t mask)
void STENCIL_OP(uint8_t sfail,  uint8_t spass)
void TAG(uint8_t s)
void TAG_MASK(uint8_t mask)
void VERTEX2F(int16_t x,  int16_t y)
void VERTEX2II(uint16_t x,  uint16_t y,  uint8_t handle, uint8_t cell)
```

### Library Public Variables

There are several variables that are public in the library. These can be read from a sketch.

The following variables are set depending on the panel chosen and set
```
uint32_t EVE_DISP_WIDTH
uint32_t EVE_DISP_HEIGHT
uint32_t EVE_DISP_HCYCLE
uint32_t EVE_DISP_VCYCLE
uint32_t EVE_DISP_HOFFSET
uint32_t EVE_DISP_VOFFSET
uint32_t EVE_DISP_HSYNC0
uint32_t EVE_DISP_HSYNC1
uint32_t EVE_DISP_VSYNC0
uint32_t EVE_DISP_VSYNC1
uint32_t EVE_DISP_PCLKPOL
uint32_t EVE_DISP_SWIZZLE
uint32_t EVE_DISP_CSPREAD
uint32_t EVE_DISP_DITHER
uint32_t EVE_DISP_PCLK
uint32_t EVE_DISP_PCLK_FREQ
```

If a touch controller is explicitly set in `EVE_config.h` then the following value is set. If it is
zero then the touch controller has been determined automatically by the device.

```
uint32_t EVE_TOUCH_ADDR
```

### Library Constants

In a similar way to the API functions, the library provides a set of constant values used in
sketch commands sent to the device.

Constant names in this library are mapped to constant values in the [EVE-MCU-Dev](https://github.com/Bridgetek/Eve-MCU-Dev) API.
Each constant in this library maps to a constant with a prefix `EVE_` in the EVE-MCU-Dev library.
Therefore, taking `eve` as the name of the library class in a sketch, calling the function
`eve.OPT_FILL` will call the function `EVE_OPT_FILL` in EVE-MCU-Dev.

```
ADC_DIFFERENTIAL
ADC_SINGLE_ENDED
ADPCM_SAMPLES
API
BEGIN_BITMAPS
BEGIN_EDGE_STRIP_A
BEGIN_EDGE_STRIP_B
BEGIN_EDGE_STRIP_L
BEGIN_EDGE_STRIP_R
BEGIN_LINES
BEGIN_LINE_STRIP
BEGIN_POINTS
BEGIN_RECTS
BLEND_DST_ALPHA
BLEND_ONE
BLEND_ONE_MINUS_DST_ALPHA
BLEND_ONE_MINUS_SRC_ALPHA
BLEND_SRC_ALPHA
BLEND_ZERO
DLSWAP_DONE
DLSWAP_FRAME
DLSWAP_LINE
FILTER_BILINEAR
FILTER_NEAREST
FORMAT_ARGB1555
FORMAT_ARGB2
FORMAT_ARGB4
FORMAT_BARGRAPH
FORMAT_L1
FORMAT_L4
FORMAT_L8
FORMAT_PALETTED
FORMAT_RGB332
FORMAT_RGB565
FORMAT_TEXT8X8
FORMAT_TEXTVGA
INT_CMDEMPTY
INT_CMDFLAG
INT_CONVCOMPLETE
INT_PLAYBACK
INT_SOUND
INT_SWAP
INT_TAG
INT_TOUCH
LINEAR_SAMPLES
LOW_FREQ_BOUND
OPT_3D
OPT_CENTER
OPT_CENTERX
OPT_CENTERY
OPT_FLAT
OPT_MONO
OPT_NOBACK
OPT_NODL
OPT_NOHANDS
OPT_NOHM
OPT_NOPOINTER
OPT_NOSECS
OPT_NOTICKS
OPT_RGB565
OPT_RIGHTX
OPT_SIGNED
RAM_CMD
RAM_CMD_SIZE
RAM_DL
RAM_DL_SIZE
RAM_G
RAM_G_SIZE
RAM_PAL
RAM_REG
ROMFONT_FORMATS
ROMFONT_HEIGHTS
ROMFONT_MAX
ROMFONT_TABLEADDRESS
ROMFONT_WIDTHS
ROM_CHIPID
ROM_FONT
STENCIL_DECR
STENCIL_INCR
STENCIL_INVERT
STENCIL_KEEP
STENCIL_REPLACE
STENCIL_ZERO
TEST_ALWAYS
TEST_EQUAL
TEST_GEQUAL
TEST_GREATER
TEST_LEQUAL
TEST_LESS
TEST_NEVER
TEST_NOTEQUAL
TOUCHMODE_CONTINUOUS
TOUCHMODE_FRAME
TOUCHMODE_OFF
TOUCHMODE_ONESHOT
ULAW_SAMPLES
VOL_ZERO
WRAP_BORDER
WRAP_REPEAT

REG_ANALOG
REG_CLOCK
REG_CMD_DL
REG_CMD_READ
REG_CMD_WRITE
REG_CPURESET
REG_CSPREAD
REG_CTOUCH_EXTENDED
REG_CTOUCH_RAW_XY
REG_CTOUCH_TAG
REG_CTOUCH_TOUCH0_XY
REG_CTOUCH_TOUCH1_XY
REG_CTOUCH_TOUCH2_XY
REG_CTOUCH_TOUCH3_XY
REG_CTOUCH_TOUCH4_X
REG_CTOUCH_TOUCH4_Y
REG_CTOUCH_TRANSFORM_A
REG_CTOUCH_TRANSFORM_B
REG_CTOUCH_TRANSFORM_C
REG_CTOUCH_TRANSFORM_D
REG_CTOUCH_TRANSFORM_E
REG_CTOUCH_TRANSFORM_F
REG_DITHER
REG_DLSWAP
REG_FRAMES
REG_FREQUENCY
REG_GPIO
REG_GPIO_DIR
REG_HCYCLE
REG_HOFFSET
REG_HSIZE
REG_HSYNC0
REG_HSYNC1
REG_ID
REG_INT_EN
REG_INT_FLAGS
REG_INT_MASK
REG_MACRO_0
REG_MACRO_1
REG_OUTBITS
REG_PCLK
REG_PCLK_POL
REG_PLAY
REG_PLAYBACK_FORMAT
REG_PLAYBACK_FREQ
REG_PLAYBACK_LENGTH
REG_PLAYBACK_LOOP
REG_PLAYBACK_PLAY
REG_PLAYBACK_READPTR
REG_PLAYBACK_START
REG_PWM_DUTY
REG_PWM_HZ
REG_ROMSUB_SEL
REG_ROTATE
REG_SCREENSHOT_BUSY
REG_SCREENSHOT_EN
REG_SCREENSHOT_READ
REG_SCREENSHOT_START
REG_SCREENSHOT_Y
REG_SOUND
REG_SWIZZLE
REG_TAG
REG_TAG_X
REG_TAG_Y
REG_TAP_CRC
REG_TAP_MASK
REG_TOUCH_ADC_MODE
REG_TOUCH_CHARGE
REG_TOUCH_DIRECT_XY
REG_TOUCH_DIRECT_Z1Z2
REG_TOUCH_MODE
REG_TOUCH_OVERSAMPLE
REG_TOUCH_RAW_XY
REG_TOUCH_RZ
REG_TOUCH_RZTHRESH
REG_TOUCH_SCREEN_XY
REG_TOUCH_SETTLE
REG_TOUCH_TAG
REG_TOUCH_TAG_XY
REG_TOUCH_TRANSFORM_A
REG_TOUCH_TRANSFORM_B
REG_TOUCH_TRANSFORM_C
REG_TOUCH_TRANSFORM_D
REG_TOUCH_TRANSFORM_E
REG_TOUCH_TRANSFORM_F
REG_TRACK
REG_TRIM
REG_VCYCLE
REG_VOFFSET
REG_VOL_PB
REG_VOL_SOUND
REG_VSIZE
REG_VSYNC0
REG_VSYNC1
```

## Examples

A simple program for Arduino would add a set of display list items to the screen. This example
will write the phrase "Testing FT800 and FT801"
in white in the centre of a black background.

```
#include <BridgetekEVE1.h>

Bridgetek_EVE1 eve;

void setup() {
  Serial.begin(9600);
  eve.setup(WUXGA);
  eve.Init();
}

void loop() {
  // Initialise the display
  Serial.print("Starting demo...\n");
  eve.LIB_BeginCoProList();
  eve.CMD_DLSTART();
  eve.CLEAR_COLOR_RGB(0, 0, 0);
  eve.CLEAR(1,1,1);
  eve.COLOR_RGB(255, 255, 255);
  eve.CMD_TEXT(EVE_DISP_WIDTH/2, EVE_DISP_HEIGHT/2,
                28, eve.OPT_CENTERX, "Testing FT800 and FT801");
  eve.DISPLAY();
  eve.CMD_SWAP();
  eve.LIB_EndCoProList();
  eve.LIB_AwaitCoProEmpty();
}
```

### Arduino IDE Examples

The examples in this library can be used to make a new Arduino IDE sketch.
Complete example sketches added by this library can be found in "File -> Examples -> Bridgetek FT800 and FT801".

The `simple_EVE1` example is an ideal sketch to start with as it shows many
aspects of writing a sketch for Arduino. It provides exactly the same display, functions
and result as the `simple` example in [EVE-MCU-Dev](https://github.com/Bridgetek/Eve-MCU-Dev) API.

## Module Connections

There are 2 standard connectors for EVE modules used by BridgeTek.

The wiring colours in the section for each connection are defined in the following table.

| Colour | EVE Signal |
| --- | --- |
| Blue | SCK |
| Green | MOSI |
| Yellow | MISO |
| Orange | CS# |
| Red | PD# |
| Brown | GND |

### Through-Board 2x8 Pins

This connector is a through-board connector 2x8 pin with 2.54mm spacing commonly found on the "ME" range of boards. These are designed with longer pins that can be used with the MM900EVxB FT9XX boards to mount the MCU board ontop of the EVE module.

| Pin | EVE Signal | Pin | EVE Signal |
| --- | --- | --- | --- |
| 1 | N/C | 2 | N/C |
| 3 | N/C | 4 | PD# |
| 5 | GND | 6 | N/C |
| 7 | 5V | 8 | N/C |
| 9 | N/C | 10 | N/C |
| 11 | N/C | 12 | N/C |
| 13 | MOSI | 14 | MISO |
| 15 | CS# | 16 | SCK |

The 2x8 header can be connected as in the following picture.

![Wiring for 2x8 Header](header2x8.png)

### Header 1x10 Pins

This connector is the header pin connector 1x10 pin with 2.54mm spacing commonly found on the "VM" range of modules such as the VM800B, VM810C50A and VM816C50A. The connector directly mates with the VA800A-SPI board.

| Pin | EVE Signal |
| --- | --- |
| 1 | SCK |
| 2 | MOSI |
| 3 | MISO |
| 4 | CS# |
| 5 | INT# |
| 6 | PD# |
| 7 | 5V |
| 8 | N/C |
| 9 | GND |
| 10 | GND |

The 1x10 header can be connected as in the following picture.

![Wiring for 1x10 Header](header1x10.png)

### Arduino Connection

The Arduino module can be connected via short wires to the corresponding signals of an EVE module. Please reference the Arduino Datasheet for more information.

| Arduino Name | Arduino Pin | EVE Signal |
| --- | --- | --- |
| SCLK | ISCP 3 | SCK |
| COPI | ISCP 4 | MOSI |
| CIPO | ISCP 1 | MISO |
| D10 | PB6 | CS# |
| D9 | PB5 | PD# |
| - | ISCP 2 | 5V |
| - | ISCP 6 / GND | GND |

Ensure that the power supply from the Arduino module is capable of also powering the EVE board. If using third-party modules which may consume more current, a separate power connection to the EVE module could be used, with the grounds of the Beaglebone Black and EVE modules common to both power sources.

An Arduino board can be connected to an EVE board as in the following picture.

![Arduino Wiring Picture](arduino.png)
