<map id="SerialWombatQuadEnc_18AB" name="SerialWombatQuadEnc_18AB">
<area shape="rect" id="Node000001" title="Extends the SerialWombatPWM class with SW18AB specific functionality, including frequency measurement..." alt="" coords="90,264,285,291"/>
<area shape="rect" id="Node000002" href="$class_serial_wombat_quad_enc.html" title="A class that uses two Serial Wombat input pins to read quadrature encoder input." alt="" coords="5,180,162,207"/>
<area shape="poly" id="edge1_Node000001_Node000002" title=" " alt="" coords="113,214,173,261,170,266,109,218"/>
<area shape="rect" id="Node000003" href="$class_serial_wombat_pin.html" title="Describes a Serial Wombat Pin. Is base class for other pin modes." alt="" coords="23,96,144,123"/>
<area shape="poly" id="edge2_Node000002_Node000003" title=" " alt="" coords="86,138,86,180,81,180,81,138"/>
<area shape="rect" id="Node000004" href="$class_serial_wombat_chip.html" title="Class for a Serial Wombat chip. Each Serial Wombat chip on a project should have its own instance." alt="" coords="19,5,148,32"/>
<area shape="poly" id="edge3_Node000003_Node000004" title=" " alt="" coords="86,48,86,95,81,95,81,48"/>
<area shape="rect" id="Node000005" href="$class_serial_wombat_abstract_processed_input.html" title="SerialWombatAnalogInput, SerialWombatPulseTimer, SerialWombatResistanceInput and others inherit from ..." alt="" coords="186,172,400,215"/>
<area shape="poly" id="edge4_Node000001_Node000005" title=" " alt="" coords="256,226,205,266,202,261,253,222"/>
</map>
