<map id="SerialWombatQuadEnc" name="SerialWombatQuadEnc">
<area shape="rect" id="Node000001" title="A class that uses two Serial Wombat input pins to read quadrature encoder input." alt="" coords="25,80,181,107"/>
<area shape="rect" id="Node000003" href="$class_serial_wombat_quad_enc__18_a_b.html" title="Extends the SerialWombatPWM class with SW18AB specific functionality, including frequency measurement..." alt="" coords="5,155,201,181"/>
<area shape="poly" id="edge2_Node000001_Node000003" title=" " alt="" coords="106,122,106,154,100,154,100,122"/>
<area shape="rect" id="Node000002" href="$class_serial_wombat_pin.html" title="Describes a Serial Wombat Pin. Is base class for other pin modes." alt="" coords="42,5,164,32"/>
<area shape="poly" id="edge1_Node000001_Node000002" title=" " alt="" coords="106,48,106,80,100,80,100,48"/>
</map>
