<map id="SerialWombatAbstractProcessedInput" name="SerialWombatAbstractProcessedInput">
<area shape="rect" id="Node000001" title="SerialWombatAnalogInput, SerialWombatPulseTimer, SerialWombatResistanceInput and others inherit from ..." alt="" coords="5,175,219,217"/>
<area shape="rect" id="Node000002" href="$class_serial_wombat18_cap_touch.html" title="A class that controls a Cap Touch Pin on the Serial Wombat 18AB chip." alt="" coords="286,5,461,32"/>
<area shape="poly" id="edge1_Node000001_Node000002" title=" " alt="" coords="136,160,191,99,226,68,265,42,292,30,294,35,268,46,230,72,195,103,140,164"/>
<area shape="rect" id="Node000003" href="$class_serial_wombat_analog_input__18_a_b.html" title="This class extends SerialWombatAnalogInput with SW18AB specific capabilities." alt="" coords="268,56,478,83"/>
<area shape="poly" id="edge2_Node000001_Node000003" title=" " alt="" coords="150,163,203,126,266,92,299,81,300,86,268,97,206,131,153,167"/>
<area shape="rect" id="Node000004" href="$class_serial_wombat_h_s_counter.html" title="This class is used to measure the frequency or cycles of a high speed input. On the Serial Wombat 18A..." alt="" coords="290,107,457,133"/>
<area shape="poly" id="edge3_Node000001_Node000004" title=" " alt="" coords="189,167,266,143,310,131,311,136,267,148,191,172"/>
<area shape="rect" id="Node000005" href="$class_serial_wombat_processed_input_pin.html" title="A Class which reads data from another pin&#39;s public data and runs it through SerialWombatAbstractInput..." alt="" coords="267,157,480,184"/>
<area shape="poly" id="edge4_Node000001_Node000005" title=" " alt="" coords="234,181,266,178,267,184,235,187"/>
<area shape="rect" id="Node000006" href="$class_serial_wombat_pulse_timer__18_a_b.html" title="extends the SerialWombatPulseTimer class with SW18AB specific functionality / This class adds functio..." alt="" coords="270,208,477,235"/>
<area shape="poly" id="edge5_Node000001_Node000006" title=" " alt="" coords="235,205,269,209,269,214,234,211"/>
<area shape="rect" id="Node000007" href="$class_serial_wombat_quad_enc__18_a_b.html" title="Extends the SerialWombatPWM class with SW18AB specific functionality, including frequency measurement..." alt="" coords="276,259,471,285"/>
<area shape="poly" id="edge6_Node000001_Node000007" title=" " alt="" coords="191,220,267,244,311,256,310,261,266,249,189,225"/>
<area shape="rect" id="Node000008" href="$class_serial_wombat_resistance_input.html" title="A class to make resistance measurements with the Serial Wombat 18AB chip." alt="" coords="275,309,472,336"/>
<area shape="poly" id="edge7_Node000001_Node000008" title=" " alt="" coords="153,225,206,261,268,295,300,306,299,311,266,300,203,266,150,229"/>
<area shape="rect" id="Node000009" href="$class_serial_wombat_ultrasonic_distance_sensor.html" title="A Class which uses one or two Serial Wombat 18AB pins to measure distance using an Ultrasonic distanc..." alt="" coords="267,360,480,403"/>
<area shape="poly" id="edge8_Node000001_Node000009" title=" " alt="" coords="141,228,196,288,230,319,268,346,290,357,288,362,265,350,227,323,192,292,137,231"/>
</map>
