<map id="SerialWombatPin" name="SerialWombatPin">
<area shape="rect" id="Node000001" title="Describes a Serial Wombat Pin. Is base class for other pin modes." alt="" coords="5,613,127,640"/>
<area shape="rect" id="Node000002" href="$class_serial_wombat18_a_b_v_g_a.html" title="A class for the Serial Wombat SW18AB chip VGA Driver." alt="" coords="207,5,370,32"/>
<area shape="poly" id="edge1_Node000001_Node000002" title=" " alt="" coords="66,598,74,478,92,311,106,226,123,149,146,86,158,61,173,42,188,30,206,22,208,27,191,35,177,46,163,64,150,88,129,151,111,227,97,312,79,478,71,598"/>
<area shape="rect" id="Node000003" href="$class_serial_wombat18_cap_touch.html" title="A class that controls a Cap Touch Pin on the Serial Wombat 18AB chip." alt="" coords="201,56,376,83"/>
<area shape="poly" id="edge2_Node000001_Node000003" title=" " alt="" coords="66,598,76,487,95,336,109,259,127,189,148,132,173,93,199,76,202,80,177,97,152,134,132,191,114,260,100,336,81,487,72,598"/>
<area shape="rect" id="Node000004" href="$class_serial_wombat_analog_input.html" title="A class to make analog measurements with the Serial Wombat." alt="" coords="203,107,374,133"/>
<area shape="poly" id="edge3_Node000001_Node000004" title=" " alt="" coords="67,598,78,497,98,361,113,292,130,230,150,178,173,143,201,126,204,130,177,147,154,181,135,231,118,293,104,362,83,497,72,598"/>
<area shape="rect" id="Node000006" href="$class_serial_wombat_debounced_input.html" title="A pin mode class that debounces inputs." alt="" coords="190,157,387,184"/>
<area shape="poly" id="edge5_Node000001_Node000006" title=" " alt="" coords="68,597,80,506,102,385,133,270,152,225,173,194,188,182,192,187,177,198,156,227,138,271,107,386,86,507,73,598"/>
<area shape="rect" id="Node000007" href="$class_serial_wombat_frequency_output.html" title="A class representing a Serial Wombat Frequency Output." alt="" coords="187,208,390,235"/>
<area shape="poly" id="edge6_Node000001_Node000007" title=" " alt="" coords="64,598,66,526,79,431,93,380,112,331,139,285,173,245,189,233,192,237,176,249,143,288,117,333,98,382,85,432,71,527,69,598"/>
<area shape="rect" id="Node000009" href="$class_serial_wombat_h_bridge.html" title="A class representing a Serial Wombat H Bridge Output." alt="" coords="214,259,363,285"/>
<area shape="poly" id="edge8_Node000001_Node000009" title=" " alt="" coords="65,597,70,535,86,453,100,410,119,368,143,329,173,295,192,283,212,275,214,280,194,287,176,299,147,332,123,371,105,412,91,454,76,535,70,598"/>
<area shape="rect" id="Node000011" href="$class_serial_wombat_h_s_clock.html" title="A Class which outputs a high speed clock signal suitable for clocking other devices." alt="" coords="211,309,366,336"/>
<area shape="poly" id="edge10_Node000001_Node000011" title=" " alt="" coords="67,597,75,544,93,476,107,440,125,406,146,374,173,346,190,335,209,327,211,332,193,339,176,350,151,377,129,408,112,442,98,477,81,545,72,598"/>
<area shape="rect" id="Node000012" href="$class_serial_wombat_h_s_counter.html" title="This class is used to measure the frequency or cycles of a high speed input. On the Serial Wombat 18A..." alt="" coords="205,360,372,387"/>
<area shape="poly" id="edge11_Node000001_Node000012" title=" " alt="" coords="70,597,81,552,101,498,131,443,150,418,173,397,203,380,206,385,176,401,154,422,135,446,106,500,86,554,75,598"/>
<area shape="rect" id="Node000013" href="$class_serial_wombat_liquid_crystal.html" title="A Class which connects to HD44780 / 1602 / 4002 / 2004 or similar interface Character LCDs." alt="" coords="199,411,378,437"/>
<area shape="poly" id="edge12_Node000001_Node000013" title=" " alt="" coords="74,598,88,563,109,522,137,481,173,447,197,434,200,439,176,451,141,485,114,525,93,565,79,600"/>
<area shape="rect" id="Node000014" href="$class_serial_wombat_p_s2_keyboard.html" title="A class for the Serial Wombat SW18AB chips which recieves input from IBM PS2 Keyboards." alt="" coords="197,461,380,488"/>
<area shape="poly" id="edge13_Node000001_Node000014" title=" " alt="" coords="81,598,118,547,144,520,173,498,198,486,200,491,176,502,147,524,122,550,85,601"/>
<area shape="rect" id="Node000015" href="$class_serial_wombat_p_w_m.html" title="A class representing a Serial Wombat PWM output." alt="" coords="221,512,356,539"/>
<area shape="poly" id="edge14_Node000001_Node000015" title=" " alt="" coords="92,601,129,573,174,548,219,533,221,538,176,553,132,578,96,605"/>
<area shape="rect" id="Node000018" href="$class_serial_wombat_processed_input_pin.html" title="A Class which reads data from another pin&#39;s public data and runs it through SerialWombatAbstractInput..." alt="" coords="182,563,394,589"/>
<area shape="poly" id="edge17_Node000001_Node000018" title=" " alt="" coords="140,607,174,599,224,587,225,593,175,604,141,612"/>
<area shape="rect" id="Node000019" href="$class_serial_wombat_protected_output.html" title="Combine and input and output pin for a protected output." alt="" coords="190,613,387,640"/>
<area shape="poly" id="edge18_Node000001_Node000019" title=" " alt="" coords="142,624,189,624,189,629,142,629"/>
<area shape="rect" id="Node000020" href="$class_serial_wombat_pulse_on_change.html" title="Monitors other pin(s) or public data in the Serial Wombat chip and generates a pin pulse on change." alt="" coords="190,664,387,691"/>
<area shape="poly" id="edge19_Node000001_Node000020" title=" " alt="" coords="141,641,175,649,225,661,224,666,174,655,140,647"/>
<area shape="rect" id="Node000021" href="$class_serial_wombat_pulse_timer.html" title="A Class which uses a Serial Wombat pin to measure the length of a pulse high and low time." alt="" coords="204,715,372,741"/>
<area shape="poly" id="edge20_Node000001_Node000021" title=" " alt="" coords="96,648,132,676,176,700,208,712,206,717,174,705,129,680,92,652"/>
<area shape="rect" id="Node000023" href="$class_serial_wombat_quad_enc.html" title="A class that uses two Serial Wombat input pins to read quadrature encoder input." alt="" coords="210,765,366,792"/>
<area shape="poly" id="edge22_Node000001_Node000023" title=" " alt="" coords="85,652,122,703,147,729,176,751,211,766,208,771,173,756,144,733,118,707,81,655"/>
<area shape="rect" id="Node000025" href="$class_serial_wombat_queued_pulse_output.html" title="A Class which outputs pulses of a duration stored in a queue." alt="" coords="179,816,398,843"/>
<area shape="poly" id="edge24_Node000001_Node000025" title=" " alt="" coords="79,654,93,688,114,729,141,769,176,802,197,813,194,818,173,806,137,772,109,731,88,691,74,656"/>
<area shape="rect" id="Node000026" href="$class_serial_wombat_resistance_input.html" title="A class to make resistance measurements with the Serial Wombat 18AB chip." alt="" coords="190,867,387,893"/>
<area shape="poly" id="edge25_Node000001_Node000026" title=" " alt="" coords="75,655,86,699,106,753,135,807,154,832,176,853,195,864,192,868,173,857,150,835,131,810,101,755,81,701,70,656"/>
<area shape="rect" id="Node000027" href="$class_serial_wombat_servo.html" title="A class to control Servos attached to the Serial Wombat chip." alt="" coords="220,917,356,944"/>
<area shape="poly" id="edge26_Node000001_Node000027" title=" " alt="" coords="72,655,81,709,98,776,112,811,129,845,151,876,176,903,197,916,220,924,219,929,195,921,173,907,146,880,125,848,107,813,93,778,75,710,67,656"/>
<area shape="rect" id="Node000030" href="$class_serial_wombat_t_m1637.html" title="A Class representing a TM1637 Seven&#45;Segment Display connected to two Serial Wombat pins." alt="" coords="214,968,363,995"/>
<area shape="poly" id="edge29_Node000001_Node000030" title=" " alt="" coords="70,655,76,718,91,799,105,841,123,883,147,921,176,954,194,966,214,974,212,979,192,971,173,958,143,924,119,885,100,843,86,800,70,719,65,656"/>
<area shape="rect" id="Node000031" href="$class_serial_wombat_throughput_consumer.html" title="A Class that consumes CPU time on the Serial Wombat chip in order to facilitate testing." alt="" coords="175,1019,402,1045"/>
<area shape="poly" id="edge30_Node000001_Node000031" title=" " alt="" coords="69,656,71,727,85,821,98,871,117,920,143,965,176,1005,192,1016,189,1020,173,1009,139,968,112,922,93,873,79,822,66,727,64,656"/>
<area shape="rect" id="Node000032" href="$class_serial_wombat_u_a_r_t.html" title="A class for the Serial Wombat 4B or SW18AB chips which creates an I2C to UART Bridge." alt="" coords="219,1069,358,1096"/>
<area shape="poly" id="edge31_Node000001_Node000032" title=" " alt="" coords="73,655,86,747,107,867,138,982,156,1026,177,1055,196,1069,220,1077,218,1082,194,1074,173,1059,152,1029,133,984,102,868,80,747,68,656"/>
<area shape="rect" id="Node000034" href="$class_serial_wombat_ultrasonic_distance_sensor.html" title="A Class which uses one or two Serial Wombat 18AB pins to measure distance using an Ultrasonic distanc..." alt="" coords="182,1120,395,1163"/>
<area shape="poly" id="edge33_Node000001_Node000034" title=" " alt="" coords="73,655,84,756,105,891,119,959,136,1021,155,1072,177,1106,190,1117,186,1121,173,1110,150,1074,131,1023,114,961,100,892,79,757,67,656"/>
<area shape="rect" id="Node000035" href="$class_serial_wombat_w_s2812.html" title="A Class representing a WS2812 or compatible RGB LED string connected to a Serial Wombat pin." alt="" coords="212,1187,364,1213"/>
<area shape="poly" id="edge34_Node000001_Node000035" title=" " alt="" coords="72,656,80,769,99,925,113,1004,131,1075,152,1134,177,1173,193,1185,213,1193,211,1198,191,1190,173,1176,147,1136,126,1077,108,1005,94,926,75,770,66,656"/>
<area shape="rect" id="Node000036" href="$class_serial_wombat_watchdog.html" title="A class to wrap around a Serial Wombat Watchdog Pin." alt="" coords="208,1237,368,1264"/>
<area shape="poly" id="edge35_Node000001_Node000036" title=" " alt="" coords="71,655,78,777,96,949,110,1036,128,1115,150,1180,163,1205,177,1223,191,1235,209,1243,207,1248,189,1239,173,1227,158,1208,145,1182,122,1117,104,1037,91,949,73,778,66,655"/>
<area shape="rect" id="Node000005" href="$class_serial_wombat_analog_input__18_a_b.html" title="This class extends SerialWombatAnalogInput with SW18AB specific capabilities." alt="" coords="466,107,676,133"/>
<area shape="poly" id="edge4_Node000004_Node000005" title=" " alt="" coords="389,117,465,117,465,123,389,123"/>
<area shape="rect" id="Node000008" href="$class_serial_wombat_frequency_output__18_a_b.html" title="Extends the SerialWombatFrequencyOutput class with SW18AB specific functionality, including SerialWom..." alt="" coords="450,208,691,235"/>
<area shape="poly" id="edge7_Node000007_Node000008" title=" " alt="" coords="405,219,450,219,450,224,405,224"/>
<area shape="rect" id="Node000010" href="$class_serial_wombat_h_bridge__18_a_b.html" title="Extends the SerialWombatHBridge class with SW18AB specific functionality, including SerialWombatAbstr..." alt="" coords="476,259,665,285"/>
<area shape="poly" id="edge9_Node000009_Node000010" title=" " alt="" coords="379,269,476,269,476,275,379,275"/>
<area shape="rect" id="Node000016" href="$class_serial_wombat_p_w_m__18_a_b.html" title="Extends the SerialWombatPWM class with SW18AB specific functionality, including SerialWombatAbstractS..." alt="" coords="484,487,658,513"/>
<area shape="poly" id="edge15_Node000015_Node000016" title=" " alt="" coords="372,515,483,505,484,510,372,521"/>
<area shape="rect" id="Node000017" href="$class_serial_wombat_p_w_m__4_a_b.html" title="Extends the SerialWombatPWM class with SW4A/SW4B specific functionality." alt="" coords="487,537,654,564"/>
<area shape="poly" id="edge16_Node000015_Node000017" title=" " alt="" coords="372,530,487,540,486,546,371,535"/>
<area shape="rect" id="Node000022" href="$class_serial_wombat_pulse_timer__18_a_b.html" title="extends the SerialWombatPulseTimer class with SW18AB specific functionality / This class adds functio..." alt="" coords="467,715,674,741"/>
<area shape="poly" id="edge21_Node000021_Node000022" title=" " alt="" coords="388,725,467,725,467,731,388,731"/>
<area shape="rect" id="Node000024" href="$class_serial_wombat_quad_enc__18_a_b.html" title="Extends the SerialWombatPWM class with SW18AB specific functionality, including frequency measurement..." alt="" coords="473,765,668,792"/>
<area shape="poly" id="edge23_Node000023_Node000024" title=" " alt="" coords="382,776,472,776,472,781,382,781"/>
<area shape="rect" id="Node000028" href="$class_serial_wombat_servo__18_a_b.html" title="A derived class that adds additional Servo Functionality for the Serial Wombat 18AB Chip." alt="" coords="483,917,658,944"/>
<area shape="poly" id="edge27_Node000027_Node000028" title=" " alt="" coords="372,928,482,928,482,933,372,933"/>
<area shape="rect" id="Node000029" href="$class_serial_wombat_high_frequency_servo.html" title="A class for the Serial Wombat 18AB Chip that adds support for high frequency hobby Servos(200 Hz,..." alt="" coords="739,909,930,952"/>
<area shape="poly" id="edge28_Node000028_Node000029" title=" " alt="" coords="674,928,739,928,739,933,674,933"/>
<area shape="rect" id="Node000033" href="$class_serial_wombat_s_w_u_a_r_t.html" title="A class for the Serial Wombat 4B or SW18AB chips which creates a software based UART on the SW18AB." alt="" coords="490,1069,651,1096"/>
<area shape="poly" id="edge32_Node000032_Node000033" title=" " alt="" coords="373,1080,490,1080,490,1085,373,1085"/>
</map>
