Serial Wombat Arduino Library

Loading...
Searching...
No Matches
Here is a list of all functions with links to the classes they belong to:

### - r -

- read() : SerialWombatMatrixKeypad, SerialWombatPS2Keyboard, SerialWombatQuadEnc, SerialWombatQueue, SerialWombatServo, SerialWombatUART
- readAverage() : SerialWombatAbstractProcessedInput
- readAveraged_mV() : SerialWombatAnalogInput
- readAveragedCounts() : SerialWombatAnalogInput
- readAveragedOhms() : SerialWombatResistanceInput
- readBirthday() : SerialWombatChip
- readBrand() : SerialWombatChip
- readBufferSize() : SerialWombatWS2812
- readBytes() : SerialWombatMatrixKeypad, SerialWombatPS2Keyboard, SerialWombatQueue, SerialWombatSWUART, SerialWombatUART
- readCounts() : SerialWombatAnalogInput, SerialWombatHSCounter
- readCurrentScanCodes() : SerialWombatPS2Keyboard
- readDeviceIdentifier() : SerialWombatChip
- readDurationInFalseState_mS() : SerialWombat18CapTouch, SerialWombatAbstractButton, SerialWombatDebouncedInput, SerialWombatMatrixButton
- readDurationInTrueState_mS() : SerialWombat18CapTouch, SerialWombatAbstractButton, SerialWombatDebouncedInput, SerialWombatMatrixButton
- readFiltered() : SerialWombatAbstractProcessedInput
- readFiltered_mV() : SerialWombatAnalogInput
- readFilteredCounts() : SerialWombatAnalogInput
- readFilteredOhms() : SerialWombatResistanceInput
- readFlashAddress() : SerialWombatChip
- readFramesExecuted() : SerialWombatChip
- readFrequency() : SerialWombatHSCounter, SerialWombatQuadEnc_18AB
- readHighCounts() : SerialWombatPulseTimer
- readLastErrorCommand() : SerialWombatChip
- readLastOutputValue() : SerialWombatAbstractScaledOutput
- ReadLastTarget() : SerialWombatAbstractScaledOutput
- readLowCounts() : SerialWombatPulseTimer
- readMaximum() : SerialWombatAbstractProcessedInput
- readMaximum_mV() : SerialWombatAnalogInput
- readMaximumCounts() : SerialWombatAnalogInput
- readMaximumOhms() : SerialWombatResistanceInput
- readMinimum() : SerialWombatAbstractProcessedInput
- readMinimum_mV() : SerialWombatAnalogInput
- readMinimumCounts() : SerialWombatAnalogInput
- readMinimumOhms() : SerialWombatResistanceInput
- readOverflowFrames() : SerialWombatChip
- readPublicData() : SerialWombatChip, SerialWombatPin
- readPulseCount() : SerialWombatUltrasonicDistanceSensor
- readPulses() : SerialWombatPulseTimer
- readRamAddress() : SerialWombatChip
- readServoSweepEntries() : SerialWombatUltrasonicDistanceSensor
- readServoSweepEntry() : SerialWombatUltrasonicDistanceSensor
- readSupplyVoltage_mV() : SerialWombatChip
- readTemperature_100thsDegC() : SerialWombatChip
- readTransitionsState() : SerialWombat18CapTouch, SerialWombatAbstractButton, SerialWombatDebouncedInput, SerialWombatMatrixButton
- readUInt16() : SerialWombatQueue
- readUniqueIdentifier() : SerialWombatChip
- readUserBuffer() : SerialWombatChip
- readVersion() : SerialWombatChip
- readVersion_uint32() : SerialWombatChip
- readVoltage_mV() : SerialWombatAnalogInput
- refresh() : SerialWombatPulseTimer
- refreshHighCountsLowCounts() : SerialWombatPulseTimer
- refreshHighCountsPulses() : SerialWombatPulseTimer
- registerErrorHandler() : SerialWombatChip
- returnErrorCode() : SerialWombatChip
- rightToLeft() : SerialWombatLiquidCrystal