Serial Wombat Arduino Library

Loading...
Searching...
No Matches
SerialWombatPS2Keyboard Member List

This is the complete list of members for SerialWombatPS2Keyboard, including all inherited members.

_pin | SerialWombatPS2Keyboard |
_pinMode | SerialWombatPin | protected
_sw | SerialWombatPin | protected
available() | SerialWombatPS2Keyboard | inline
availableForWrite() | SerialWombatPS2Keyboard | inline
begin(uint8_t clockPin, uint8_t dataPin, uint8_t bufferMode=0, uint8_t queueMode=0, uint16_t queueAddress=0xFFFF, uint8_t pullUpDown=0) | SerialWombatPS2Keyboard | inline
digitalRead() | SerialWombatPin | inline
digitalWrite(uint8_t val) | SerialWombatPin | inline
disable() | SerialWombatPin | inline
enableOpenDrain(bool enabled) | SerialWombatPin | inline
enablePullDown(bool enabled) | SerialWombatPin | inline
enablePullup(bool enabled) | SerialWombatPin | inline
flush() | SerialWombatPS2Keyboard | inline
initPacketNoResponse(uint8_t packetNumber, uint8_t param0=0x55, uint8_t param1=0x55, uint8_t param2=0x55, uint8_t param3=0x55, uint8_t param4=0x55) | SerialWombatPin | inline
initPacketNoResponse(uint8_t packetNumber, uint16_t param0=0x55, uint8_t param1=0x55, uint8_t param2=0x55, uint8_t param3=0x55) | SerialWombatPin | inline
initPacketNoResponse(uint8_t packetNumber, uint16_t param0, uint16_t param1, uint8_t param2=0x55) | SerialWombatPin | inline
isKeyPressed(uint8_t scanCode) | SerialWombatPS2Keyboard | inline
isKeyPressed(PS2KeyboardScanCode scanCode) | SerialWombatPS2Keyboard | inline
peek() | SerialWombatPS2Keyboard | inline
pin() | SerialWombatPin | inline
pinMode(uint8_t mode, bool pullDown=false, bool openDrain=false) | SerialWombatPin | inline
read() | SerialWombatPS2Keyboard | inline
readBytes(char *buffer, size_t length) | SerialWombatPS2Keyboard | inline
readCurrentScanCodes(uint8_t *buffer, uint8_t startValue) | SerialWombatPS2Keyboard | inline
readPublicData() | SerialWombatPin | inline
scanCodeToAscii(uint8_t scanCode, bool shiftActive=false) | SerialWombatPS2Keyboard | inline
SerialWombatPin(SerialWombatChip &serialWombatChip) | SerialWombatPin | inline
SerialWombatPin(SerialWombatChip &serialWombatChip, uint8_t pin) | SerialWombatPin | inline
SerialWombatPS2Keyboard(SerialWombatChip &serialWombat) | SerialWombatPS2Keyboard | inline
setTimeout(long timeout_mS) | SerialWombatPS2Keyboard | inline
swPinModeNumber() | SerialWombatPin | inline
timeout | SerialWombatPS2Keyboard | protected
write(uint8_t data) | SerialWombatPS2Keyboard | inline
write(const uint8_t *buffer, size_t size) | SerialWombatPS2Keyboard | inline
writePublicData(uint16_t value) | SerialWombatPin | inline