Serial Wombat Arduino Library

Loading...
Searching...
No Matches
PCB0031_Grip Member List

This is the complete list of members for PCB0031_Grip, including all inherited members.

_supplyVoltagemV | SerialWombatChip |
address | SerialWombatChip |
analogRead(uint8_t pin) | SerialWombatChip | inline
analogWrite(uint8_t pin, int val) | SerialWombatChip | inline
begin(uint8_t i2cAddress, bool pin3IsVoltage=false) | PCB0031_Grip | inline
SerialWombatChip::begin(HardwareSerial &serial, bool reset=true) | SerialWombatChip | inline
SerialWombatChip::begin(uint8_t i2cAddress) | SerialWombatChip |
SerialWombatChip::begin(TwoWire &wire, uint8_t i2cAddress, bool reset=true) | SerialWombatChip | inline
communicationErrorRetries | SerialWombatChip |
comparePublicDataToThreshold(uint16_t threshold=0) | SerialWombatChip | inline
configureDigitalPin(uint8_t pin, uint8_t highLow) | SerialWombatChip | inline
deviceIdentifier | SerialWombatChip |
deviceRevision | SerialWombatChip |
digitalRead(uint8_t pin) | SerialWombatChip | inline
digitalWrite(uint8_t pin, uint8_t val) | SerialWombatChip | inline
echo(uint8_t data[], uint8_t count=7) | SerialWombatChip | inline
echo(char *data) | SerialWombatChip | inline
eraseFlashPage(uint32_t address) | SerialWombatChip | inline
errorCount | SerialWombatChip |
find(bool keepTrying=false) | SerialWombatChip | inline static
fwVersion | SerialWombatChip |
gs0 | PCB0031_Grip |
gs1 | PCB0031_Grip |
gs2 | PCB0031_Grip |
gs3 | PCB0031_Grip |
gsArray | PCB0031_Grip |
hardwareReset() | SerialWombatChip | inline
inBoot | SerialWombatChip |
initialize() | SerialWombatChip | inline
isLatestFirmware(void) | SerialWombatChip | inline
isSW08() | SerialWombatChip | inline
isSW18() | SerialWombatChip | inline
jumpToBoot() | SerialWombatChip | inline
lastErrorCode | SerialWombatChip |
model | SerialWombatChip |
PCB0031_Grip() | PCB0031_Grip | inline
pinMode(uint8_t pin, uint8_t mode, bool pullDown=false, bool openDrain=false) | SerialWombatChip | inline
powerVoltage | PCB0031_Grip |
queryVersion() | SerialWombatChip | inline
readBirthday() | SerialWombatChip | inline
readBrand(char *data) | SerialWombatChip | inline
readDeviceIdentifier() | SerialWombatChip | inline
readFlashAddress(uint32_t address) | SerialWombatChip | inline
readFramesExecuted() | SerialWombatChip | inline
readLastErrorCommand(uint8_t *cmd) | SerialWombatChip | inline
readOverflowFrames() | SerialWombatChip | inline
readPowerVoltage_mv() | PCB0031_Grip | inline
readPublicData(uint8_t pin) | SerialWombatChip | inline
readPublicData(SerialWombatDataSource dataSource) | SerialWombatChip | inline
readRamAddress(uint16_t address) | SerialWombatChip | inline
readSupplyVoltage_mV(void) | SerialWombatChip | inline
readTemperature_100thsDegC(void) | SerialWombatChip | inline
readUniqueIdentifier() | SerialWombatChip | inline
readUserBuffer(uint16_t index, uint8_t *buffer, uint16_t count) | SerialWombatChip | inline
readVersion(void) | SerialWombatChip | inline
readVersion_uint32(void) | SerialWombatChip | inline
registerErrorHandler(SerialWombatErrorHandler_t handler) | SerialWombatChip | inline
returnErrorCode(uint8_t *rx) | SerialWombatChip | inline
sendPacket(uint8_t tx[], uint8_t rx[]) | SerialWombatChip |
sendPacket(uint8_t tx[]) | SerialWombatChip |
sendPacket(uint8_t tx[], uint8_t rx[], bool retryIfEchoDoesntMatch, uint8_t beginningBytesToMatch=8, uint8_t endBytesToMatch=0) | SerialWombatChip |
sendPacket(uint8_t tx[], bool retryIfEchoDoesntMatch) | SerialWombatChip |
sendPacketNoResponse(uint8_t tx[]) | SerialWombatChip |
sendReadyTime | SerialWombatChip |
SerialWombatChip() | SerialWombatChip |
setThroughputPin(uint8_t pin) | SerialWombatChip | inline
setThroughputPin(uint32_t address) | SerialWombatChip | inline
sleep() | SerialWombatChip | inline
uniqueIdentifier | SerialWombatChip |
uniqueIdentifierLength | SerialWombatChip |
wake() | SerialWombatChip | inline
writeFlashRow(uint32_t address) | SerialWombatChip | inline
writeFrameTimerPin(uint8_t pin) | SerialWombatChip | inline
writePublicData(uint8_t pin, uint16_t value) | SerialWombatChip | inline
writeRamAddress(uint16_t address, uint8_t value) | SerialWombatChip | inline
writeUserBuffer(uint16_t index, uint8_t *buffer, uint16_t count) | SerialWombatChip | inline
writeUserBuffer(uint16_t index, char *s) | SerialWombatChip | inline
writeUserBuffer(uint16_t index, const char s[]) | SerialWombatChip | inline
~SerialWombatChip() | SerialWombatChip |