Serial Wombat Arduino Library

Loading...
Searching...
No Matches
SerialWombatIRRx Member List

This is the complete list of members for SerialWombatIRRx, including all inherited members.

_pin | SerialWombatPin | protected
_pinMode | SerialWombatPin | protected
_sw | SerialWombatPin | protected
ADDRESS enum value | SerialWombatIRRx |
available() | SerialWombatIRRx | inline
availableForWrite() | SerialWombatIRRx | inline
begin(uint8_t pin, uint8_t irMode=0, bool useRepeat=true, SerialWombatPinState_t activeState=SW_LOW, uint16_t publicDataTimeoutPeriod_mS=1000, uint16_t publicDataTimeoutValue=0xFFFF, bool useAddressFilter=false, uint16_t addressFilterValue=0x1234, SerialWombatIRRx::publicDataOutput dataOutput=SerialWombatIRRx::publicDataOutput::COMMAND) | SerialWombatIRRx | inline
COMMAND enum value | SerialWombatIRRx |
DATACOUNT enum value | SerialWombatIRRx |
digitalRead() | SerialWombatPin | inline
digitalWrite(uint8_t val) | SerialWombatPin | inline
disable() | SerialWombatPin | inline
enableOpenDrain(bool enabled) | SerialWombatPin | inline
enablePulldown(bool enabled) | SerialWombatPin | inline
enablePullup(bool enabled) | SerialWombatPin | inline
flush() | SerialWombatIRRx | inline
forceDMA(bool enabled) | SerialWombatPin | inline
initPacketNoResponse(uint8_t packetNumber, uint8_t param0=0x55, uint8_t param1=0x55, uint8_t param2=0x55, uint8_t param3=0x55, uint8_t param4=0x55) | SerialWombatPin | inline
initPacketNoResponse(uint8_t packetNumber, uint16_t param0=0x55, uint8_t param1=0x55, uint8_t param2=0x55, uint8_t param3=0x55) | SerialWombatPin | inline
initPacketNoResponse(uint8_t packetNumber, uint16_t param0, uint16_t param1, uint8_t param2=0x55) | SerialWombatPin | inline
operator=(SerialWombatIRRx &irrx) | SerialWombatIRRx | inline
peek() | SerialWombatIRRx | inline
pin() | SerialWombatPin | inline
pinMode(uint8_t mode, bool pullDown=false, bool openDrain=false) | SerialWombatPin | inline
publicDataOutput enum name | SerialWombatIRRx |
read() | SerialWombatIRRx | inline
readAddress() | SerialWombatIRRx | inline
readBytes(char *buffer, size_t length) | SerialWombatIRRx | inline
readDataCount() | SerialWombatIRRx | inline
readPublicData() | SerialWombatPin | inline
SerialWombatIRRx(SerialWombatChip &sw) | SerialWombatIRRx | inline
SerialWombatPin(SerialWombatChip &serialWombatChip) | SerialWombatPin | inline
SerialWombatPin(SerialWombatChip &serialWombatChip, uint8_t pin) | SerialWombatPin | inline
setTimeout(long timeout_mS) | SerialWombatIRRx | inline
swPinModeNumber() | SerialWombatPin | inline
timeout | SerialWombatIRRx | protected
write(uint8_t data) | SerialWombatIRRx | inline
write(const uint8_t *buffer, size_t size) | SerialWombatIRRx | inline
writePublicData(uint16_t value) | SerialWombatPin | inline