Serial Wombat Arduino Library

Loading...
Searching...
No Matches
SerialWombatUART Member List

This is the complete list of members for SerialWombatUART, including all inherited members.

_baudMarker | SerialWombatUART | protected
_pin | SerialWombatPin | protected
_pinMode | SerialWombatUART | protected
_rx7Command | SerialWombatUART | protected
_rxPin | SerialWombatUART | protected
_sw | SerialWombatPin | protected
_tx7Command | SerialWombatUART | protected
_txPin | SerialWombatUART | protected
available() | SerialWombatUART | inline virtual
availableForWrite() | SerialWombatUART | inline virtual
begin(uint32_t baudRate, uint8_t pin, uint8_t rxPin, uint8_t txPin, uint8_t HWinterface=1) | SerialWombatUART | inline
digitalRead() | SerialWombatPin | inline
digitalWrite(uint8_t val) | SerialWombatPin | inline
disable() | SerialWombatPin | inline
enableOpenDrain(bool enabled) | SerialWombatPin | inline
enablePulldown(bool enabled) | SerialWombatPin | inline
enablePullup(bool enabled) | SerialWombatPin | inline
flush() | SerialWombatUART | inline virtual
forceDMA(bool enabled) | SerialWombatPin | inline
initPacketNoResponse(uint8_t packetNumber, uint8_t param0=0x55, uint8_t param1=0x55, uint8_t param2=0x55, uint8_t param3=0x55, uint8_t param4=0x55) | SerialWombatPin | inline
initPacketNoResponse(uint8_t packetNumber, uint16_t param0=0x55, uint8_t param1=0x55, uint8_t param2=0x55, uint8_t param3=0x55) | SerialWombatPin | inline
initPacketNoResponse(uint8_t packetNumber, uint16_t param0, uint16_t param1, uint8_t param2=0x55) | SerialWombatPin | inline
peek() | SerialWombatUART | inline virtual
pin() | SerialWombatPin | inline
pinMode(uint8_t mode, bool pullDown=false, bool openDrain=false) | SerialWombatPin | inline
read() | SerialWombatUART | inline virtual
readBytes(char *buffer, size_t length) | SerialWombatUART | inline virtual
readPublicData() | SerialWombatPin | inline
SerialWombatPin(SerialWombatChip &serialWombatChip) | SerialWombatPin | inline
SerialWombatPin(SerialWombatChip &serialWombatChip, uint8_t pin) | SerialWombatPin | inline
SerialWombatUART(SerialWombatChip &serialWombat) | SerialWombatUART | inline
setTimeout(long timeout_mS) | SerialWombatUART | inline virtual
swPinModeNumber() | SerialWombatPin | inline
timeout | SerialWombatUART | protected
write(uint8_t data) | SerialWombatUART | inline virtual
write(const uint8_t *buffer, size_t size) | SerialWombatUART | inline virtual
writePublicData(uint16_t value) | SerialWombatPin | inline