Serial Wombat Arduino Library

Loading...
Searching...
No Matches
SerialWombatProtectedOutput Member List

This is the complete list of members for SerialWombatProtectedOutput, including all inherited members.

_pin | SerialWombatPin | protected
_pinMode | SerialWombatPin | protected
_sw | SerialWombatPin | protected
begin(uint8_t pin, uint8_t monitoredPin) | SerialWombatProtectedOutput | inline
configure(PO_COMPARE_t compareMode, uint16_t compareValue, uint8_t debounceTime, SerialWombatPinState_t activeState, SerialWombatPinState_t safeState) | SerialWombatProtectedOutput | inline
digitalRead() | SerialWombatPin | inline
digitalWrite(uint8_t state) | SerialWombatProtectedOutput | inline
disable() | SerialWombatPin | inline
enableOpenDrain(bool enabled) | SerialWombatPin | inline
enablePulldown(bool enabled) | SerialWombatPin | inline
enablePullup(bool enabled) | SerialWombatPin | inline
forceDMA(bool enabled) | SerialWombatPin | inline
initPacketNoResponse(uint8_t packetNumber, uint8_t param0=0x55, uint8_t param1=0x55, uint8_t param2=0x55, uint8_t param3=0x55, uint8_t param4=0x55) | SerialWombatPin | inline
initPacketNoResponse(uint8_t packetNumber, uint16_t param0=0x55, uint8_t param1=0x55, uint8_t param2=0x55, uint8_t param3=0x55) | SerialWombatPin | inline
initPacketNoResponse(uint8_t packetNumber, uint16_t param0, uint16_t param1, uint8_t param2=0x55) | SerialWombatPin | inline
isInSafeState() | SerialWombatProtectedOutput | inline
makeInput() | SerialWombatProtectedOutput | inline
pin() | SerialWombatPin | inline
pinMode(uint8_t mode, bool pullDown=false, bool openDrain=false) | SerialWombatPin | inline
readPublicData() | SerialWombatPin | inline
SerialWombatPin(SerialWombatChip &serialWombatChip) | SerialWombatPin | inline
SerialWombatPin(SerialWombatChip &serialWombatChip, uint8_t pin) | SerialWombatPin | inline
SerialWombatProtectedOutput(SerialWombatChip &serialWombat) | SerialWombatProtectedOutput | inline
setPinNumberForTesting(uint8_t pin) | SerialWombatPin | inline
swPinModeNumber() | SerialWombatPin | inline
writePublicData(uint16_t value) | SerialWombatPin | inline