Serial Wombat Arduino Library

Loading...
Searching...
No Matches
SerialWombatUltrasonicDistanceSensor Member List

This is the complete list of members for SerialWombatUltrasonicDistanceSensor, including all inherited members.

_pin | SerialWombatPin | protected
_pinMode | SerialWombatPin | protected
_sw | SerialWombatPin | protected
AVERAGE enum value | SerialWombatAbstractProcessedInput |
begin(uint8_t echoPin, driver driver, uint8_t triggerPin, bool autoTrigger=true, bool pullUp=false) | SerialWombatUltrasonicDistanceSensor | inline
configureIntegrator(uint16_t negativeMaxIndex, uint16_t negativeMidIndex, uint16_t negativeDeadZone, uint16_t positiveDeadZone, uint16_t positiveMidIndex, uint16_t positiveMaxIndex, uint16_t midIncrement, uint16_t maxIncrement, uint16_t initialValue, uint8_t updateFrequencyMask=0) | SerialWombatAbstractProcessedInput | inline
configureOutputValue(OutputValue outputValue) | SerialWombatAbstractProcessedInput | inline
configureQueue(SerialWombatQueue *queue, Period period, bool queueHighByte=true, bool queueLowByte=true) | SerialWombatAbstractProcessedInput | inline
configureServoSweep(uint8_t servoPin, uint16_t memoryIndex, uint16_t servoPositions_, uint16_t servoIncrement, bool reverse=false, uint16_t servoMoveDelay=100, uint16_t servoReturnDelay=1000) | SerialWombatUltrasonicDistanceSensor | inline
digitalRead() | SerialWombatPin | inline
digitalWrite(uint8_t val) | SerialWombatPin | inline
disable() | SerialWombatPin | inline
driver enum name | SerialWombatUltrasonicDistanceSensor |
enableOpenDrain(bool enabled) | SerialWombatPin | inline
enablePulldown(bool enabled) | SerialWombatPin | inline
enablePullup(bool enabled) | SerialWombatPin | inline
enableServoSweep(bool enable=true) | SerialWombatUltrasonicDistanceSensor | inline
FIRST_ORDER_FILTERED enum value | SerialWombatAbstractProcessedInput |
forceDMA(bool enabled) | SerialWombatPin | inline
HC_SR04 enum value | SerialWombatUltrasonicDistanceSensor |
initPacketNoResponse(uint8_t packetNumber, uint8_t param0=0x55, uint8_t param1=0x55, uint8_t param2=0x55, uint8_t param3=0x55, uint8_t param4=0x55) | SerialWombatPin | inline
initPacketNoResponse(uint8_t packetNumber, uint16_t param0=0x55, uint8_t param1=0x55, uint8_t param2=0x55, uint8_t param3=0x55) | SerialWombatPin | inline
initPacketNoResponse(uint8_t packetNumber, uint16_t param0, uint16_t param1, uint8_t param2=0x55) | SerialWombatPin | inline
LINEAR_MXB enum value | SerialWombatAbstractProcessedInput |
manualTrigger() | SerialWombatUltrasonicDistanceSensor | inline
NONE enum value | SerialWombatAbstractProcessedInput |
OutputValue enum name | SerialWombatAbstractProcessedInput |
Period enum name | SerialWombatAbstractProcessedInput |
PERIOD_1024mS enum value | SerialWombatAbstractProcessedInput |
PERIOD_128mS enum value | SerialWombatAbstractProcessedInput |
PERIOD_16mS enum value | SerialWombatAbstractProcessedInput |
PERIOD_1mS enum value | SerialWombatAbstractProcessedInput |
PERIOD_256mS enum value | SerialWombatAbstractProcessedInput |
PERIOD_2mS enum value | SerialWombatAbstractProcessedInput |
PERIOD_32mS enum value | SerialWombatAbstractProcessedInput |
PERIOD_4mS enum value | SerialWombatAbstractProcessedInput |
PERIOD_512mS enum value | SerialWombatAbstractProcessedInput |
PERIOD_64mS enum value | SerialWombatAbstractProcessedInput |
PERIOD_8mS enum value | SerialWombatAbstractProcessedInput |
pin() | SerialWombatUltrasonicDistanceSensor | inline virtual
pinMode(uint8_t mode, bool pullDown=false, bool openDrain=false) | SerialWombatPin | inline
RAW enum value | SerialWombatAbstractProcessedInput |
readAverage() | SerialWombatAbstractProcessedInput | inline
readFiltered() | SerialWombatAbstractProcessedInput | inline
readMaximum(bool resetAfterRead=false) | SerialWombatAbstractProcessedInput | inline
readMinimum(bool resetAfterRead=false) | SerialWombatAbstractProcessedInput | inline
readPublicData() | SerialWombatPin | inline
readPulseCount() | SerialWombatUltrasonicDistanceSensor | inline
readServoSweepEntries(uint16_t *entries, uint16_t count) | SerialWombatUltrasonicDistanceSensor | inline
readServoSweepEntry(uint16_t servoSweepEntry) | SerialWombatUltrasonicDistanceSensor | inline
SCALE_RANGE enum value | SerialWombatAbstractProcessedInput |
SerialWombatAbstractProcessedInput(SerialWombatChip &sw) | SerialWombatAbstractProcessedInput | inline
SerialWombatPin(SerialWombatChip &serialWombatChip) | SerialWombatPin | inline
SerialWombatPin(SerialWombatChip &serialWombatChip, uint8_t pin) | SerialWombatPin | inline
SerialWombatUltrasonicDistanceSensor(SerialWombatChip &serialWombat) | SerialWombatUltrasonicDistanceSensor | inline
servoMemoryIndex | SerialWombatUltrasonicDistanceSensor |
servoPositions | SerialWombatUltrasonicDistanceSensor |
setPinNumberForTesting(uint8_t pin) | SerialWombatPin | inline
swPinModeNumber() | SerialWombatUltrasonicDistanceSensor | inline virtual
Transform enum name | SerialWombatAbstractProcessedInput |
writeAveragingNumberOfSamples(uint16_t numberOfSamples) | SerialWombatAbstractProcessedInput | inline
writeExcludeBelowAbove(uint16_t low, uint16_t high) | SerialWombatAbstractProcessedInput | inline
writeFirstOrderFilteringConstant(uint16_t constant) | SerialWombatAbstractProcessedInput | inline
writeInverted(bool inverted) | SerialWombatAbstractProcessedInput | inline
writeProcessedInputEnable(bool enabled) | SerialWombatAbstractProcessedInput | inline
writePublicData(uint16_t value) | SerialWombatPin | inline
writeTransformLinearMXB(int32_t m, int32_t b) | SerialWombatAbstractProcessedInput | inline
writeTransformScaleRange(uint16_t min, uint16_t max) | SerialWombatAbstractProcessedInput | inline