Serial Wombat Arduino Library

Loading...
Searching...
No Matches
SerialWombatPulseOnChange Member List

This is the complete list of members for SerialWombatPulseOnChange, including all inherited members.

_pin | SerialWombatPin | protected
_pinMode | SerialWombatPin | protected
_sw | SerialWombatPin | protected
begin(uint8_t pin, SerialWombatPinState_t activeMode=SW_HIGH, SerialWombatPinState_t inactiveMode=SW_LOW, uint16_t pulseOnTime=50, uint16_t pulseOffTime=50, uint8_t orNotAnd=1, uint16_t PWMperiod=0, uint16_t PWMdutyCycle=0x8000) | SerialWombatPulseOnChange | inline
digitalRead() | SerialWombatPin | inline
digitalWrite(uint8_t val) | SerialWombatPin | inline
disable() | SerialWombatPin | inline
enableOpenDrain(bool enabled) | SerialWombatPin | inline
enablePulldown(bool enabled) | SerialWombatPin | inline
enablePullup(bool enabled) | SerialWombatPin | inline
forceDMA(bool enabled) | SerialWombatPin | inline
initPacketNoResponse(uint8_t packetNumber, uint8_t param0=0x55, uint8_t param1=0x55, uint8_t param2=0x55, uint8_t param3=0x55, uint8_t param4=0x55) | SerialWombatPin | inline
initPacketNoResponse(uint8_t packetNumber, uint16_t param0=0x55, uint8_t param1=0x55, uint8_t param2=0x55, uint8_t param3=0x55) | SerialWombatPin | inline
initPacketNoResponse(uint8_t packetNumber, uint16_t param0, uint16_t param1, uint8_t param2=0x55) | SerialWombatPin | inline
pin() | SerialWombatPin | inline
pinMode(uint8_t mode, bool pullDown=false, bool openDrain=false) | SerialWombatPin | inline
readPublicData() | SerialWombatPin | inline
SerialWombatPin(SerialWombatChip &serialWombatChip) | SerialWombatPin | inline
SerialWombatPin(SerialWombatChip &serialWombatChip, uint8_t pin) | SerialWombatPin | inline
SerialWombatPulseOnChange(SerialWombatChip &serialWombat) | SerialWombatPulseOnChange | inline
setEntryOnChange(uint8_t entryID, uint8_t sourcePin) | SerialWombatPulseOnChange | inline
setEntryOnDecrease(uint8_t entryID, uint8_t sourcePin) | SerialWombatPulseOnChange | inline
setEntryOnEqualValue(uint8_t entryID, uint8_t sourcePin, uint16_t value) | SerialWombatPulseOnChange | inline
setEntryOnGreaterThanValue(uint8_t entryID, uint8_t sourcePin, uint16_t value) | SerialWombatPulseOnChange | inline
setEntryOnIncrease(uint8_t entryID, uint8_t sourcePin) | SerialWombatPulseOnChange | inline
setEntryOnLessThanValue(uint8_t entryID, uint8_t sourcePin, uint16_t value) | SerialWombatPulseOnChange | inline
setEntryOnNotEqualValue(uint8_t entryID, uint8_t sourcePin, uint16_t value) | SerialWombatPulseOnChange | inline
setEntryOnPinCrossAscending(uint8_t entryID, uint8_t sourcePin, uint16_t value) | SerialWombatPulseOnChange |
setEntryOnPinCrossDescending(uint8_t entryID, uint8_t sourcePin, uint16_t value) | SerialWombatPulseOnChange |
setEntryOnPinCrossValue(uint8_t entryID, uint8_t sourcePin, uint16_t value) | SerialWombatPulseOnChange |
setEntryOnPinGTPin(uint8_t entryID, uint8_t sourcePin, uint8_t secondPin) | SerialWombatPulseOnChange |
setEntryOnPinLTPin(uint8_t entryID, uint8_t sourcePin, uint8_t secondPin) | SerialWombatPulseOnChange |
setEntryOnPinOutsideRange(uint8_t entryID, uint8_t sourcePin, uint16_t lowValue, uint16_t highValue) | SerialWombatPulseOnChange |
setEntryOnPinsEqual(uint8_t entryID, uint8_t sourcePin, uint8_t secondPin) | SerialWombatPulseOnChange | inline
setEntryOnPinsNotEqual(uint8_t entryID, uint8_t sourcePin, uint8_t secondPin) | SerialWombatPulseOnChange | inline
setEntryOnPinWithinRange(uint8_t entryID, uint8_t sourcePin, uint16_t lowValue, uint16_t highValue) | SerialWombatPulseOnChange |
setPinNumberForTesting(uint8_t pin) | SerialWombatPin | inline
swPinModeNumber() | SerialWombatPin | inline
writePublicData(uint16_t value) | SerialWombatPin | inline