Serial Wombat Arduino Library

Loading...
Searching...
No Matches
SerialWombatAnalogInput Member List

This is the complete list of members for SerialWombatAnalogInput, including all inherited members.

_pin | SerialWombatPin | protected
_pinMode | SerialWombatPin | protected
_sw | SerialWombatPin | protected
begin(uint8_t pin, uint16_t averageSamples=64, uint16_t filterConstant=0xFF80, AnalogInputPublicDataOutput publicDataOutput=AnalogInputPublicDataOutput::AnalogInputPublicDataOutput_Raw) | SerialWombatAnalogInput | inline
digitalRead() | SerialWombatPin | inline
digitalWrite(uint8_t val) | SerialWombatPin | inline
disable() | SerialWombatPin | inline
enableOpenDrain(bool enabled) | SerialWombatPin | inline
enablePulldown(bool enabled) | SerialWombatPin | inline
enablePullup(bool enabled) | SerialWombatPin | inline
forceDMA(bool enabled) | SerialWombatPin | inline
initPacketNoResponse(uint8_t packetNumber, uint8_t param0=0x55, uint8_t param1=0x55, uint8_t param2=0x55, uint8_t param3=0x55, uint8_t param4=0x55) | SerialWombatPin | inline
initPacketNoResponse(uint8_t packetNumber, uint16_t param0=0x55, uint8_t param1=0x55, uint8_t param2=0x55, uint8_t param3=0x55) | SerialWombatPin | inline
initPacketNoResponse(uint8_t packetNumber, uint16_t param0, uint16_t param1, uint8_t param2=0x55) | SerialWombatPin | inline
pin() | SerialWombatPin | inline
pinMode(uint8_t mode, bool pullDown=false, bool openDrain=false) | SerialWombatPin | inline
readAveraged_mV() | SerialWombatAnalogInput | inline
readAveragedCounts() | SerialWombatAnalogInput | inline
readCounts() | SerialWombatAnalogInput | inline
readFiltered_mV() | SerialWombatAnalogInput | inline
readFilteredCounts() | SerialWombatAnalogInput | inline
readMaximum_mV(bool resetAfterRead=false) | SerialWombatAnalogInput | inline
readMaximumCounts(bool resetAfterRead=false) | SerialWombatAnalogInput | inline
readMinimum_mV(bool resetAfterRead=false) | SerialWombatAnalogInput | inline
readMinimumCounts(bool resetAfterRead=false) | SerialWombatAnalogInput | inline
readPublicData() | SerialWombatPin | inline
readVoltage_mV() | SerialWombatAnalogInput | inline
SerialWombatAnalogInput(SerialWombatChip &SerialWombatChip) | SerialWombatAnalogInput | inline
SerialWombatPin(SerialWombatChip &serialWombatChip) | SerialWombatPin | inline
SerialWombatPin(SerialWombatChip &serialWombatChip, uint8_t pin) | SerialWombatPin | inline
setPinNumberForTesting(uint8_t pin) | SerialWombatPin | inline
swPinModeNumber() | SerialWombatPin | inline
updateSupplyVoltage_mV() | SerialWombatAnalogInput | inline
writePublicData(uint16_t value) | SerialWombatPin | inline