Serial Wombat Arduino Library

Loading...
Searching...
No Matches
SerialWombatTM1637 Member List

This is the complete list of members for SerialWombatTM1637, including all inherited members.

_pin | SerialWombatPin | protected
_pinMode | SerialWombatPin | protected
_sw | SerialWombatPin | protected
availableForWrite() | SerialWombatTM1637 | inline virtual
begin(uint8_t clkPin, uint8_t dioPin, uint8_t digits, SWTM1637Mode mode, uint8_t dataSourcePin, uint8_t brightness0to7) | SerialWombatTM1637 | inline
digitalRead() | SerialWombatPin | inline
digitalWrite(uint8_t val) | SerialWombatPin | inline
disable() | SerialWombatPin | inline
enableOpenDrain(bool enabled) | SerialWombatPin | inline
enablePulldown(bool enabled) | SerialWombatPin | inline
enablePullup(bool enabled) | SerialWombatPin | inline
forceDMA(bool enabled) | SerialWombatPin | inline
initPacketNoResponse(uint8_t packetNumber, uint8_t param0=0x55, uint8_t param1=0x55, uint8_t param2=0x55, uint8_t param3=0x55, uint8_t param4=0x55) | SerialWombatPin | inline
initPacketNoResponse(uint8_t packetNumber, uint16_t param0=0x55, uint8_t param1=0x55, uint8_t param2=0x55, uint8_t param3=0x55) | SerialWombatPin | inline
initPacketNoResponse(uint8_t packetNumber, uint16_t param0, uint16_t param1, uint8_t param2=0x55) | SerialWombatPin | inline
pin() | SerialWombatPin | inline
pinMode(uint8_t mode, bool pullDown=false, bool openDrain=false) | SerialWombatPin | inline
readPublicData() | SerialWombatPin | inline
SerialWombatPin(SerialWombatChip &serialWombatChip) | SerialWombatPin | inline
SerialWombatPin(SerialWombatChip &serialWombatChip, uint8_t pin) | SerialWombatPin | inline
SerialWombatTM1637(SerialWombatChip &serialWombat) | SerialWombatTM1637 | inline
setPinNumberForTesting(uint8_t pin) | SerialWombatPin | inline
suppressLeadingZeros(bool suppress) | SerialWombatTM1637 | inline
swPinModeNumber() | SerialWombatPin | inline
write(uint8_t data) | SerialWombatTM1637 | inline
write(const uint8_t *buffer, size_t size) | SerialWombatTM1637 | inline
writeAnimation(uint16_t bufferIndex, uint16_t delay, uint8_t numberOfFrames, uint8_t data[][6]) | SerialWombatTM1637 | inline
writeArray(uint8_t data[6]) | SerialWombatTM1637 | inline
writeBlinkBitmap(uint8_t blinkBitmapLSBleftDigit) | SerialWombatTM1637 | inline
writeBrightness(uint8_t brightness0to7) | SerialWombatTM1637 | inline
writeDecimalBitmap(uint8_t decimalBitmapLSBleftDigit) | SerialWombatTM1637 | inline
writeDigitOrder(uint8_t first, uint8_t second, uint8_t third, uint8_t fourth, uint8_t fifth, uint8_t sixth) | SerialWombatTM1637 | inline
writePublicData(uint16_t value) | SerialWombatPin | inline