Serial Wombat Arduino Library

Loading...
Searching...
No Matches
SerialWombatSimulatedQuadEnc Member List

This is the complete list of members for SerialWombatSimulatedQuadEnc, including all inherited members.

bothPinsHigh() | SerialWombatSimulatedQuadEnc | inline
currentPosition | SerialWombatSimulatedQuadEnc |
delayAfterFirstPinFirstTransition_mS | SerialWombatSimulatedQuadEnc |
delayAfterFirstPinSecondTransition_mS | SerialWombatSimulatedQuadEnc |
delayAfterSecondPinFirstTransition_mS | SerialWombatSimulatedQuadEnc |
delayAfterSecondPinSecondTransition_mS | SerialWombatSimulatedQuadEnc |
doubleTransition | SerialWombatSimulatedQuadEnc |
initialize() | SerialWombatSimulatedQuadEnc | inline
lastTransitionTime_millis | SerialWombatSimulatedQuadEnc |
openDrain | SerialWombatSimulatedQuadEnc |
pin0High() | SerialWombatSimulatedQuadEnc | inline
pin0Low() | SerialWombatSimulatedQuadEnc | inline
pin1High() | SerialWombatSimulatedQuadEnc | inline
pin1Low() | SerialWombatSimulatedQuadEnc | inline
SerialWombatSimulatedQuadEnc(SerialWombatChip &serialWombat0, SerialWombatChip &serialWombat1, uint8_t _pin0, uint8_t _pin1, bool openDrain, bool doubleTransition) | SerialWombatSimulatedQuadEnc | inline
service() | SerialWombatSimulatedQuadEnc | inline
state | SerialWombatSimulatedQuadEnc |
targetPosition | SerialWombatSimulatedQuadEnc |
togglePin0() | SerialWombatSimulatedQuadEnc | inline
togglePin1() | SerialWombatSimulatedQuadEnc | inline