Serial Wombat Arduino Library

Loading...
Searching...
No Matches
SerialWombat18ABVGA Member List

This is the complete list of members for SerialWombat18ABVGA, including all inherited members.

_pin | SerialWombatPin | protected
_pinMode | SerialWombatPin | protected
_sw | SerialWombatPin | protected
begin(uint8_t vsyncPin, uint16_t bufferIndex=0) | SerialWombat18ABVGA | inline
digitalRead() | SerialWombatPin | inline
digitalWrite(uint8_t val) | SerialWombatPin | inline
disable() | SerialWombatPin | inline
enableOpenDrain(bool enabled) | SerialWombatPin | inline
enablePulldown(bool enabled) | SerialWombatPin | inline
enablePullup(bool enabled) | SerialWombatPin | inline
fillRect(uint8_t x, uint8_t y, uint8_t w, uint8_t h, uint8_t color) | SerialWombat18ABVGA | inline
fillScreen(uint8_t color) | SerialWombat18ABVGA | inline
forceDMA(bool enabled) | SerialWombatPin | inline
initPacketNoResponse(uint8_t packetNumber, uint8_t param0=0x55, uint8_t param1=0x55, uint8_t param2=0x55, uint8_t param3=0x55, uint8_t param4=0x55) | SerialWombatPin | inline
initPacketNoResponse(uint8_t packetNumber, uint16_t param0=0x55, uint8_t param1=0x55, uint8_t param2=0x55, uint8_t param3=0x55) | SerialWombatPin | inline
initPacketNoResponse(uint8_t packetNumber, uint16_t param0, uint16_t param1, uint8_t param2=0x55) | SerialWombatPin | inline
pin() | SerialWombatPin | inline
pinMode(uint8_t mode, bool pullDown=false, bool openDrain=false) | SerialWombatPin | inline
readPublicData() | SerialWombatPin | inline
SerialWombat18ABVGA(SerialWombatChip &serialWombat) | SerialWombat18ABVGA | inline
SerialWombatPin(SerialWombatChip &serialWombatChip) | SerialWombatPin | inline
SerialWombatPin(SerialWombatChip &serialWombatChip, uint8_t pin) | SerialWombatPin | inline
setLineColor(uint8_t color, uint8_t y) | SerialWombat18ABVGA | inline
setLineColor(uint8_t color, uint8_t start, uint8_t end) | SerialWombat18ABVGA | inline
setPinNumberForTesting(uint8_t pin) | SerialWombatPin | inline
swPinModeNumber() | SerialWombatPin | inline
writePixel(uint8_t x, uint8_t y, uint8_t color) | SerialWombat18ABVGA | inline
writePublicData(uint16_t value) | SerialWombatPin | inline