<map id="SerialWombatAnalogInput" name="SerialWombatAnalogInput">
<area shape="rect" id="Node000001" title="A class to make analog measurements with the Serial Wombat." alt="" coords="25,80,196,107"/>
<area shape="rect" id="Node000003" href="$class_serial_wombat_analog_input__18_a_b.html" title="This class extends SerialWombatAnalogInput with SW18AB specific capabilities." alt="" coords="5,155,216,181"/>
<area shape="poly" id="edge2_Node000001_Node000003" title=" " alt="" coords="113,122,113,154,108,154,108,122"/>
<area shape="rect" id="Node000002" href="$class_serial_wombat_pin.html" title="Describes a Serial Wombat Pin. Is base class for other pin modes." alt="" coords="50,5,171,32"/>
<area shape="poly" id="edge1_Node000001_Node000002" title=" " alt="" coords="113,48,113,80,108,80,108,48"/>
<area shape="rect" id="Node000004" href="$class_grip_a_c_s712.html" title="A class representing an Allegro ACS712 5A current sensor connected to a SW8B Analog input on a PCB003..." alt="" coords="63,229,158,256"/>
<area shape="poly" id="edge3_Node000003_Node000004" title=" " alt="" coords="113,197,113,229,108,229,108,197"/>
</map>
