Serial Wombat Arduino Library

Loading...
Searching...
No Matches
SerialWombatAbstractProcessedInput Member List

This is the complete list of members for SerialWombatAbstractProcessedInput, including all inherited members.

AVERAGE enum value | SerialWombatAbstractProcessedInput |
configureIntegrator(uint16_t negativeMaxIndex, uint16_t negativeMidIndex, uint16_t negativeDeadZone, uint16_t positiveDeadZone, uint16_t positiveMidIndex, uint16_t positiveMaxIndex, uint16_t midIncrement, uint16_t maxIncrement, uint16_t initialValue, uint8_t updateFrequencyMask=0) | SerialWombatAbstractProcessedInput | inline
configureOutputValue(OutputValue outputValue) | SerialWombatAbstractProcessedInput | inline
configureQueue(SerialWombatQueue *queue, Period period, bool queueHighByte=true, bool queueLowByte=true) | SerialWombatAbstractProcessedInput | inline
FIRST_ORDER_FILTERED enum value | SerialWombatAbstractProcessedInput |
LINEAR_MXB enum value | SerialWombatAbstractProcessedInput |
NONE enum value | SerialWombatAbstractProcessedInput |
OutputValue enum name | SerialWombatAbstractProcessedInput |
Period enum name | SerialWombatAbstractProcessedInput |
PERIOD_1024mS enum value | SerialWombatAbstractProcessedInput |
PERIOD_128mS enum value | SerialWombatAbstractProcessedInput |
PERIOD_16mS enum value | SerialWombatAbstractProcessedInput |
PERIOD_1mS enum value | SerialWombatAbstractProcessedInput |
PERIOD_256mS enum value | SerialWombatAbstractProcessedInput |
PERIOD_2mS enum value | SerialWombatAbstractProcessedInput |
PERIOD_32mS enum value | SerialWombatAbstractProcessedInput |
PERIOD_4mS enum value | SerialWombatAbstractProcessedInput |
PERIOD_512mS enum value | SerialWombatAbstractProcessedInput |
PERIOD_64mS enum value | SerialWombatAbstractProcessedInput |
PERIOD_8mS enum value | SerialWombatAbstractProcessedInput |
pin()=0 | SerialWombatAbstractProcessedInput | pure virtual
RAW enum value | SerialWombatAbstractProcessedInput |
readAverage() | SerialWombatAbstractProcessedInput | inline
readFiltered() | SerialWombatAbstractProcessedInput | inline
readMaximum(bool resetAfterRead=false) | SerialWombatAbstractProcessedInput | inline
readMinimum(bool resetAfterRead=false) | SerialWombatAbstractProcessedInput | inline
SCALE_RANGE enum value | SerialWombatAbstractProcessedInput |
SerialWombatAbstractProcessedInput(SerialWombatChip &sw) | SerialWombatAbstractProcessedInput | inline
swPinModeNumber()=0 | SerialWombatAbstractProcessedInput | pure virtual
Transform enum name | SerialWombatAbstractProcessedInput |
writeAveragingNumberOfSamples(uint16_t numberOfSamples) | SerialWombatAbstractProcessedInput | inline
writeExcludeBelowAbove(uint16_t low, uint16_t high) | SerialWombatAbstractProcessedInput | inline
writeFirstOrderFilteringConstant(uint16_t constant) | SerialWombatAbstractProcessedInput | inline
writeInverted(bool inverted) | SerialWombatAbstractProcessedInput | inline
writeProcessedInputEnable(bool enabled) | SerialWombatAbstractProcessedInput | inline
writeTransformLinearMXB(int32_t m, int32_t b) | SerialWombatAbstractProcessedInput | inline
writeTransformScaleRange(uint16_t min, uint16_t max) | SerialWombatAbstractProcessedInput | inline