Serial Wombat Arduino Library

Loading...
Searching...
No Matches
PCB0041_Remcon.h
Go to the documentation of this file.
1#pragma once
2/*
3 Copyright 2026 Broadwell Consulting Inc.
4
5"Serial Wombat" is a registered trademark of Broadwell Consulting Inc. in
6 the United States. See SerialWombat.com for usage guidance.
7
8 Permission is hereby granted, free of charge, to any person obtaining a
9 copy of this software and associated documentation files (the "Software"),
10 to deal in the Software without restriction, including without limitation
11 the rights to use, copy, modify, merge, publish, distribute, sublicense,
12 and/or sell copies of the Software, and to permit persons to whom the
13 Software is furnished to do so, subject to the following conditions:
14
15 The above copyright notice and this permission notice shall be included in
16 all copies or substantial portions of the Software.
17
18 THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR
19 IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY,
20 FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL
21 THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR
22 OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE,
23 ARISING FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
24 OTHER DEALINGS IN THE SOFTWARE.
25*/
29#include "SerialWombat.h"
30
70
71 class PCB0041_Remcon : public SerialWombatChip
72{
73 public:
74 PCB0041_Remcon() : SerialWombatChip(), irrx(*this), irtx(*this), blink(*this)
75 {}
76
77 SerialWombatIRRx irrx;
78 SerialWombatIRTx irtx;
79 SerialWombatBlink blink;
80
81
82
83
94 int16_t begin(uint8_t i2cAddress, uint16_t irTxAddress = 0x1234, bool enableBlink = true )
95 {
96 SerialWombatChip::begin(Wire, i2cAddress, true);
97 irrx.begin((uint8_t)3);
98 irtx.begin((uint8_t)7, irTxAddress);
99 irtx.enableSW8b38KHzWP6 ();
100 if (enableBlink)
101 {
102 blink.begin((uint8_t)1,(uint8_t)3);
103 }
104 return (0);
105 }
106
107 private:
108};
109
SerialWombat.h
PCB0041_Remcon::irtx
SerialWombatIRTx irtx
Definition PCB0041_Remcon.h:78
PCB0041_Remcon::blink
SerialWombatBlink blink
Definition PCB0041_Remcon.h:79
PCB0041_Remcon::begin
int16_t begin(uint8_t i2cAddress, uint16_t irTxAddress=0x1234, bool enableBlink=true)
Initialize a PCB0048 Remcon pcb on a given I2C address.
Definition PCB0041_Remcon.h:94
PCB0041_Remcon::PCB0041_Remcon
PCB0041_Remcon()
Definition PCB0041_Remcon.h:74
PCB0041_Remcon::irrx
SerialWombatIRRx irrx
Definition PCB0041_Remcon.h:77
SerialWombatBlink
A class representing a Serial Wombat Blink Output.
Definition SerialWombatBlink.h:53
SerialWombatChip::SerialWombatChip
SerialWombatChip()
Definition SerialWombat.cpp:31
SerialWombatChip::begin
int16_t begin(HardwareSerial &serial, bool reset=true)
initialize a Serial Wombat chip to use a Serial Interface.
Definition SerialWombat.h:550
SerialWombatIRRx
A class for the Serial Wombat SW8B or SW18AB chips which received IR remote signals....
Definition SerialWombatIRRx.h:63
SerialWombatIRTx
A class for the Serial Wombat 8B or SW18AB chips which allows sending NEC IR Commands.
Definition SerialWombatIRTx.h:64