Serial Wombat Arduino Library

Loading...
Searching...
No Matches
SerialWombatResistanceInput Member List

This is the complete list of members for SerialWombatResistanceInput, including all inherited members.

_pin | SerialWombatPin | protected
_pinMode | SerialWombatPin | protected
_sw | SerialWombatPin | protected
AVERAGE enum value | SerialWombatAbstractProcessedInput |
begin(uint8_t pin) | SerialWombatResistanceInput | inline
begin(uint8_t pin, uint16_t averageSamples, uint16_t filterConstant) | SerialWombatResistanceInput | inline
begin(uint8_t pin, uint16_t averageSamples, uint16_t filterConstant, ResistanceInputPublicDataOutput publicDataOutput) | SerialWombatResistanceInput | inline
configureIntegrator(uint16_t negativeMaxIndex, uint16_t negativeMidIndex, uint16_t negativeDeadZone, uint16_t positiveDeadZone, uint16_t positiveMidIndex, uint16_t positiveMaxIndex, uint16_t midIncrement, uint16_t maxIncrement, uint16_t initialValue, uint8_t updateFrequencyMask=0) | SerialWombatAbstractProcessedInput | inline
configureOutputValue(OutputValue outputValue) | SerialWombatAbstractProcessedInput | inline
configureQueue(SerialWombatQueue *queue, Period period, bool queueHighByte=true, bool queueLowByte=true) | SerialWombatAbstractProcessedInput | inline
digitalRead() | SerialWombatPin | inline
digitalWrite(uint8_t val) | SerialWombatPin | inline
disable() | SerialWombatPin | inline
enableOpenDrain(bool enabled) | SerialWombatPin | inline
enablePulldown(bool enabled) | SerialWombatPin | inline
enablePullup(bool enabled) | SerialWombatPin | inline
FIRST_ORDER_FILTERED enum value | SerialWombatAbstractProcessedInput |
forceDMA(bool enabled) | SerialWombatPin | inline
initPacketNoResponse(uint8_t packetNumber, uint8_t param0=0x55, uint8_t param1=0x55, uint8_t param2=0x55, uint8_t param3=0x55, uint8_t param4=0x55) | SerialWombatPin | inline
initPacketNoResponse(uint8_t packetNumber, uint16_t param0=0x55, uint8_t param1=0x55, uint8_t param2=0x55, uint8_t param3=0x55) | SerialWombatPin | inline
initPacketNoResponse(uint8_t packetNumber, uint16_t param0, uint16_t param1, uint8_t param2=0x55) | SerialWombatPin | inline
LINEAR_MXB enum value | SerialWombatAbstractProcessedInput |
NONE enum value | SerialWombatAbstractProcessedInput |
OutputValue enum name | SerialWombatAbstractProcessedInput |
Period enum name | SerialWombatAbstractProcessedInput |
PERIOD_1024mS enum value | SerialWombatAbstractProcessedInput |
PERIOD_128mS enum value | SerialWombatAbstractProcessedInput |
PERIOD_16mS enum value | SerialWombatAbstractProcessedInput |
PERIOD_1mS enum value | SerialWombatAbstractProcessedInput |
PERIOD_256mS enum value | SerialWombatAbstractProcessedInput |
PERIOD_2mS enum value | SerialWombatAbstractProcessedInput |
PERIOD_32mS enum value | SerialWombatAbstractProcessedInput |
PERIOD_4mS enum value | SerialWombatAbstractProcessedInput |
PERIOD_512mS enum value | SerialWombatAbstractProcessedInput |
PERIOD_64mS enum value | SerialWombatAbstractProcessedInput |
PERIOD_8mS enum value | SerialWombatAbstractProcessedInput |
pin() | SerialWombatResistanceInput | inline virtual
pinMode(uint8_t mode, bool pullDown=false, bool openDrain=false) | SerialWombatPin | inline
RAW enum value | SerialWombatAbstractProcessedInput |
readAverage() | SerialWombatAbstractProcessedInput | inline
readAveragedOhms() | SerialWombatResistanceInput | inline
readFiltered() | SerialWombatAbstractProcessedInput | inline
readFilteredOhms() | SerialWombatResistanceInput | inline
readMaximum(bool resetAfterRead=false) | SerialWombatAbstractProcessedInput | inline
readMaximumOhms(bool resetAfterRead) | SerialWombatResistanceInput | inline
readMinimum(bool resetAfterRead=false) | SerialWombatAbstractProcessedInput | inline
readMinimumOhms(bool resetAfterRead) | SerialWombatResistanceInput | inline
readPublicData() | SerialWombatPin | inline
SCALE_RANGE enum value | SerialWombatAbstractProcessedInput |
SerialWombatAbstractProcessedInput(SerialWombatChip &sw) | SerialWombatAbstractProcessedInput | inline
SerialWombatPin(SerialWombatChip &serialWombatChip) | SerialWombatPin | inline
SerialWombatPin(SerialWombatChip &serialWombatChip, uint8_t pin) | SerialWombatPin | inline
SerialWombatResistanceInput(SerialWombatChip &serialWombatChip) | SerialWombatResistanceInput | inline
setPinNumberForTesting(uint8_t pin) | SerialWombatPin | inline
swPinModeNumber() | SerialWombatResistanceInput | inline virtual
Transform enum name | SerialWombatAbstractProcessedInput |
writeAveragingNumberOfSamples(uint16_t numberOfSamples) | SerialWombatAbstractProcessedInput | inline
writeExcludeBelowAbove(uint16_t low, uint16_t high) | SerialWombatAbstractProcessedInput | inline
writeFirstOrderFilteringConstant(uint16_t constant) | SerialWombatAbstractProcessedInput | inline
writeInverted(bool inverted) | SerialWombatAbstractProcessedInput | inline
writeProcessedInputEnable(bool enabled) | SerialWombatAbstractProcessedInput | inline
writePublicData(uint16_t value) | SerialWombatPin | inline
writeTransformLinearMXB(int32_t m, int32_t b) | SerialWombatAbstractProcessedInput | inline
writeTransformScaleRange(uint16_t min, uint16_t max) | SerialWombatAbstractProcessedInput | inline