<map id="SerialWombatIRTx" name="SerialWombatIRTx">
<area shape="rect" id="Node000001" title="A class for the Serial Wombat 8B or SW18AB chips which allows sending NEC IR Commands." alt="" coords="9,172,140,199"/>
<area shape="rect" id="Node000002" title=" " alt="" coords="5,96,69,123"/>
<area shape="poly" id="edge1_Node000001_Node000002" title=" " alt="" coords="52,135,70,170,66,173,48,137"/>
<area shape="rect" id="Node000003" href="$class_serial_wombat_pin.html" title="Describes a Serial Wombat Pin. Is base class for other pin modes." alt="" coords="92,96,214,123"/>
<area shape="poly" id="edge2_Node000001_Node000003" title=" " alt="" coords="130,135,89,174,86,170,127,131"/>
<area shape="rect" id="Node000004" href="$class_serial_wombat_chip.html" title="Class for a Serial Wombat chip. Each Serial Wombat chip on a project should have its own instance." alt="" coords="88,5,218,32"/>
<area shape="poly" id="edge3_Node000003_Node000004" title=" " alt="" coords="156,48,156,95,150,95,150,48"/>
</map>
