# New features of V2
  - Retentive D Memory from D200 - D1000
  - Retentive T Memory
  - Retentive D Memory
  - Retentive S Bit memory
  - Retentive M Bit memory
  - DS1307 RTC added
  - High speed output (Y4)
  - I2C port (4 pin) >>> GND,VCC,SDA.SCL

# PLC Compatible version (FX2N)
  - Input           :   6   Input   (24 VDC , Source type)
  - Output          :   4   Output  (Relay)
  - RS485           :   1   Channel (Auto direction)
  - Wifi            :   Yes
  - Ethernet        :   Yes (W5500)
  - Retentive memory:   8 K
  - I2C port        :   1 Channel
  - RTC             :   Yes (DS1307)

# DINO PLC V2 1.0.0
  - First released
# DINO PLC V2 1.0.1
  - Blynk fixed
# DINO PLC V2 1.0.2
  - Minor updated
# DINO PLC V2 1.0.3
