# Example L:  Verifying CRC Values<!-- {#example_l_page} -->

This is a simple demonstration of the SDI-12 library for Arduino.

This is a very basic (stripped down) example where the user initiates a measurement with a CRC check and receives and verifies the CRC response

[//]: # ( @section l_verify_crc_pio PlatformIO Configuration )

[//]: # ( @include{lineno} l_verify_crc/platformio.ini )

[//]: # ( @section l_verify_crc_code The Complete Example )

[//]: # ( @include{lineno} l_verify_crc/l_verify_crc.ino )
