# Example F: Basic Data Request to a Single Sensor<!--! {#example_f_page} -->

This is a simple demonstration of the SDI-12 library for Arduino.

This is a very basic (stripped down) example where the user initiates a measurement and receives the results to a terminal window without typing numerous commands into the terminal.

<!--! @section f_basic_data_request_pio PlatformIO Configuration -->

<!--! @include{lineno} f_basic_data_request/platformio.ini -->

<!--! @section f_basic_data_request_code The Complete Example -->

<!--! @include{lineno} f_basic_data_request/f_basic_data_request.ino -->
