| ButtonToSwitch Library for Arduino v4.0.1 A library that provides elaborated switch mechanism behavior simulation for digital signals inputs

Loading...
Searching...
No Matches
Here is a list of all documented functions with links to the class documentation for each member:

### - b -

- begin() : DblActnLtchMPBttn, DbncdMPBttn, HntdTmLtchMPBttn, LtchMPBttn, SnglSrvcVdblMPBttn, TmVdblMPBttn, XtrnUnltchMPBttn

### - c -

- clrStatus() : DblActnLtchMPBttn, DbncdMPBttn, DDlydDALtchMPBttn, HntdTmLtchMPBttn, LtchMPBttn, SldrDALtchMPBttn, TmLtchMPBttn, TmVdblMPBttn, VdblMPBttn, XtrnUnltchMPBttn

### - d -

- DblActnLtchMPBttn() : DblActnLtchMPBttn
- DbncdDlydMPBttn() : DbncdDlydMPBttn
- DbncdMPBttn() : DbncdMPBttn
- DDlydDALtchMPBttn() : DDlydDALtchMPBttn
- disable() : DbncdMPBttn

### - e -

- enable() : DbncdMPBttn
- end() : DbncdMPBttn

### - g -

- getCurDbncTime() : DbncdMPBttn
- getFnWhnTrnOff() : DbncdMPBttn
- getFnWhnTrnOffPilot() : HntdTmLtchMPBttn
- getFnWhnTrnOffScndry() : DblActnLtchMPBttn
- getFnWhnTrnOffVdd() : VdblMPBttn
- getFnWhnTrnOffWrnng() : HntdTmLtchMPBttn
- getFnWhnTrnOn() : DbncdMPBttn
- getFnWhnTrnOnPilot() : HntdTmLtchMPBttn
- getFnWhnTrnOnScndry() : DblActnLtchMPBttn
- getFnWhnTrnOnVdd() : VdblMPBttn
- getFnWhnTrnOnWrnng() : HntdTmLtchMPBttn
- getFrcOtptLvlWhnVdd() : VdblMPBttn
- getIsEnabled() : DbncdMPBttn
- getIsLatched() : LtchMPBttn
- getIsOn() : DbncdMPBttn
- getIsOnDisabled() : DbncdMPBttn
- getIsOnScndry() : DblActnLtchMPBttn
- getIsVoided() : VdblMPBttn
- getLstPollTime() : DbncdMPBttn
- getOtptCurVal() : SldrDALtchMPBttn
- getOtptCurValIsMax() : SldrDALtchMPBttn
- getOtptCurValIsMin() : SldrDALtchMPBttn
- getOtptSldrSpd() : SldrDALtchMPBttn
- getOtptSldrStpSize() : SldrDALtchMPBttn
- getOtptsSttsPkgd() : DbncdMPBttn
- getOtptValMax() : SldrDALtchMPBttn
- getOtptValMin() : SldrDALtchMPBttn
- getOutputsChange() : DbncdMPBttn
- getPilotOn() : HntdTmLtchMPBttn
- getPollPeriodMs() : DbncdMPBttn
- getScndModActvDly() : DblActnLtchMPBttn
- getSldrDirUp() : SldrDALtchMPBttn
- getSrvcTime() : TmLtchMPBttn
- getStOnWhnOtpFrcd() : VdblMPBttn
- getStrtDelay() : DbncdMPBttn
- getTrnOffASAP() : LtchMPBttn
- getUnlatchPend() : LtchMPBttn
- getUnlatchRlsPend() : LtchMPBttn
- getUpdTmrAttchd() : DbncdMPBttn
- getVoidTime() : TmVdblMPBttn
- getWrnngOn() : HntdTmLtchMPBttn

### - h -

- HntdTmLtchMPBttn() : HntdTmLtchMPBttn

### - i -

- init() : DbncdDlydMPBttn, DbncdMPBttn

### - l -

- LtchMPBttn() : LtchMPBttn

### - p -

- pause() : DbncdMPBttn

### - r -

- resetDbncTime() : DbncdMPBttn
- resetFda() : DbncdMPBttn
- resume() : DbncdMPBttn

### - s -

- setDbncTime() : DbncdMPBttn
- setFnWhnTrnOffPilotPtr() : HntdTmLtchMPBttn
- setFnWhnTrnOffPtr() : DbncdMPBttn
- setFnWhnTrnOffScndryPtr() : DblActnLtchMPBttn
- setFnWhnTrnOffVddPtr() : VdblMPBttn
- setFnWhnTrnOffWrnngPtr() : HntdTmLtchMPBttn
- setFnWhnTrnOnPilotPtr() : HntdTmLtchMPBttn
- setFnWhnTrnOnPtr() : DbncdMPBttn
- setFnWhnTrnOnScndryPtr() : DblActnLtchMPBttn
- setFnWhnTrnOnVddPtr() : VdblMPBttn
- setFnWhnTrnOnWrnngPtr() : HntdTmLtchMPBttn
- setIsNotVoided() : VdblMPBttn
- setIsOnDisabled() : DbncdMPBttn
- setIsVoided() : VdblMPBttn
- setKeepPilot() : HntdTmLtchMPBttn
- setOtptCurVal() : SldrDALtchMPBttn
- setOtptSldrSpd() : SldrDALtchMPBttn
- setOtptSldrStpSize() : SldrDALtchMPBttn
- setOtptValMax() : SldrDALtchMPBttn
- setOtptValMin() : SldrDALtchMPBttn
- setOutputsChange() : DbncdMPBttn
- setScndModActvDly() : DblActnLtchMPBttn
- setSldrDirDn() : SldrDALtchMPBttn
- setSldrDirUp() : SldrDALtchMPBttn
- setSrvcTime() : HntdTmLtchMPBttn, TmLtchMPBttn
- setStrtDelay() : DbncdDlydMPBttn
- setSwpDirOnEnd() : SldrDALtchMPBttn
- setSwpDirOnPrss() : SldrDALtchMPBttn
- setTmerRstbl() : TmLtchMPBttn
- setTrnOffASAP() : LtchMPBttn
- setUnlatchPend() : LtchMPBttn
- setUnlatchRlsPend() : LtchMPBttn
- setVoidTime() : TmVdblMPBttn
- setWrnngPrctg() : HntdTmLtchMPBttn
- SldrDALtchMPBttn() : SldrDALtchMPBttn
- SnglSrvcVdblMPBttn() : SnglSrvcVdblMPBttn
- swapSldrDir() : SldrDALtchMPBttn

### - t -

- TgglLtchMPBttn() : TgglLtchMPBttn
- TmLtchMPBttn() : TmLtchMPBttn
- TmVdblMPBttn() : TmVdblMPBttn

### - u -

- unlatch() : LtchMPBttn

### - v -

- VdblMPBttn() : VdblMPBttn

### - x -

- XtrnUnltchMPBttn() : XtrnUnltchMPBttn

### - ~ -

- ~DblActnLtchMPBttn() : DblActnLtchMPBttn
- ~DbncdMPBttn() : DbncdMPBttn
- ~DDlydDALtchMPBttn() : DDlydDALtchMPBttn
- ~SldrDALtchMPBttn() : SldrDALtchMPBttn
- ~SnglSrvcVdblMPBttn() : SnglSrvcVdblMPBttn
- ~TmVdblMPBttn() : TmVdblMPBttn
- ~VdblMPBttn() : VdblMPBttn