| ButtonToSwitch Library for Arduino v4.6.0 A library that provides elaborated switch mechanism behavior simulation for digital signals inputs

Loading...
Searching...
No Matches
Here is a list of all documented class members with links to the class documentation for each member:

### - s -

- setBeginDisabled() : DbncdMPBttn
- setDbncTime() : DbncdMPBttn
- setFnWhnTrnOffPilotPtr() : HntdTmLtchMPBttn
- setFnWhnTrnOffPtr() : DbncdMPBttn
- setFnWhnTrnOffScndryPtr() : DblActnLtchMPBttn
- setFnWhnTrnOffSldrDirUp() : SldrDALtchMPBttn
- setFnWhnTrnOffSldrMaxPtr() : SldrDALtchMPBttn
- setFnWhnTrnOffSldrMinPtr() : SldrDALtchMPBttn
- setFnWhnTrnOffVddPtr() : VdblMPBttn
- setFnWhnTrnOffWrnngPtr() : HntdTmLtchMPBttn
- setFnWhnTrnOnPilotPtr() : HntdTmLtchMPBttn
- setFnWhnTrnOnPtr() : DbncdMPBttn
- setFnWhnTrnOnScndryPtr() : DblActnLtchMPBttn
- setFnWhnTrnOnSldrDirUp() : SldrDALtchMPBttn
- setFnWhnTrnOnSldrMaxPtr() : SldrDALtchMPBttn
- setFnWhnTrnOnSldrMinPtr() : SldrDALtchMPBttn
- setFnWhnTrnOnVddPtr() : VdblMPBttn
- setFnWhnTrnOnWrnngPtr() : HntdTmLtchMPBttn
- setFVPPWhnTrnOff() : DbncdMPBttn
- setFVPPWhnTrnOffArgPtr() : DbncdMPBttn
- setFVPPWhnTrnOffPilot() : HntdTmLtchMPBttn
- setFVPPWhnTrnOffPilotArgPtr() : HntdTmLtchMPBttn
- setFVPPWhnTrnOffScndry() : DblActnLtchMPBttn
- setFVPPWhnTrnOffScndryArgPtr() : DblActnLtchMPBttn
- setFVPPWhnTrnOffSldrDirUp() : SldrDALtchMPBttn
- setFVPPWhnTrnOffSldrDirUpArgPtr() : SldrDALtchMPBttn
- setFVPPWhnTrnOffSldrMax() : SldrDALtchMPBttn
- setFVPPWhnTrnOffSldrMaxArgPtr() : SldrDALtchMPBttn
- setFVPPWhnTrnOffSldrMin() : SldrDALtchMPBttn
- setFVPPWhnTrnOffSldrMinArgPtr() : SldrDALtchMPBttn
- setFVPPWhnTrnOffVdd() : VdblMPBttn
- setFVPPWhnTrnOffVddArgPtr() : VdblMPBttn
- setFVPPWhnTrnOffWrnng() : HntdTmLtchMPBttn
- setFVPPWhnTrnOffWrnngArgPtr() : HntdTmLtchMPBttn
- setFVPPWhnTrnOn() : DbncdMPBttn
- setFVPPWhnTrnOnArgPtr() : DbncdMPBttn
- setFVPPWhnTrnOnPilot() : HntdTmLtchMPBttn
- setFVPPWhnTrnOnPilotArgPtr() : HntdTmLtchMPBttn
- setFVPPWhnTrnOnScndry() : DblActnLtchMPBttn
- setFVPPWhnTrnOnScndryArgPtr() : DblActnLtchMPBttn
- setFVPPWhnTrnOnSldrDirUp() : SldrDALtchMPBttn
- setFVPPWhnTrnOnSldrDirUpArgPtr() : SldrDALtchMPBttn
- setFVPPWhnTrnOnSldrMax() : SldrDALtchMPBttn
- setFVPPWhnTrnOnSldrMaxArgPtr() : SldrDALtchMPBttn
- setFVPPWhnTrnOnSldrMin() : SldrDALtchMPBttn
- setFVPPWhnTrnOnSldrMinArgPtr() : SldrDALtchMPBttn
- setFVPPWhnTrnOnVdd() : VdblMPBttn
- setFVPPWhnTrnOnVddArgPtr() : VdblMPBttn
- setFVPPWhnTrnOnWrnng() : HntdTmLtchMPBttn
- setFVPPWhnTrnOnWrnngArgPtr() : HntdTmLtchMPBttn
- setIsNotVoided() : VdblMPBttn
- setIsOnDisabled() : DbncdMPBttn
- setIsVoided() : VdblMPBttn
- setKeepPilot() : HntdTmLtchMPBttn
- setOtptCurVal() : SldrDALtchMPBttn
- setOtptSldrSpd() : SldrDALtchMPBttn
- setOtptSldrStpSize() : SldrDALtchMPBttn
- setOtptValMax() : SldrDALtchMPBttn
- setOtptValMin() : SldrDALtchMPBttn
- setOutputsChange() : DbncdMPBttn
- setScndModActvDly() : DblActnLtchMPBttn
- setSldrDirDn() : SldrDALtchMPBttn
- setSldrDirUp() : SldrDALtchMPBttn
- setSrvcTime() : HntdTmLtchMPBttn, TmLtchMPBttn
- setStrtDelay() : DbncdDlydMPBttn
- setSwpDirOnEnd() : SldrDALtchMPBttn
- setSwpDirOnPrss() : SldrDALtchMPBttn
- setTmerRstbl() : TmLtchMPBttn
- setTrnOffASAP() : LtchMPBttn
- setUnlatchPend() : LtchMPBttn
- setUnlatchRlsPend() : LtchMPBttn
- setVoidTime() : TmVdblMPBttn
- setWrnngPrctg() : HntdTmLtchMPBttn
- SldrDALtchMPBttn() : SldrDALtchMPBttn
- SnglSrvcVdblMPBttn() : SnglSrvcVdblMPBttn
- swapSldrDir() : SldrDALtchMPBttn