| ButtonToSwitch Library for ESP32 (Arduino) v4.6.1 A library that provides elaborated switch mechanism behavior simulation for digital signals inputs

Loading...
Searching...
No Matches
XtrnUnltchMPBttn Class Reference

Models an External Unlatch LDD-MPB, a.k.a. Emergency Latched Switch (XULDD-MPB) More...

`#include <ButtonToSwitch_ESP32.h>`

Inheritance diagram for XtrnUnltchMPBttn:
[legend]
Collaboration diagram for XtrnUnltchMPBttn:
[legend]

## Public Member Functions
| XtrnUnltchMPBttn ()
| Default constructor.
| XtrnUnltchMPBttn (const int8_t &mpbttnPin, DbncdDlydMPBttn *unLtchBttn, const bool &pulledUp, const bool &typeNO, const unsigned long int &dbncTimeOrigSett, const unsigned long int &strtDelay)
| Class constructor.
| XtrnUnltchMPBttn (const int8_t &mpbttnPin, const bool &pulledUp, const bool &typeNO, const unsigned long int &dbncTimeOrigSett, const unsigned long int &strtDelay)
| Class constructor.
virtual bool | begin (const unsigned long int &pollDelayMs=_StdPollDelay)
| See DbncdMPBttn::begin(const unsigned long int)
void | clrStatus (bool clrIsOn=true)
| See DbncdMPBttn::clrStatus(bool)
Public Member Functions inherited from LtchMPBttn
| LtchMPBttn ()
| Default constructor.
| LtchMPBttn (const int8_t &mpbttnPin, const bool &pulledUp=true, const bool &typeNO=true, const unsigned long int &dbncTimeOrigSett=0, const unsigned long int &strtDelay=0)
| Class constructor.
| LtchMPBttn (const LtchMPBttn &other)
| Copy constructor.
virtual | ~LtchMPBttn ()
| Class virtual destructor.
void | clrStatus (bool clrIsOn=true)
| See DbncdMPBttn::clrStatus(bool)
const bool | getIsLatched () const
| Returns the value of the isLatched attribute flag, indicating the Latched or Unlatched condition of the object.
bool | getTrnOffASAP ()
| Returns the value of the trnOffASAP attribute flag.
const bool | getUnlatchPend () const
| Returns the value of the "Valid Unlatch Pending" attribute.
const bool | getUnlatchRlsPend () const
| Returns the value of the "Valid Unlatch Release Pending" attribute.
void | setTrnOffASAP (const bool &newVal)
| Sets the value of the trnOffASAP attribute.
void | setUnlatchPend (const bool &newVal)
| Sets the value of the "Valid Unlatch Pending" attribute.
void | setUnlatchRlsPend (const bool &newVal)
| Sets the value of the "Valid Unlatch Release Pending" attribute.
bool | unlatch ()
| Sets the values of the flags needed to unlatch a latched MPB.
Public Member Functions inherited from DbncdDlydMPBttn
| DbncdDlydMPBttn ()
| Default constructor.
| DbncdDlydMPBttn (const int8_t &mpbttnPin, const bool &pulledUp=true, const bool &typeNO=true, const unsigned long int &dbncTimeOrigSett=0, const unsigned long int &strtDelay=0)
| Class constructor.
| DbncdDlydMPBttn (const DbncdDlydMPBttn &other)
| Copy constructor.
virtual | ~DbncdDlydMPBttn ()
| Class destructor.
bool | init (const int8_t &mpbttnPin, const bool &pulledUp=true, const bool &typeNO=true, const unsigned long int &dbncTimeOrigSett=0, const unsigned long int &strtDelay=0)
| see DbncdMPBttn::init(const int8_t, const bool, const bool, const unsigned long int)
void | setStrtDelay (const unsigned long int &newStrtDelay)
| Sets a new value to the "Start Delay" strtDelay attribute.
Public Member Functions inherited from DbncdMPBttn
| DbncdMPBttn ()
| Default class constructor.
| DbncdMPBttn (const int8_t &mpbttnPin, const bool &pulledUp=true, const bool &typeNO=true, const unsigned long int &dbncTimeOrigSett=0)
| Class constructor.
| DbncdMPBttn (const DbncdMPBttn &other)
| Copy constructor.
virtual | ~DbncdMPBttn ()
| Default virtual destructor.
void | clrStatus (bool clrIsOn=true)
| Clears and resets flags, timers and counters modified through the object's signals processing.
void | disable ()
| Disables the input signal processing, ignoring the changes of its values.
void | enable ()
| Enables the input signal processing.
bool | end ()
| Detaches the object from the timer that monitors the input pins, compute and updates the object's status. The timer daemon entry is deleted for the object.
const unsigned long int | getCurDbncTime () const
| Returns the current debounce period time set for the object.
fncPtrType | getFnWhnTrnOff ()
| Returns a pointer to a function that is set to execute every time the object enters the Off State.
fncPtrType | getFnWhnTrnOn ()
| Returns a pointer to a function that is set to execute every time the object enters the On State.
fncVdPtrPrmPtrType | getFVPPWhnTrnOff ()
| Returns a pointer to a function that is set to execute every time the object enters the Off State.
void * | getFVPPWhnTrnOffArgPtr ()
| Returns a pointer to the argument to be passed to the function set to execute every time the object enters the Off State.
fncVdPtrPrmPtrType | getFVPPWhnTrnOn ()
| Returns a pointer to a function that is set to execute every time the object enters the On State.
void * | getFVPPWhnTrnOnArgPtr ()
| Returns a pointer to the argument to be passed to the function set to execute every time the object enters the On State.
const bool | getIsEnabled () const
| Returns the value of the isEnabled attribute flag, indicating the Enabled or Disabled status of the object.
const bool | getIsOn () const
| Returns the value of the isOn attribute flag.
const bool | getIsOnDisabled () const
| Returns the value of the isOnDisabled attribute flag.
const DbncdMPBttn * | getMpbInstnc () const
| Returns a pointer to the present instanced object.
const uint32_t | getOtptsSttsPkgd ()
| Returns the relevant attribute flags values for the object state encoded as a 32 bits value, required to pass current state of the object to another thread/task managing the outputs.
const bool | getOutputsChange () const
| Returns the value of the outputsChange attribute flag.
unsigned long int | getStrtDelay ()
| Returns the current value of strtDelay attribute.
const TaskHandle_t | getTaskToNotify () const
| Returns the task to be notified by the object when its output flags changes.
const TaskHandle_t | getTaskWhileOn ()
| Returns the task to be run (resumed) while the object is in the On state.
bool | init (const int8_t &mpbttnPin, const bool &pulledUp=true, const bool &typeNO=true, const unsigned long int &dbncTimeOrigSett=0)
| Initializes an object instantiated by the default constructor.
bool | pause ()
| Pauses the software timer updating the computation of the object's internal flags value.
void | resetDbncTime ()
| Resets the debounce process time of the object to the value used at instantiation.
void | resetFda ()
| Resets the MPB behavior automaton to it's Initial or Start State
bool | resume ()
| Restarts the software timer updating the calculation of the object internal flags.
void | setBeginDisabled (const bool &newBeginDisabled=false)
| Sets the starting isDisabled state.
bool | setDbncTime (const unsigned long int &newDbncTime)
| Sets the debounce process time.
void | setFnWhnTrnOffPtr (fncPtrType newFnWhnTrnOff)
| Sets the function that will be called to execute every time the object enters the Off State.
void | setFnWhnTrnOnPtr (fncPtrType newFnWhnTrnOn)
| Sets the function that will be called to execute every time the object enters the On State.
void | setFVPPWhnTrnOff (fncVdPtrPrmPtrType newFVPPWhnTrnOff, void *argPtr=nullptr)
| Sets a function to be executed every time the object enters the Off State.
void | setFVPPWhnTrnOffArgPtr (void *newFVPPWhnTrnOffArgPtr)
| Sets a pointer to an argument to be passed to the function set to execute every time the object enters the Off State.
void | setFVPPWhnTrnOn (fncVdPtrPrmPtrType newFVPPWhnTrnOn, void *argPtr=nullptr)
| Sets a function to be executed every time the object enters the On State.
void | setFVPPWhnTrnOnArgPtr (void *newFVPPWhnTrnOnArgPtr)
| Sets a pointer to an argument to be passed to the function set to execute every time the object enters the On State.
void | setIsOnDisabled (const bool &newIsOnDisabled)
| Sets the value of the isOnDisabled attribute flag.
void | setOutputsChange (bool newOutputsChange)
| Sets the value of the attribute flag indicating if a change took place in any of the output attribute flags (IsOn included).
void | setTaskToNotify (const TaskHandle_t &newTaskHandle)
| Sets the handle to the task to be notified by the object when its output attribute flags changes.
virtual void | setTaskWhileOn (const TaskHandle_t &newTaskHandle)
| Sets the task to be run while the object is in the On state.

## Detailed Description

Models an External Unlatch LDD-MPB, a.k.a. Emergency Latched Switch (XULDD-MPB)

The External released toggle switch (a.k.a. Emergency latched), keeps the On state since the moment the signal is stable (debounced & delayed), and until an external signal is received. This kind of switch is used when an "abnormal situation" demands the push of the switch On, but a higher authority is needed to reset it to Off from a different signal source. The On State will then not only start a response to the exception arisen, but will be kept to flag the triggering event. Smoke, flood, intrusion alarms and "last man locks" are some examples of the use of this switch. As the external release signal can be physical or logical generated it can be implemented to be received from a switch or a remote signal of any usual kind.

class XtrnUnltchMPBttn

## Constructor & Destructor Documentation

## ◆ XtrnUnltchMPBttn() [1/2]

XtrnUnltchMPBttn::XtrnUnltchMPBttn | ( | const int8_t & | mpbttnPin,
|  | DbncdDlydMPBttn * | unLtchBttn,
|  | const bool & | pulledUp,
|  | const bool & | typeNO,
|  | const unsigned long int & | dbncTimeOrigSett,
|  | const unsigned long int & | strtDelay )

Class constructor.

This class constructor makes specific reference to a source for the unlatch signal by including a parameter referencing an object that implements the needed getIsOn() method to get the external unlatch signal.

Parameters

  unLtchBttn | Pointer to a DbncdDlydMPBttn object that will provide the unlatch source signal through it's getIsOn() method.

Warning
  Referencing a DbncdDlydMPBttn subclass object that keeps the isOn flag set for a preset time period might affect the latching/unlatching process, as this class's objects don't check for the isOn condition of the unlatching object prior to setting it's own isOn flag.

Note
  For the other parameters see DbncdDlydMPBttn(const int8_t, const bool, const bool, const unsigned long int, const unsigned long int)
  Other unlatch signal origins might be developed through the unlatch() method provided.

Here is the call graph for this function:

## ◆ XtrnUnltchMPBttn() [2/2]

XtrnUnltchMPBttn::XtrnUnltchMPBttn | ( | const int8_t & | mpbttnPin,
|  | const bool & | pulledUp,
|  | const bool & | typeNO,
|  | const unsigned long int & | dbncTimeOrigSett,
|  | const unsigned long int & | strtDelay )

Class constructor.

This class constructor instantiates an object that relies on the unlatch() method invocation to release the latched MPB

Note
  For the parameters see DbncdDlydMPBttn(const int8_t, const bool, const bool, const unsigned long int, const unsigned long int)

Here is the call graph for this function: