Seven Segments Displays Agnostic Library for ESP32 (Arduino) v3.2.0 A library that provides a class that models a Seven Segment Display and provides an unified API through it's members independently of the display technology.

Loading...
Searching...
No Matches
SevenSegDisplays Member List

This is the complete list of members for SevenSegDisplays, including all inherited members.

begin(uint32_t updtLps=0) | SevenSegDisplays | virtual
blink() | SevenSegDisplays |
blink(const uint32_t &onRate, const uint32_t &offRate=0) | SevenSegDisplays |
clear() | SevenSegDisplays |
doubleGauge(const int &levelLeft, const int &levelRight, char labelLeft=' ', char labelRight=' ') | SevenSegDisplays |
end() | SevenSegDisplays |
gauge(const int &level, char label=' ') | SevenSegDisplays |
gauge(const double &level, char label=' ') | SevenSegDisplays |
getCurBrghtnssLvl() | SevenSegDisplays |
getDigitsQty() | SevenSegDisplays |
getDspCount() | SevenSegDisplays |
getDspIsDmmbl() | SevenSegDisplays |
getDspUndrlHwPtr() | SevenSegDisplays |
getDspValMax() | SevenSegDisplays |
getDspValMin() | SevenSegDisplays |
getIsOn() | SevenSegDisplays |
getMaxBlinkRate() | SevenSegDisplays |
getMaxBrghtnssLvl() | SevenSegDisplays |
getMinBlinkRate() | SevenSegDisplays |
getMinBrghtnssLvl() | SevenSegDisplays |
getSerialNbr() | SevenSegDisplays |
isBlank() | SevenSegDisplays |
isBlinking() | SevenSegDisplays |
isWaiting() | SevenSegDisplays |
noBlink() | SevenSegDisplays |
noWait() | SevenSegDisplays |
print(String text) | SevenSegDisplays |
print(const int32_t &value, bool rgtAlgn=false, bool zeroPad=false) | SevenSegDisplays |
print(const double &value, const unsigned int &decPlaces, bool rgtAlgn=false, bool zeroPad=false) | SevenSegDisplays |
resetBlinkMask() | SevenSegDisplays |
setBlinkMask(const bool *newBlnkMsk) | SevenSegDisplays |
setBlinkRate(const uint32_t &newOnRate, const uint32_t &newOffRate=0) | SevenSegDisplays |
setBrghtnssLvl(const uint8_t &newBrghtnssLvl) | SevenSegDisplays |
setWaitChar(const char &newChar) | SevenSegDisplays |
setWaitRate(const uint32_t &newWaitRate) | SevenSegDisplays |
SevenSegDisplays(SevenSegDispHw *dspUndrlHwPtr) | SevenSegDisplays |
turnOff() | SevenSegDisplays |
turnOn() | SevenSegDisplays |
turnOn(const uint8_t &newBrghtnssLvl) | SevenSegDisplays |
wait() | SevenSegDisplays |
wait(const uint32_t &newWaitRate) | SevenSegDisplays |
write(const uint8_t &segments, const uint8_t &port) | SevenSegDisplays |
write(const String &character, const uint8_t &port) | SevenSegDisplays |
~SevenSegDisplays() | SevenSegDisplays |