Seven Segments Displays Agnostic Library for ESP32 (Arduino) v3.2.0 A library that provides a class that models a Seven Segment Display and provides an unified API through it's members independently of the display technology.

Loading...
Searching...
No Matches
Class Hierarchy

Go to the graphical class hierarchy

This inheritance list is sorted roughly, but not completely, alphabetically:
[detail level 1 2 3 4]

▼C SevenSegDispHw | Base abstract class models a generic Seven Segment display hardware
▼C SevenSegDynamic | Abstract class models a generic dynamically updated Seven Segment display hardware
C SevenSegDynDummy | Models a dynamic display with no screen, for tests or remote display of the data.
C SevenSegDynHC595 | Models seven segment displays driven by two 74HC595 shift registers
▼C SevenSegStatic | Abstract class that models displays that don't need permanent MCU data updating to keep the data correctly displayed
C SevenSegMax7219 | Models a Seven Segment display hardware using a Max7219 display controller component
C SevenSegStatHC595 | Models displays driven by 74HC595 or similar shift registers, one shift register per display port, wired so that the eight output pins of each shift register is connected to the 8 segment pins of the corresponding display module.
▼C SevenSegTM163X | Abstract class that models Seven Segments LEDs static displays hardware using Titan Micro TM163X series chips as display controller component
C SevenSegTM1636 | Models a Seven Segment display hardware controlled by a TM1636 display controller component.
C SevenSegTM1637 | Models a Seven Segment display hardware controlled by a TM1637 display controller component.
C SevenSegTM1639 | Models a Seven Segment display hardware controlled by a TM1639 display controller component.
C SevenSegDisplays | Default constructor