Seven Segments Displays Agnostic Library for ESP32 (Arduino) v3.2.0 A library that provides a class that models a Seven Segment Display and provides an unified API through it's members independently of the display technology.

Loading...
Searching...
No Matches
Here is a list of all documented variables with links to the class documentation for each member:

- _allLedsOff : SevenSegDispHw
- _brghtnssLvl : SevenSegDispHw
- _brghtnssLvlMax : SevenSegDispHw
- _brghtnssLvlMin : SevenSegDispHw
- _dspBlankBuffPtr : SevenSegDispHw
- _dspBuffPtr : SevenSegDispHw
- _dspBuffPtrBkp : SevenSegDispHw
- _isOn : SevenSegDispHw
- _lclDspBuffPtr : SevenSegMax7219, SevenSegTM163X
- _xcdDspBuffPtr : SevenSegDispHw
- _xcdDspDigitsQty : SevenSegDispHw