| MD_MAXPanel LED Matrix Panel Arduino Library 1.4 Library to control a panel of connected MAX72XX devices

Loading...
Searching...
No Matches
Macros
MD_MAXPanel_lib.h File Reference

Includes library only definitions. More...

This graph shows which files directly or indirectly include this file:

## Macros
#define | MP_DEBUG 0
| Enable or disable (default) debugging output from the MD_MAX72xx library.
#define | PRINT(s, v)
| Print a string followed by a value (decimal)
#define | PRINTX(s, v)
| Print a string followed by a value (hex)
#define | PRINTB(s, v)
| Print a string followed by a value (binary)
#define | PRINTS(s)
| Print a string.
#define | X2COL(x, y) (((y / ROW_SIZE) * (getXMax() + 1)) + (getXMax() - (x % (getXMax() + 1))))
| Convert x coord to linear coord.
#define | Y2ROW(x, y) (ROW_SIZE - (y % ROW_SIZE) - 1)
| Convert y coord to linear coord.
#define | CHAR_SPACING_DEFAULT 1
| Default number of pixels between characters.

## Detailed Description

Includes library only definitions.