| MD_MAXPanel LED Matrix Panel Arduino Library 1.4 Library to control a panel of connected MAX72XX devices

Loading...
Searching...
No Matches
Revision History

Jun 2023 version 1.4.0

- Added Scoreboard example
- begin() returns bool value

Nov 2022 version 1.3.2

- Fixed incorrect reference to MD_MAX72XX in constructor

Sep 2022 version 1.3.1

- Updated illegal repeat for default parameters in function

May 2022 version 1.3.0

- Added LEDaSketch example
- Added constructor with specified SPI interface

Nov 2018 version 1.2.3

- Corrected default parameters for WEMOS compiler

Oct 2018 version 1.2.2

- Corrected some documentation mistakes

Oct 2018 version 1.2.1

- Updated library.properties and READ.MD files

Sep 2018 version 1.2.0

- Fixed reported WEMOS D1 compiler issues
- Added polygon Fill functions contributed by AndreasPercher

Jul 2018 version 1.1.1

- Finalized preferred orientation for examples

Jul 2018 version 1.1.0

- Renamed textRotation_t to rotation_t
- Allow rotation of display (eg, landscape to portrait)
- Restored missing bricks example

Jun 2018 version 1.0.1

- Extracted common elements of examples in .h file

Jun 2018 version 1.0.0

- First Release