| MD_TCS230 Color Sensor Arduino Library 1.2 Library to control TCS230 Color Sensor

Loading...
Searching...
No Matches
MD_TCS230 Member List

This is the complete list of members for MD_TCS230, including all inherited members.

available(void) | MD_TCS230 |
begin(void) | MD_TCS230 |
getRaw(sensorData *d) | MD_TCS230 |
getRGB(colorData *rgb) | MD_TCS230 |
MD_TCS230(uint8_t s2, uint8_t s3) | MD_TCS230 |
MD_TCS230(uint8_t s2, uint8_t s3, uint8_t oe) | MD_TCS230 |
MD_TCS230(uint8_t s2, uint8_t s3, uint8_t s0, uint8_t s1) | MD_TCS230 |
MD_TCS230(uint8_t s2, uint8_t s3, uint8_t s0, uint8_t s1, uint8_t oe) | MD_TCS230 |
read(void) | MD_TCS230 |
readSingle(void) | MD_TCS230 |
setDarkCal(sensorData *d) | MD_TCS230 |
setEnable(bool t) | MD_TCS230 |
setFilter(uint8_t f) | MD_TCS230 |
setFrequency(uint8_t f) | MD_TCS230 |
setSampling(uint8_t t) | MD_TCS230 |
setWhiteCal(sensorData *d) | MD_TCS230 |
~MD_TCS230(void) | MD_TCS230 |