BOARD:  Arduino UNO
IDE:    1.8.19

(Hardware SPI)

INA229_LIB_VERSION: 0.3.0


========================================================
Speed: 1000000

test_core
getBusVoltage:	68
getShuntVoltage:	72
getCurrent:	68
getPower:	80
getTemperature:	60
getEnergy:	100
getCharge:	92

test_config
getAccumulation:	44
getConversionDelay:	52
getTemperatureCompensation:	48
getADCRange:	52

test_adc_config
getMode:	48
getBusVoltageConversionTime:	48
getShuntVoltageConversionTime:	52
getTemperatureConversionTime:	48
getAverage:	48

test_others
getShuntTemperatureCoefficent:	48
getDiagnoseAlert:	48

test_thresholds
getShuntOvervoltageTH:	48
getShuntUndervoltageTH:	44
getBusOvervoltageTH:	44
getBusUndervoltageTH:	48
getTemperatureOverLimitTH:	48
getPowerOverLimitTH:	48

========================================================
Speed: 2000000

test_core
getBusVoltage:	52
getShuntVoltage:	52
getCurrent:	56
getPower:	64
getTemperature:	48
getEnergy:	76
getCharge:	68

test_config
getAccumulation:	36
getConversionDelay:	36
getTemperatureCompensation:	44
getADCRange:	36

test_adc_config
getMode:	32
getBusVoltageConversionTime:	36
getShuntVoltageConversionTime:	36
getTemperatureConversionTime:	36
getAverage:	36

test_others
getShuntTemperatureCoefficent:	36
getDiagnoseAlert:	36

test_thresholds
getShuntOvervoltageTH:	36
getShuntUndervoltageTH:	36
getBusOvervoltageTH:	36
getBusUndervoltageTH:	32
getTemperatureOverLimitTH:	32
getPowerOverLimitTH:	32

========================================================
Speed: 4000000

test_core
getBusVoltage:	40
getShuntVoltage:	40
getCurrent:	40
getPower:	44
getTemperature:	32
getEnergy:	64
getCharge:	60

test_config
getAccumulation:	36
getConversionDelay:	32
getTemperatureCompensation:	28
getADCRange:	32

test_adc_config
getMode:	28
getBusVoltageConversionTime:	28
getShuntVoltageConversionTime:	32
getTemperatureConversionTime:	32
getAverage:	32

test_others
getShuntTemperatureCoefficent:	28
getDiagnoseAlert:	28

test_thresholds
getShuntOvervoltageTH:	28
getShuntUndervoltageTH:	32
getBusOvervoltageTH:	28
getBusUndervoltageTH:	28
getTemperatureOverLimitTH:	32
getPowerOverLimitTH:	28

========================================================
Speed: 8000000

test_core
getBusVoltage:	40
getShuntVoltage:	40
getCurrent:	44
getPower:	52
getTemperature:	36
getEnergy:	56
getCharge:	52

test_config
getAccumulation:	24
getConversionDelay:	28
getTemperatureCompensation:	28
getADCRange:	28

test_adc_config
getMode:	28
getBusVoltageConversionTime:	28
getShuntVoltageConversionTime:	28
getTemperatureConversionTime:	24
getAverage:	28

test_others
getShuntTemperatureCoefficent:	28
getDiagnoseAlert:	24

test_thresholds
getShuntOvervoltageTH:	32
getShuntUndervoltageTH:	32
getBusOvervoltageTH:	32
getBusUndervoltageTH:	28
getTemperatureOverLimitTH:	28
getPowerOverLimitTH:	32

Done