BOARD:  Arduino UNO
IDE:    1.8.19

(Hardware SPI)

INA229_LIB_VERSION: 0.1.0


========================================================
Speed: 1000000

test_core
getBusVoltage:	68
getShuntVoltage:	116
getCurrent:	68
getPower:	80
getTemperature:	56
getEnergy:	184
getCharge:	176

test_config
getAccumulation:	48
getConversionDelay:	48
getTemperatureCompensation:	48
getADCRange:	48

test_adc_config
getMode:	48
getBusVoltageConversionTime:	48
getShuntVoltageConversionTime:	48
getTemperatureConversionTime:	48
getAverage:	48

test_others
getShuntTemperatureCoefficent:	44
getDiagnoseAlert:	48

test_thresholds
getShuntOvervoltageTH:	48
getShuntUndervoltageTH:	48
getBusOvervoltageTH:	48
getBusUndervoltageTH:	44
getTemperatureOverLimitTH:	44
getPowerOverLimitTH:	44

========================================================
Speed: 2000000

test_core
getBusVoltage:	52
getShuntVoltage:	88
getCurrent:	56
getPower:	64
getTemperature:	44
getEnergy:	156
getCharge:	152

test_config
getAccumulation:	36
getConversionDelay:	40
getTemperatureCompensation:	44
getADCRange:	36

test_adc_config
getMode:	36
getBusVoltageConversionTime:	36
getShuntVoltageConversionTime:	36
getTemperatureConversionTime:	36
getAverage:	36

test_others
getShuntTemperatureCoefficent:	36
getDiagnoseAlert:	36

test_thresholds
getShuntOvervoltageTH:	36
getShuntUndervoltageTH:	36
getBusOvervoltageTH:	36
getBusUndervoltageTH:	36
getTemperatureOverLimitTH:	36
getPowerOverLimitTH:	32

========================================================
Speed: 4000000

test_core
getBusVoltage:	44
getShuntVoltage:	72
getCurrent:	48
getPower:	56
getTemperature:	40
getEnergy:	148
getCharge:	140

test_config
getAccumulation:	28
getConversionDelay:	28
getTemperatureCompensation:	32
getADCRange:	32

test_adc_config
getMode:	28
getBusVoltageConversionTime:	32
getShuntVoltageConversionTime:	28
getTemperatureConversionTime:	28
getAverage:	32

test_others
getShuntTemperatureCoefficent:	32
getDiagnoseAlert:	32

test_thresholds
getShuntOvervoltageTH:	28
getShuntUndervoltageTH:	28
getBusOvervoltageTH:	28
getBusUndervoltageTH:	28
getTemperatureOverLimitTH:	28
getPowerOverLimitTH:	28

========================================================
Speed: 8000000

test_core
getBusVoltage:	44
getShuntVoltage:	68
getCurrent:	40
getPower:	48
getTemperature:	40
getEnergy:	140
getCharge:	132

test_config
getAccumulation:	24
getConversionDelay:	28
getTemperatureCompensation:	28
getADCRange:	28

test_adc_config
getMode:	28
getBusVoltageConversionTime:	24
getShuntVoltageConversionTime:	28
getTemperatureConversionTime:	28
getAverage:	28

test_others
getShuntTemperatureCoefficent:	24
getDiagnoseAlert:	28

test_thresholds
getShuntOvervoltageTH:	28
getShuntUndervoltageTH:	28
getBusOvervoltageTH:	24
getBusUndervoltageTH:	24
getTemperatureOverLimitTH:	24
getPowerOverLimitTH:	28

Done