BOARD:  Arduino UNO
IDE:    1.8.19

(Hardware SPI)

INA229_LIB_VERSION: 0.1.1


========================================================
Speed: 1000000

test_core
getBusVoltage:	68
getShuntVoltage:	72
getCurrent:	68
getPower:	80
getTemperature:	60
getEnergy:	184
getCharge:	172

test_config
getAccumulation:	44
getConversionDelay:	48
getTemperatureCompensation:	52
getADCRange:	4

test_adc_config
getMode:	48
getBusVoltageConversionTime:	44
getShuntVoltageConversionTime:	48
getTemperatureConversionTime:	48
getAverage:	48

test_others
getShuntTemperatureCoefficent:	44
getDiagnoseAlert:	48

test_thresholds
getShuntOvervoltageTH:	48
getShuntUndervoltageTH:	48
getBusOvervoltageTH:	44
getBusUndervoltageTH:	44
getTemperatureOverLimitTH:	48
getPowerOverLimitTH:	48

========================================================
Speed: 2000000

test_core
getBusVoltage:	52
getShuntVoltage:	56
getCurrent:	52
getPower:	60
getTemperature:	48
getEnergy:	160
getCharge:	152

test_config
getAccumulation:	36
getConversionDelay:	36
getTemperatureCompensation:	36
getADCRange:	4

test_adc_config
getMode:	36
getBusVoltageConversionTime:	36
getShuntVoltageConversionTime:	40
getTemperatureConversionTime:	36
getAverage:	32

test_others
getShuntTemperatureCoefficent:	32
getDiagnoseAlert:	32

test_thresholds
getShuntOvervoltageTH:	32
getShuntUndervoltageTH:	36
getBusOvervoltageTH:	36
getBusUndervoltageTH:	32
getTemperatureOverLimitTH:	32
getPowerOverLimitTH:	32

========================================================
Speed: 4000000

test_core
getBusVoltage:	44
getShuntVoltage:	48
getCurrent:	44
getPower:	52
getTemperature:	40
getEnergy:	148
getCharge:	136

test_config
getAccumulation:	32
getConversionDelay:	32
getTemperatureCompensation:	32
getADCRange:	4

test_adc_config
getMode:	28
getBusVoltageConversionTime:	32
getShuntVoltageConversionTime:	28
getTemperatureConversionTime:	28
getAverage:	32

test_others
getShuntTemperatureCoefficent:	32
getDiagnoseAlert:	28

test_thresholds
getShuntOvervoltageTH:	28
getShuntUndervoltageTH:	28
getBusOvervoltageTH:	28
getBusUndervoltageTH:	28
getTemperatureOverLimitTH:	28
getPowerOverLimitTH:	32

========================================================
Speed: 8000000

test_core
getBusVoltage:	40
getShuntVoltage:	44
getCurrent:	44
getPower:	48
getTemperature:	36
getEnergy:	140
getCharge:	132

test_config
getAccumulation:	24
getConversionDelay:	28
getTemperatureCompensation:	28
getADCRange:	4

test_adc_config
getMode:	24
getBusVoltageConversionTime:	28
getShuntVoltageConversionTime:	28
getTemperatureConversionTime:	28
getAverage:	28

test_others
getShuntTemperatureCoefficent:	28
getDiagnoseAlert:	24

test_thresholds
getShuntOvervoltageTH:	24
getShuntUndervoltageTH:	28
getBusOvervoltageTH:	24
getBusUndervoltageTH:	24
getTemperatureOverLimitTH:	24
getPowerOverLimitTH:	28

Done