BOARD:  Arduino UNO R3
IDE:    1.8.19

(Hardware SPI)

D:\Rob\WORK\Arduino\libraries\INA229\examples\INA229_performance\INA229_performance.ino

INA229_LIB_VERSION: 0.4.1


========================================================
Speed: 1000000

test_core
getBusVoltage:	64
getShuntVoltage:	64
getCurrent:	68
getPower:	68
getTemperature:	52
getEnergy:	100
getCharge:	92

test_config
getAccumulation:	44
getConversionDelay:	48
getTemperatureCompensation:	48
getADCRange:	48

test_adc_config
getMode:	48
getBusVoltageConversionTime:	44
getShuntVoltageConversionTime:	48
getTemperatureConversionTime:	48
getAverage:	48

test_others
getShuntTemperatureCoefficent:	44
getDiagnoseAlert:	44

test_thresholds
getShuntOvervoltageTH:	44
getShuntUndervoltageTH:	44
getBusOvervoltageTH:	44
getBusUndervoltageTH:	44
getTemperatureOverLimitTH:	44
getPowerOverLimitTH:	48

========================================================
Speed: 2000000

test_core
getBusVoltage:	48
getShuntVoltage:	52
getCurrent:	48
getPower:	52
getTemperature:	44
getEnergy:	76
getCharge:	72

test_config
getAccumulation:	40
getConversionDelay:	36
getTemperatureCompensation:	36
getADCRange:	40

test_adc_config
getMode:	32
getBusVoltageConversionTime:	36
getShuntVoltageConversionTime:	36
getTemperatureConversionTime:	36
getAverage:	36

test_others
getShuntTemperatureCoefficent:	36
getDiagnoseAlert:	36

test_thresholds
getShuntOvervoltageTH:	32
getShuntUndervoltageTH:	32
getBusOvervoltageTH:	32
getBusUndervoltageTH:	36
getTemperatureOverLimitTH:	36
getPowerOverLimitTH:	32

========================================================
Speed: 4000000

test_core
getBusVoltage:	40
getShuntVoltage:	40
getCurrent:	40
getPower:	44
getTemperature:	32
getEnergy:	60
getCharge:	60

test_config
getAccumulation:	32
getConversionDelay:	28
getTemperatureCompensation:	28
getADCRange:	32

test_adc_config
getMode:	28
getBusVoltageConversionTime:	32
getShuntVoltageConversionTime:	28
getTemperatureConversionTime:	28
getAverage:	28

test_others
getShuntTemperatureCoefficent:	28
getDiagnoseAlert:	28

test_thresholds
getShuntOvervoltageTH:	28
getShuntUndervoltageTH:	28
getBusOvervoltageTH:	28
getBusUndervoltageTH:	28
getTemperatureOverLimitTH:	28
getPowerOverLimitTH:	32

========================================================
Speed: 8000000

test_core
getBusVoltage:	36
getShuntVoltage:	36
getCurrent:	36
getPower:	40
getTemperature:	32
getEnergy:	60
getCharge:	56

test_config
getAccumulation:	24
getConversionDelay:	28
getTemperatureCompensation:	28
getADCRange:	28

test_adc_config
getMode:	28
getBusVoltageConversionTime:	24
getShuntVoltageConversionTime:	28
getTemperatureConversionTime:	28
getAverage:	24

test_others
getShuntTemperatureCoefficent:	28
getDiagnoseAlert:	28

test_thresholds
getShuntOvervoltageTH:	24
getShuntUndervoltageTH:	28
getBusOvervoltageTH:	24
getBusUndervoltageTH:	24
getTemperatureOverLimitTH:	24
getPowerOverLimitTH:	24

Done