
**AutoAnalogAudio for Arduino by TMRh20 2016**

Automated analog reads and analog output (streaming) using Arduino DAC(or PWM), ADC and Timers

**New** Now also supports AVR devices (Uno,Nano,Mega,etc) with pseudo DAC using PWM

Plays and records analog (wav/pcm audio) data using onboard DAC and ADC.
Timers are adjusted automatically based on the rate of data delivery, to ensure smooth playback.
DMA transfers used to maximize efficiency.

Documentation: http://TMRh20.github.io/AutoAnalogAudio/
Also see: http://nRF24.github.io/RF24Audio/

    AutoAnalogAudio streaming via DAC & ADC by TMRh20
    Copyright (C) 2016  TMRh20 - tmrh20@gmail.com, github.com/TMRh20

    This program is free software: you can redistribute it and/or modify
    it under the terms of the GNU General Public License as published by
    the Free Software Foundation, either version 3 of the License, or
    (at your option) any later version.

    This program is distributed in the hope that it will be useful,
    but WITHOUT ANY WARRANTY; without even the implied warranty of
    MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
    GNU General Public License for more details.

    You should have received a copy of the GNU General Public License
    along with this program.  If not, see <http://www.gnu.org/licenses/>.
