DevLab_ICM20948 1.0.0 Driver para sensor ICM-20948

Loading...
Searching...
No Matches
ICM20948_IntPinConfig Struct Reference

`#include <DevLab_ICM20948.h>`

## Public Attributes
uint8_t | activeLevel: 1
uint8_t | driveMode: 1
uint8_t | latchMode: 1
uint8_t | clearMode: 1
uint8_t | fsyncActLevel: 1
uint8_t | fsyncIntEn: 1
uint8_t | bypassEn: 1

## Detailed Description

ICM20948_IntPinConfig

- Physical configuration of the INT pin (INT_PIN_CFG register, BANK 0)
- Controls electrical behavior and clear condition of the interrupt line
- Pass to intInit() to apply settings

Definition at line 103 of file DevLab_ICM20948.h.

## Member Data Documentation

## ◆ activeLevel

uint8_t ICM20948_IntPinConfig::activeLevel

Definition at line 105 of file DevLab_ICM20948.h.

## ◆ bypassEn

uint8_t ICM20948_IntPinConfig::bypassEn

Definition at line 111 of file DevLab_ICM20948.h.

## ◆ clearMode

uint8_t ICM20948_IntPinConfig::clearMode

Definition at line 108 of file DevLab_ICM20948.h.

## ◆ driveMode

uint8_t ICM20948_IntPinConfig::driveMode

Definition at line 106 of file DevLab_ICM20948.h.

## ◆ fsyncActLevel

uint8_t ICM20948_IntPinConfig::fsyncActLevel

Definition at line 109 of file DevLab_ICM20948.h.

## ◆ fsyncIntEn

uint8_t ICM20948_IntPinConfig::fsyncIntEn

Definition at line 110 of file DevLab_ICM20948.h.

## ◆ latchMode

uint8_t ICM20948_IntPinConfig::latchMode

Definition at line 107 of file DevLab_ICM20948.h.

The documentation for this struct was generated from the following file:

- src/DevLab_ICM20948.h