DevLab_ICM20948 1.0.0 Driver para sensor ICM-20948

Loading...
Searching...
No Matches
DevLab_ICM20948 Class Reference

`#include <DevLab_ICM20948.h>`

## Public Member Functions
| DevLab_ICM20948 ()
bool | beginI2C (uint8_t address=0x69, TwoWire &i2cPort=Wire, uint32_t i2cSpeed=400000)
bool | beginSPI (uint8_t csPin, SPIClass &spiPort=SPI, uint32_t spiSpeed=1000000)
bool | readWhoAmI (uint8_t &whoAmI)
bool | selectBank (uint8_t bank)
bool | softReset ()
bool | sleep (bool en)
bool | applyBasicDefaults ()
bool | readAccel (float &x, float &y, float &z)
bool | readGyro (float &x, float &y, float &z)
bool | readTemperature (float &temperature)
bool | readMag (float &x, float &y, float &z)
bool | initMag ()
bool | setMagOpMode (ICM20948_Op_Mode opMode)
bool | setLowPower (bool enable)
bool | getLowPower (bool &enable)
bool | setClock (ICM20948_Clock_Source clock)
bool | getClock (uint8_t &clock)
bool | setGyroSampleRate (float sampleRate)
bool | getGyroSampleRate (float &sampleRate)
bool | setGyroDivRate (uint8_t divisor)
bool | setDLPF (ICM20948_Gyro_DLPF dlpf, bool bypass)
bool | getDLPF (uint8_t &dlpf, bool &bypass)
bool | setGyroScale (ICM20948_Gyro_FullScale fullScale)
bool | setGyroAveraging (ICM20948_Gyro_Average avg)
bool | getGyroScale (uint8_t &fullScale)
bool | selfTestGyro (bool x, bool y, bool z)
bool | setAccelDivRate (uint16_t divisor)
bool | setAccelSampleRate (uint16_t sampleRate)
bool | getAccelSampleRate (float &sampleRate)
bool | selfTestAccel (bool x, bool y, bool z)
bool | setAccelScale (ICM20948_Accel_FullScale fullScale)
bool | getAccelScale (uint8_t &fullScale)
bool | setAccelDLPF (uint8_t dlpf, bool bypass)
bool | getAccelDLPF (uint8_t &dlpf, bool &bypass)
bool | setAccelAveraging (ICM20948_Accel_Average avg)
bool | getAccelAveraging (uint8_t &avg)
bool | setSensors (bool accel_on, bool gyro_on, bool temp_on)
bool | getSensors (bool &accel_on, bool &gyro_on, bool &temp_on)
bool | setGyroOffset (uint16_t offsetX, uint16_t offsetY, uint16_t offsetZ)
bool | getGyroOffset (int16_t &offsetX, int16_t &offsetY, int16_t &offsetZ)
bool | setAccelOffset (int16_t offsetX, int16_t offsetY, int16_t offsetZ)
bool | getAccelOffset (int16_t &offsetX, int16_t &offsetY, int16_t &offsetZ)
bool | intInit (const ICM20948_IntPinConfig &cfg)
bool | intEnableConfig (const ICM20948_IntEnableConfig &cfg)
bool | checkIntStatus (ICM20948_IntStatus &status)
bool | auxMasterEnable (uint8_t clkFreq)
bool | auxWriteByte (uint8_t slaveAddr, uint8_t reg, uint8_t data)
bool | auxReadByte (uint8_t slaveAddr, uint8_t reg, uint8_t &data)
bool | auxWriteCommand (uint8_t slaveAddr, uint8_t cmd)
bool | auxConfigSlave (uint8_t slaveAddr, uint8_t reg, uint8_t numBytes)
bool | auxReadSensorData (uint8_t *buf, uint8_t len)
bool | auxReadResponse (uint8_t slaveAddr, uint8_t &data)
bool | auxRead12bit (uint16_t &raw)

## Detailed Description

Class

- Manages ICM-20948 over I2C (SPI path disabled in this cut)
- Caches scale factors for LSB->physical conversions

Definition at line 172 of file DevLab_ICM20948.h.

## Constructor & Destructor Documentation

## ◆ DevLab_ICM20948()

DevLab_ICM20948::DevLab_ICM20948 | ( |  | ) |

- Construct with default I2C address; call begin() to attach bus

Definition at line 4 of file DevLab_ICM20948.cpp.

## Member Function Documentation

## ◆ applyBasicDefaults()

bool DevLab_ICM20948::applyBasicDefaults | ( |  | ) |

applyBasicDefaults

- Apply basic sensor configuration
- Configure power, filters, ranges, and sampling rates

Returns:

- true → Configuration successful
- false → Any register write failed

Definition at line 181 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:
Here is the caller graph for this function:

## ◆ auxConfigSlave()

bool DevLab_ICM20948::auxConfigSlave | ( | uint8_t | slaveAddr,
|  | uint8_t | reg,
|  | uint8_t | numBytes )

auxConfigSlave

- Configure SLV0 for automatic periodic reads from an auxiliary I2C slave
- The ICM20948 master will read numBytes starting at reg on every ODR cycle
- Data is deposited into EXT_SLV_SENS_DATA_00 and subsequent registers
- Call once during initialization; read results with auxReadSensorData

Parameters:

- slaveAddr: 7-bit I2C address of the auxiliary slave
- reg: starting register address to read from on the slave
- numBytes: number of bytes to read per cycle (1–15)

Returns:

- true → SLV0 configured successfully
- false → Operation failed

Definition at line 1374 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ auxMasterEnable()

bool DevLab_ICM20948::auxMasterEnable | ( | uint8_t | clkFreq | ) |

auxMasterEnable

- Enable the ICM20948 internal I2C master for auxiliary bus
- Clears BYPASS_EN so the aux bus is controlled by the ICM
- Sets I2C_MST_EN in USER_CTRL
- Configures auxiliary master clock frequency

Parameters:

- clkFreq: clock divider value (e.g. 0x07 ≈ 345.6 kHz, 0x0D ≈ 400 kHz)

Returns:

- true → Master enabled successfully
- false → Operation failed

Definition at line 1260 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ auxRead12bit()

bool DevLab_ICM20948::auxRead12bit | ( | uint16_t & | raw | ) |

auxRead12bit

- Read a 12-bit value previously configured via auxConfigSlave (SLV0, numBytes = 2)
- Assumes little-endian packing: first byte = LSB, second byte = MSB
- Result is masked to 12 bits (0-4095)

Returns:

- true → Read successful
- false → Read failed

Definition at line 1424 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ auxReadByte()

bool DevLab_ICM20948::auxReadByte | ( | uint8_t | slaveAddr,
|  | uint8_t | reg,
|  | uint8_t & | data )

auxReadByte

- Read a single byte from a register of an auxiliary I2C slave via SLV4
- Generates a combined write-then-read transaction (reg byte + repeated START)
- Suitable for slaves that follow standard I2C register-read protocol

Note: slaves that need separate write/read transactions (e.g. command-response firmware) should use auxWriteCommand + auxReadResponse instead.

Parameters:

- slaveAddr: 7-bit I2C address of the auxiliary slave
- reg: register address to read from
- data: output byte received from slave

Returns:

- true → Read successful
- false → Timeout or NACK

Definition at line 1312 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ auxReadResponse()

bool DevLab_ICM20948::auxReadResponse | ( | uint8_t | slaveAddr,
|  | uint8_t & | data )

auxReadResponse

- Read a single response byte from an auxiliary I2C slave via SLV4
- Generates a pure read transaction: [START, addr+R, 1 byte, STOP]
- No register byte is sent (REG_DIS); slave must already be ready to transmit
- Use after auxWriteCommand to complete a command-response exchange with slaves that require separate write and read transactions (e.g. PY32F0 firmware slaves)

Parameters:

- slaveAddr: 7-bit I2C address of the auxiliary slave
- data: output byte received from slave

Returns:

- true → Response received successfully
- false → Timeout or NACK

Definition at line 1397 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ auxReadSensorData()

bool DevLab_ICM20948::auxReadSensorData | ( | uint8_t * | buf,
|  | uint8_t | len )

auxReadSensorData

- Read bytes from EXT_SLV_SENS_DATA registers (BANK 0)
- Returns data collected by the ICM20948 master from SLV0–SLV3 on the last cycle
- Must call auxConfigSlave first to set up the automatic read

Parameters:

- buf: output buffer to store the received bytes
- len: number of bytes to read (must match numBytes configured in auxConfigSlave)

Returns:

- true → Read successful
- false → Bus error

Definition at line 1391 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:
Here is the caller graph for this function:

## ◆ auxWriteByte()

bool DevLab_ICM20948::auxWriteByte | ( | uint8_t | slaveAddr,
|  | uint8_t | reg,
|  | uint8_t | data )

auxWriteByte

- Write a single byte to a register of an auxiliary I2C slave via SLV4
- Uses one-shot SLV4 transaction: polls SLV4_DONE, checks for NACK
- Suitable for configuration writes (not continuous streaming)

Parameters:

- slaveAddr: 7-bit I2C address of the auxiliary slave
- reg: target register address on the slave
- data: byte to write

Returns:

- true → Write acknowledged by slave
- false → Timeout or NACK

Definition at line 1281 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ auxWriteCommand()

bool DevLab_ICM20948::auxWriteCommand | ( | uint8_t | slaveAddr,
|  | uint8_t | cmd )

auxWriteCommand

- Send a single command byte to an auxiliary I2C slave via SLV4
- Uses REG_DIS: generates [START, addr+W, cmd_byte, STOP] with no register prefix
- Designed for slaves that use a command-response protocol (no register addressing)

Parameters:

- slaveAddr: 7-bit I2C address of the auxiliary slave
- cmd: command byte to send

Returns:

- true → Command acknowledged by slave
- false → Timeout or NACK

Definition at line 1346 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ beginI2C()

bool DevLab_ICM20948::beginI2C | ( | uint8_t | address = 0x69,
|  | TwoWire & | i2cPort = Wire,
|  | uint32_t | i2cSpeed = 400000 )

beginI2C

- Initialize ICM20948 using I2C interface
- Sets up communication layer (Interface + BusIO)
- Verifies device identity (WHO_AM_I)
- Configures basic power and clock settings

Returns:

- true → Device initialized successfully
- false → Communication or configuration failed

Definition at line 6 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ beginSPI()

bool DevLab_ICM20948::beginSPI | ( | uint8_t | csPin,
|  | SPIClass & | spiPort = SPI,
|  | uint32_t | spiSpeed = 1000000 )

Definition at line 60 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ checkIntStatus()

bool DevLab_ICM20948::checkIntStatus | ( | ICM20948_IntStatus & | status | ) |

checkIntStatus

- Read and parse all four interrupt status registers in a single burst read
- Covers INT_STATUS (0x19), INT_STATUS_1 (0x1A), INT_STATUS_2 (0x1B), INT_STATUS_3 (0x1C) from BANK 0
- Reading clears the interrupt flags when clearMode = 0 in ICM20948_IntPinConfig
- Typically called inside the INT pin ISR or polled in the main loop

Parameters:

- status: ICM20948_IntStatus struct populated with the current interrupt flags

Returns:

- true → Status read successfully
- false → Operation failed

Definition at line 1231 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ getAccelAveraging()

bool DevLab_ICM20948::getAccelAveraging | ( | uint8_t & | avg | ) |

getAccelAveraging

- Read accelerometer averaging / decimation setting (DEC3)

Flow:

- Validate bus pointer
- Select USER BANK 2
- Read DEC3 bits [1:0]

Returns:

- true → Read successful
- false → Operation failed

Definition at line 988 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ getAccelDLPF()

bool DevLab_ICM20948::getAccelDLPF | ( | uint8_t & | dlpf,
|  | bool & | bypass )

getAccelDLPF

- Read accelerometer DLPF configuration
- Returns filter setting and bypass state

Flow:

- Validate bus pointer
- Select USER BANK 2
- Read ACCEL_CONFIG register
- Extract bypass and DLPF bits

Returns:

- true → Read successful
- false → Operation failed

Definition at line 926 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ getAccelOffset()

bool DevLab_ICM20948::getAccelOffset | ( | int16_t & | offsetX,
|  | int16_t & | offsetY,
|  | int16_t & | offsetZ )

getAccelOffset

- Read accelerometer offset values for X, Y, Z axes
- Reads offset registers from USER BANK 1

Flow:

- Validate bus pointer
- Select USER BANK 1
- Read offset registers
- Convert to signed values

Returns:

- true → Read successful
- false → Operation failed

Definition at line 1151 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ getAccelSampleRate()

bool DevLab_ICM20948::getAccelSampleRate | ( | float & | sampleRate | ) |

getAccelSampleRate

- Get accelerometer output data rate (ODR)
- Computes value from divider registers

Returns:

- true → Read successful
- false → Operation failed

Definition at line 796 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ getAccelScale()

bool DevLab_ICM20948::getAccelScale | ( | uint8_t & | fullScale | ) |

getAccelScale

- Get current accelerometer full-scale range (FS_SEL)

Returns:

- true → Read successful
- false → Operation failed

Definition at line 878 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ getClock()

bool DevLab_ICM20948::getClock | ( | uint8_t & | clock | ) |

getClock

- Read current clock source (CLKSEL [2:0])

Returns:

- true → Read successful
- false → Operation failed

Definition at line 534 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ getDLPF()

bool DevLab_ICM20948::getDLPF | ( | uint8_t & | dlpf,
|  | bool & | bypass )

getDLPF

- Read gyroscope DLPF configuration
- Returns filter setting and bypass state

Returns:

- true → Read successful
- false → Operation failed

Definition at line 619 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ getGyroOffset()

bool DevLab_ICM20948::getGyroOffset | ( | int16_t & | offsetX,
|  | int16_t & | offsetY,
|  | int16_t & | offsetZ )

getGyroOffset

- Read gyroscope offset values for X, Y, Z axes
- Reads offset registers from USER BANK 2

Flow:

- Validate bus pointer
- Select USER BANK 2
- Read offset registers
- Convert to signed values

Returns:

- true → Read successful
- false → Operation failed

Definition at line 1099 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ getGyroSampleRate()

bool DevLab_ICM20948::getGyroSampleRate | ( | float & | sampleRate | ) |

getGyroSampleRate

- Get current gyroscope sample rate
- Computes value from divider register

Returns:

- true → Read successful
- false → Operation failed

Definition at line 571 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ getGyroScale()

bool DevLab_ICM20948::getGyroScale | ( | uint8_t & | fullScale | ) |

getGyroScale

- Get current gyroscope full-scale range (FS_SEL

Returns:

- true → Read successful
- false → Operation failed

Definition at line 665 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ getLowPower()

bool DevLab_ICM20948::getLowPower | ( | bool & | enable | ) |

getLowPower

- Read low power mode status
- Returns state of LP_EN bit

Returns:

- true → Read successful
- false → Operation failed

Definition at line 502 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ getSensors()

bool DevLab_ICM20948::getSensors | ( | bool & | accel_on,
|  | bool & | gyro_on,
|  | bool & | temp_on )

getSensors

- Read accel, gyro, and temperature enable state

Flow:

- Validate bus pointer
- Select USER BANK 0
- Read PWR_MGMT_2 register
- Read TEMP_DIS bit
- Decode enable states

Returns:

- true → Read successful
- false → Operation failed

Definition at line 1039 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ initMag()

bool DevLab_ICM20948::initMag | ( |  | ) |

initMag

- Initialize AK09916 magnetometer using internal I2C master
- Verifies WHO_AM_I and enables continuous mode
- Configures SLV0 for automatic data read

Returns:

- true → Initialization successful
- false → Operation failed

Definition at line 334 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ intEnableConfig()

bool DevLab_ICM20948::intEnableConfig | ( | const ICM20948_IntEnableConfig & | cfg | ) |

intEnableConfig

- Enable or disable individual interrupt sources routed to the INT pin
- Writes INT_ENABLE (0x10), INT_ENABLE_1 (0x11), INT_ENABLE_2 (0x12), and INT_ENABLE_3 (0x13) in BANK 0
- Must call intInit() first to configure the pin electrical behavior

Parameters:

- cfg: ICM20948_IntEnableConfig struct with the desired interrupt sources enabled

Returns:

- true → All four registers written successfully
- false → Operation failed

Definition at line 1200 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ intInit()

bool DevLab_ICM20948::intInit | ( | const ICM20948_IntPinConfig & | cfg | ) |

intInit

- Configure the physical behavior of the INT pin (INT_PIN_CFG register, BANK 0)
- Sets active level, drive mode (push-pull / open-drain), latch vs pulse mode, clear condition, FSYNC level, FSYNC interrupt enable, and I2C bypass

Parameters:

- cfg: ICM20948_IntPinConfig struct with the desired pin settings

Returns:

- true → Configuration written successfully
- false → Operation failed

Definition at line 1176 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ readAccel()

bool DevLab_ICM20948::readAccel | ( | float & | x,
|  | float & | y,
|  | float & | z )

readAccel

- Read accelerometer data (X, Y, Z)
- Convert raw values to g using LSB scale

Returns:

- true → Read successful
- false → Read failed

Definition at line 238 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ readGyro()

bool DevLab_ICM20948::readGyro | ( | float & | x,
|  | float & | y,
|  | float & | z )

readGyro

- Read gyroscope data (X, Y, Z)
- Convert raw values to dps using LSB scale

Returns:

- true → Read successful
- false → Read failed

Definition at line 258 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ readMag()

bool DevLab_ICM20948::readMag | ( | float & | x,
|  | float & | y,
|  | float & | z )

readMag

- Read magnetometer data via internal I2C master
- Data comes from EXT_SLV_SENS_DATA registers
- Convert raw values to µT

Returns:

- true → Read successful
- false → Read failed

Definition at line 310 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ readTemperature()

bool DevLab_ICM20948::readTemperature | ( | float & | temperature | ) |

readTemperature

- Read temperature sensor
- Convert raw values to °C

Returns:

- true → Read successful
- false → Read failed

Definition at line 278 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ readWhoAmI()

bool DevLab_ICM20948::readWhoAmI | ( | uint8_t & | whoAmI | ) |

readWhoAmI

- Read WHO_AM_I register (device ID)
- Used during initialization to verify ICM20948
- Expected value: 0xEA

Returns:

- true → Read successful
- false → Operation failed

Definition at line 118 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:
Here is the caller graph for this function:

## ◆ selectBank()

bool DevLab_ICM20948::selectBank | ( | uint8_t | bank | ) |

selectBank

- Select USER BANK (0–3)
- Used to access different register groups inside ICM20948

Returns:

- true → Bank switch successful
- false → Write failed

Definition at line 132 of file DevLab_ICM20948.cpp.

## ◆ selfTestAccel()

bool DevLab_ICM20948::selfTestAccel | ( | bool | x,
|  | bool | y,
|  | bool | z )

selfTestAccel

- Enable or disable accelerometer self-test per axis

Returns:

- true → Operation successful
- false → Operation failed

Definition at line 826 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ selfTestGyro()

bool DevLab_ICM20948::selfTestGyro | ( | bool | x,
|  | bool | y,
|  | bool | z )

selfTestGyro

- Enable or disable gyroscope self-test per axis

Returns:

- true → Operation successful
- false → Operation failed

Definition at line 683 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ setAccelAveraging()

bool DevLab_ICM20948::setAccelAveraging | ( | ICM20948_Accel_Average | avg | ) |

setAccelAveraging

- Configure accelerometer averaging / decimation (DEC3)
- Controls internal averaging of accel samples

Flow:

- Validate bus pointer
- Select USER BANK 2
- Write DEC3 bits [1:0]

Returns:

- true → Operation successful
- false → Operation failed

Definition at line 952 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ setAccelDivRate()

bool DevLab_ICM20948::setAccelDivRate | ( | uint16_t | divisor | ) |

Definition at line 748 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ setAccelDLPF()

bool DevLab_ICM20948::setAccelDLPF | ( | uint8_t | dlpf,
|  | bool | bypass )

setAccelDLPF

- Configure accelerometer digital low-pass filter (DLPF)
- Option to bypass filter (full bandwidth)

Flow:

- Validate bus pointer
- Select USER BANK 2
- Set or clear bypass bit
- Configure DLPF bits if not bypassed

Returns:

- true → Operation successful
- false → Operation failed

Definition at line 897 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ setAccelOffset()

bool DevLab_ICM20948::setAccelOffset | ( | int16_t | offsetX,
|  | int16_t | offsetY,
|  | int16_t | offsetZ )

setAccelOffset

- Set accelerometer offset values for X, Y, Z axes
- Writes offset registers in USER BANK 1

Flow:

- Validate bus pointer
- Select USER BANK 1
- Pack offsets into byte array
- Write to offset registers

Returns:

- true → Operation successful
- false → Operation failed

Definition at line 1124 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ setAccelSampleRate()

bool DevLab_ICM20948::setAccelSampleRate | ( | uint16_t | sampleRate | ) |

setAccelSampleRate

- Set accelerometer output data rate (ODR)
- Uses 1125 Hz base rate with 12-bit divider

Returns:

- true → Operation successful
- false → Operation failed

Definition at line 709 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ setAccelScale()

bool DevLab_ICM20948::setAccelScale | ( | ICM20948_Accel_FullScale | fullScale | ) |

setAccelScale

- Set accelerometer full-scale range (FS_SEL)
- Controls measurement range (±2g, ±4g, ±8g, ±16g)

Returns:

- true → Operation successful
- false → Operation failed

Definition at line 857 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ setClock()

bool DevLab_ICM20948::setClock | ( | ICM20948_Clock_Source | clock | ) |

setClock

- Set clock source (CLKSEL [2:0])
- Selects internal clock for sensor operation

Returns:

- true → Operation successful
- false → Operation failed

Definition at line 520 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ setDLPF()

bool DevLab_ICM20948::setDLPF | ( | ICM20948_Gyro_DLPF | dlpf,
|  | bool | bypass )

setDLPF

- Configure gyroscope digital low-pass filter (DLPF)
- Option to bypass filter (full bandwidth)

Returns:

- true → Operation successful
- false → Operation failed

Definition at line 593 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ setGyroAveraging()

bool DevLab_ICM20948::setGyroAveraging | ( | ICM20948_Gyro_Average | avg | ) |

Definition at line 970 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ setGyroDivRate()

bool DevLab_ICM20948::setGyroDivRate | ( | uint8_t | divisor | ) |

Definition at line 780 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ setGyroOffset()

bool DevLab_ICM20948::setGyroOffset | ( | uint16_t | offsetX,
|  | uint16_t | offsetY,
|  | uint16_t | offsetZ )

setGyroOffset

- Set gyroscope offset values for X, Y, Z axes
- Writes offset registers in USER BANK 2

Flow:

- Validate bus pointer
- Select USER BANK 2
- Pack offsets into byte array
- Write to offset registers

Returns:

- true → Operation successful
- false → Operation failed

Definition at line 1072 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ setGyroSampleRate()

bool DevLab_ICM20948::setGyroSampleRate | ( | float | sampleRate | ) |

setGyroSampleRate

- Set gyroscope sample rate
- Uses internal divider (SRD) based on 1100 Hz base rate

Returns:

- true → Operation successful
- false → Invalid input or write failed

Definition at line 550 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ setGyroScale()

bool DevLab_ICM20948::setGyroScale | ( | ICM20948_Gyro_FullScale | fullScale | ) |

setGyroScale

- Set gyroscope full-scale range (FS_SEL)
- Controls sensitivity (dps range)

Flow:

- Validate bus pointer
- Select USER BANK 2
- Write FS_SEL bits [2:1]

Returns:

- true → Operation successful
- false → Operation failed

Definition at line 644 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ setLowPower()

bool DevLab_ICM20948::setLowPower | ( | bool | enable | ) |

setLowPower

- Enable or disable low power mode
- Controls LP_EN bit in PWR_MGMT_1

Returns:

- true → Operation successful
- false → Operation failed

Definition at line 488 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ setMagOpMode()

bool DevLab_ICM20948::setMagOpMode | ( | ICM20948_Op_Mode | opMode | ) |

setMagOpMode

- Set magnetometer operation mode

Returns:

- true → Mode set successfully
- false → Write failed

Definition at line 410 of file DevLab_ICM20948.cpp.

## ◆ setSensors()

bool DevLab_ICM20948::setSensors | ( | bool | accel_on,
|  | bool | gyro_on,
|  | bool | temp_on )

setSensors

- Enable or disable accel, gyro, and temperature sensor
- Controls power gating via PWR_MGMT_2 and TEMP_DIS

Flow:

- Validate bus pointer
- Select USER BANK 0
- Build PWR_MGMT_2 mask
- Configure temperature enable/disable

Returns:

- true → Operation successful
- false → Operation failed

Definition at line 1006 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:

## ◆ sleep()

bool DevLab_ICM20948::sleep | ( | bool | en | ) |

sleep

- Enable or disable sleep mode
- Maintains clock source (CLKSEL = 1)

Flow:

- Select USER BANK 0
- Set or clear SLEEP bit

Returns:

- true → Operation successful
- false → Operation failed

Definition at line 164 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:
Here is the caller graph for this function:

## ◆ softReset()

bool DevLab_ICM20948::softReset | ( |  | ) |

softReset

- Perform software reset of ICM20948
- Resets all internal registers to default state

Flow:

- Select USER BANK 0
- Set DEVICE_RESET bit
- Wait for device to restart

Returns:

- true → Reset successful
- false → Operation failed

Definition at line 144 of file DevLab_ICM20948.cpp.

Here is the call graph for this function:
Here is the caller graph for this function:

The documentation for this class was generated from the following files:

- src/DevLab_ICM20948.h
- src/DevLab_ICM20948.cpp