DevLab_ICM20948 1.0.0 ICM-20948 9-Axis Motion Sensor Driver

Loading...
Searching...
No Matches
SPI_Interface Member List

This is the complete list of members for SPI_Interface, including all inherited members.

beginI2C(uint8_t, TwoWire &, uint32_t, uint8_t, uint8_t) override | SPI_Interface | inline virtual
beginSPI(uint8_t csPin, SPIClass &spiPort, uint32_t spiSpeed, uint8_t sck=255, uint8_t miso=255, uint8_t mosi=255) override | SPI_Interface | inline virtual
cs | SPI_Interface |
delay_us(uint32_t us) | Interface_7Semi | inline protected static
read(uint8_t reg, uint8_t *data, uint32_t len) override | SPI_Interface | inline virtual
speed | SPI_Interface |
spi | SPI_Interface |
write(uint8_t reg, const uint8_t *data, uint32_t len) override | SPI_Interface | inline virtual
~Interface_7Semi() | Interface_7Semi | inline virtual