<map id="DevLab_ICM20948::setAccelAveraging" name="DevLab_ICM20948::setAccelAveraging">
<area shape="rect" id="Node000001" title=" " alt="" coords="164,23,371,63"/>
<area shape="rect" id="Node000002" href="$test2_8ino.html#a73c1d2766fc4db839bb9adf5cab93c80" title="Apply one accelerometer full&#45;scale, DLPF, and averaging configuration." alt="" coords="5,5,116,31"/>
<area shape="poly" id="edge1_Node000001_Node000002" title=" " alt="" coords="150,32,116,27,117,22,150,26"/>
<area shape="rect" id="Node000003" href="$i2c__accel_8ino.html#a4fc01d736fe50cf5b977f755b675f11d" title="Configure the IMU for accelerometer&#45;only operation over I2C." alt="" coords="31,55,90,80"/>
<area shape="poly" id="edge2_Node000001_Node000003" title=" " alt="" coords="150,60,90,67,90,61,150,54"/>
</map>
