APDS9999 LED Config Test
------------------------
APDS9999 found!
Testing LED pulses (1, 64, 128, 255)...

Pulses 1: PASS
Pulses 64: PASS
Pulses 128: PASS
Pulses 255: PASS

Testing LED current...

Current 10mA: PASS
Current 25mA: PASS

Testing LED frequency...

Frequency 60kHz: PASS
Frequency 70kHz: PASS
Frequency 80kHz: PASS
Frequency 90kHz: PASS
Frequency 100kHz: PASS

=== FUNCTIONAL TEST: LED Current Affects Readings ===

Moving paper in front of sensor...
Prox with 10mA current: 75
Prox with 25mA current: 213
Current affects readings: PASS (25mA 213 > 10mA 75)

=== FUNCTIONAL TEST: LED Pulses Affect Readings ===

Moving paper in front of sensor...
Prox with 4 pulses: 4
Prox with 64 pulses: 75
Pulses affect readings: PASS (64 pulses 75 > 4 pulses 4)

Passed: 13 / Failed: 0
*** TEST PASSED ***
