| SX126x-Arduino 1.3.0

Macros | Functions | Variables
RegionUS915-Hybrid.h File Reference

Region definition for US915. More...

Go to the source code of this file.

## Macros
#define | US915_HYBRID_MAX_NB_CHANNELS 72
#define | US915_HYBRID_TX_MIN_DATARATE DR_0
#define | US915_HYBRID_TX_MAX_DATARATE DR_4
#define | US915_HYBRID_RX_MIN_DATARATE DR_8
#define | US915_HYBRID_RX_MAX_DATARATE DR_13
#define | US915_HYBRID_DEFAULT_DATARATE DR_0
#define | US915_HYBRID_MIN_RX1_DR_OFFSET 0
#define | US915_HYBRID_MAX_RX1_DR_OFFSET 3
#define | US915_HYBRID_DEFAULT_RX1_DR_OFFSET 0
#define | US915_HYBRID_MIN_TX_POWER TX_POWER_10
#define | US915_HYBRID_MAX_TX_POWER TX_POWER_0
#define | US915_HYBRID_DEFAULT_TX_POWER TX_POWER_0
#define | US915_HYBRID_DEFAULT_MAX_ERP 30.0f
#define | US915_HYBRID_ADR_ACK_LIMIT 64
#define | US915_HYBRID_ADR_ACK_DELAY 32
#define | US915_HYBRID_DUTY_CYCLE_ENABLED 0
#define | US915_HYBRID_MAX_RX_WINDOW 3000
#define | US915_HYBRID_RECEIVE_DELAY1 1000
#define | US915_HYBRID_RECEIVE_DELAY2 2000
#define | US915_HYBRID_JOIN_ACCEPT_DELAY1 5000
#define | US915_HYBRID_JOIN_ACCEPT_DELAY2 6000
#define | US915_HYBRID_MAX_FCNT_GAP 16384
#define | US915_HYBRID_ACKTIMEOUT 2000
#define | US915_HYBRID_ACK_TIMEOUT_RND 1000
#define | US915_HYBRID_RX_WND_2_FREQ 923300000
#define | US915_HYBRID_RX_WND_2_DR DR_8
#define | US915_HYBRID_MAX_NB_BANDS 1
#define | US915_HYBRID_BAND0
#define | US915_HYBRID_FIRST_RX1_CHANNEL ((uint32_t)923300000)
#define | US915_HYBRID_LAST_RX1_CHANNEL ((uint32_t)927500000)
#define | US915_HYBRID_STEPWIDTH_RX1_CHANNEL ((uint32_t)600000)

## Functions
PhyParam_t | RegionUS915HybridGetPhyParam (GetPhyParams_t *getPhy)
| The function gets a value of a specific phy attribute. More...
void | RegionUS915HybridSetBandTxDone (SetBandTxDoneParams_t *txDone)
| Updates the last TX done parameters of the current channel. More...
void | RegionUS915HybridInitDefaults (InitType_t type)
| Initializes the channels masks and the channels. More...
bool | RegionUS915HybridVerify (VerifyParams_t *verify, PhyAttribute_t phyAttribute)
| Verifies a parameter. More...
void | RegionUS915HybridApplyCFList (ApplyCFListParams_t *applyCFList)
| The function parses the input buffer and sets up the channels of the CF list. More...
bool | RegionUS915HybridChanMaskSet (ChanMaskSetParams_t *chanMaskSet)
| Sets a channels mask. More...
bool | RegionUS915HybridAdrNext (AdrNextParams_t *adrNext, int8_t *drOut, int8_t *txPowOut, uint32_t *adrAckCounter)
| Calculates the next datarate to set, when ADR is on or off. More...
void | RegionUS915HybridComputeRxWindowParameters (int8_t datarate, uint8_t minRxSymbols, uint32_t rxError, RxConfigParams_t *rxConfigParams)
bool | RegionUS915HybridRxConfig (RxConfigParams_t *rxConfig, int8_t *datarate)
| Configuration of the RX windows. More...
bool | RegionUS915HybridTxConfig (TxConfigParams_t *txConfig, int8_t *txPower, TimerTime_t *txTimeOnAir)
| TX configuration. More...
uint8_t | RegionUS915HybridLinkAdrReq (LinkAdrReqParams_t *linkAdrReq, int8_t *drOut, int8_t *txPowOut, uint8_t *nbRepOut, uint8_t *nbBytesParsed)
| The function processes a Link ADR Request. More...
uint8_t | RegionUS915HybridRxParamSetupReq (RxParamSetupReqParams_t *rxParamSetupReq)
| The function processes a RX Parameter Setup Request. More...
uint8_t | RegionUS915HybridNewChannelReq (NewChannelReqParams_t *newChannelReq)
| The function processes a Channel Request. More...
int8_t | RegionUS915HybridTxParamSetupReq (TxParamSetupReqParams_t *txParamSetupReq)
| The function processes a TX ParamSetup Request. More...
uint8_t | RegionUS915HybridDlChannelReq (DlChannelReqParams_t *dlChannelReq)
| The function processes a DlChannel Request. More...
int8_t | RegionUS915HybridAlternateDr (AlternateDrParams_t *alternateDr)
| Alternates the datarate of the channel for the join request. More...
void | RegionUS915HybridCalcBackOff (CalcBackOffParams_t *calcBackOff)
| Calculates the back-off time. More...
bool | RegionUS915HybridNextChannel (NextChanParams_t *nextChanParams, uint8_t *channel, TimerTime_t *time, TimerTime_t *aggregatedTimeOff)
| Searches and set the next random available channel. More...
LoRaMacStatus_t | RegionUS915HybridChannelAdd (ChannelAddParams_t *channelAdd)
| Adds a channel. More...
bool | RegionUS915HybridChannelsRemove (ChannelRemoveParams_t *channelRemove)
| Removes a channel. More...
void | RegionUS915HybridSetContinuousWave (ContinuousWaveParams_t *continuousWave)
| Sets the radio into continuous wave mode. More...
uint8_t | RegionUS915HybridApplyDrOffset (uint8_t downlinkDwellTime, int8_t dr, int8_t drOffset)
| Computes new datarate according to the given offset. More...

## Variables
static const uint8_t | DataratesUS915_HYBRID [] = {10, 9, 8, 7, 8, 0, 0, 0, 12, 11, 10, 9, 8, 7, 0, 0}
static const uint32_t | BandwidthsUS915_HYBRID [] = {125000, 125000, 125000, 125000, 500000, 0, 0, 0, 500000, 500000, 500000, 500000, 500000, 500000, 0, 0}
static const int8_t | DatarateOffsetsUS915_HYBRID [5][4]
static const uint8_t | MaxPayloadOfDatarateUS915_HYBRID [] = {11, 53, 125, 242, 242, 0, 0, 0, 53, 129, 242, 242, 242, 242, 0, 0}
static const uint8_t | MaxPayloadOfDatarateRepeaterUS915_HYBRID [] = {11, 53, 125, 242, 242, 0, 0, 0, 33, 109, 222, 222, 222, 222, 0, 0}

## Detailed Description

Region definition for US915.

Copyright
  Revised BSD License, see file LICENSE.

______ _
/ _____) _ | |
( (____ _____ ____ _| |_ _____ ____| |__
\____ \| ___ | (_ _) ___ |/ ___) _ \
_____) ) ____| | | || |_| ____( (___| | | |
(______/|_____)_|_|_| \__)_____)\____)_| |_|
(C)2013 Semtech
___ _____ _ ___ _ _____ ___ ___ ___ ___
/ __|_ _/_\ / __| |/ / __/ _ \| _ \/ __| __|
\__ \ | |/ _ \ (__| ' <| _| (_) | / (__| _|
|___/ |_/_/ \_\___|_|\_\_| \___/|_|_\\___|___|
embedded.connectivity.solutions===============

Author
  Miguel Luis ( Semtech )
  Gregory Cristian ( Semtech )
  Daniel Jaeckle ( STACKFORCE )