| SX126x-Arduino 2.0.1

RegionCN779.h
Go to the documentation of this file.
1
35 #ifndef __REGION_CN779_H__
36 #define __REGION_CN779_H__
37
38 extern "C"
39 {
40
44 #define CN779_MAX_NB_CHANNELS 16
45
49 #define CN779_NUMB_DEFAULT_CHANNELS 3
50
54 #define CN779_NUMB_CHANNELS_CF_LIST 5
55
59 #define CN779_TX_MIN_DATARATE DR_0
60
64 #define CN779_TX_MAX_DATARATE DR_7
65
69 #define CN779_RX_MIN_DATARATE DR_0
70
74 #define CN779_RX_MAX_DATARATE DR_7
75
79 #define CN779_DEFAULT_DATARATE DR_0
80
84 #define CN779_MIN_RX1_DR_OFFSET 0
85
89 #define CN779_MAX_RX1_DR_OFFSET 5
90
94 #define CN779_DEFAULT_RX1_DR_OFFSET 0
95
99 #define CN779_MIN_TX_POWER TX_POWER_5
100
104 #define CN779_MAX_TX_POWER TX_POWER_0
105
109 #define CN779_DEFAULT_TX_POWER TX_POWER_0
110
114 #define CN779_DEFAULT_MAX_EIRP 12.15f
115
119 #define CN779_DEFAULT_ANTENNA_GAIN 2.15f
120
124 #define CN779_ADR_ACK_LIMIT 64
125
129 #define CN779_ADR_ACK_DELAY 32
130
134 #define CN779_DUTY_CYCLE_ENABLED 1
135
139 #define CN779_MAX_RX_WINDOW 3000
140
144 #define CN779_RECEIVE_DELAY1 1000
145
149 #define CN779_RECEIVE_DELAY2 2000
150
154 #define CN779_JOIN_ACCEPT_DELAY1 5000
155
159 #define CN779_JOIN_ACCEPT_DELAY2 6000
160
164 #define CN779_MAX_FCNT_GAP 16384
165
169 #define CN779_ACKTIMEOUT 2000
170
174 #define CN779_ACK_TIMEOUT_RND 1000
175
179 #if (CN779_DEFAULT_DATARATE > DR_5)
180 #error "A default DR higher than DR_5 may lead to connectivity loss."
181 #endif
182
186 #define CN779_RX_WND_2_FREQ 786000000
187
191 #define CN779_RX_WND_2_DR DR_0
192
196 #define CN779_MAX_NB_BANDS 1
197
202 #define CN779_BAND0 \
203 { \
204 100, CN779_MAX_TX_POWER, 0, 0 \
205 } // 1.0 %
206
211 #define CN779_LC1 \
212 { \
213 779500000, 0, {((DR_5 << 4) | DR_0)}, 0 \
214 }
215
219 #define CN779_LC2 \
220 { \
221 779700000, 0, {((DR_5 << 4) | DR_0)}, 0 \
222 }
223
228 #define CN779_LC3 \
229 { \
230 779900000, 0, {((DR_5 << 4) | DR_0)}, 0 \
231 }
232
236 #define CN779_JOIN_CHANNELS (uint16_t)(LC(1) | LC(2) | LC(3))
237
241 static const uint8_t DataratesCN779[] = {12, 11, 10, 9, 8, 7, 7, 50};
242
246 static const uint32_t BandwidthsCN779[] = {125000, 125000, 125000, 125000, 125000, 125000, 250000, 0};
247
251 static const uint8_t MaxPayloadOfDatarateCN779[] = {51, 51, 51, 115, 242, 242, 242, 242};
252
256 static const uint8_t MaxPayloadOfDatarateRepeaterCN779[] = {51, 51, 51, 115, 222, 222, 222, 222};
257
265 PhyParam_t RegionCN779GetPhyParam(GetPhyParams_t *getPhy);
266
272 void RegionCN779SetBandTxDone(SetBandTxDoneParams_t *txDone);
273
279 void RegionCN779InitDefaults(InitType_t type);
280
290 bool RegionCN779Verify(VerifyParams_t *verify, PhyAttribute_t phyAttribute);
291
298 void RegionCN779ApplyCFList(ApplyCFListParams_t *applyCFList);
299
307 bool RegionCN779ChanMaskSet(ChanMaskSetParams_t *chanMaskSet);
308
322 bool RegionCN779AdrNext(AdrNextParams_t *adrNext, int8_t *drOut, int8_t *txPowOut, uint32_t *adrAckCounter);
323
337 void RegionCN779ComputeRxWindowParameters(int8_t datarate, uint8_t minRxSymbols, uint32_t rxError, RxConfigParams_t *rxConfigParams);
338
348 bool RegionCN779RxConfig(RxConfigParams_t *rxConfig, int8_t *datarate);
349
361 bool RegionCN779TxConfig(TxConfigParams_t *txConfig, int8_t *txPower, TimerTime_t *txTimeOnAir);
362
378 uint8_t RegionCN779LinkAdrReq(LinkAdrReqParams_t *linkAdrReq, int8_t *drOut, int8_t *txPowOut, uint8_t *nbRepOut, uint8_t *nbBytesParsed);
379
387 uint8_t RegionCN779RxParamSetupReq(RxParamSetupReqParams_t *rxParamSetupReq);
388
396 uint8_t RegionCN779NewChannelReq(NewChannelReqParams_t *newChannelReq);
397
407 int8_t RegionCN779TxParamSetupReq(TxParamSetupReqParams_t *txParamSetupReq);
408
416 uint8_t RegionCN779DlChannelReq(DlChannelReqParams_t *dlChannelReq);
417
425 int8_t RegionCN779AlternateDr(AlternateDrParams_t *alternateDr);
426
432 void RegionCN779CalcBackOff(CalcBackOffParams_t *calcBackOff);
433
448 bool RegionCN779NextChannel(NextChanParams_t *nextChanParams, uint8_t *channel, TimerTime_t *time, TimerTime_t *aggregatedTimeOff);
449
457 LoRaMacStatus_t RegionCN779ChannelAdd(ChannelAddParams_t *channelAdd);
458
466 bool RegionCN779ChannelsRemove(ChannelRemoveParams_t *channelRemove);
467
473 void RegionCN779SetContinuousWave(ContinuousWaveParams_t *continuousWave);
474
486 uint8_t RegionCN779ApplyDrOffset(uint8_t downlinkDwellTime, int8_t dr, int8_t drOffset);
487
489 };
490 #endif // __REGION_CN779_H__
sChannelRemoveParams
Definition: Region.h:1217
LoRaMacStatus_t
enum eLoRaMacStatus LoRaMacStatus_t
sTxConfigParams
Definition: Region.h:999
InitType_t
enum eInitType InitType_t
sSetBandTxDoneParams
Definition: Region.h:832
RegionCN779ApplyDrOffset
uint8_t RegionCN779ApplyDrOffset(uint8_t downlinkDwellTime, int8_t dr, int8_t drOffset)
Computes new datarate according to the given offset.
sRxParamSetupReqParams
Definition: Region.h:1065
RegionCN779RxConfig
bool RegionCN779RxConfig(RxConfigParams_t *rxConfig, int8_t *datarate)
Configuration of the RX windows.
RegionCN779SetContinuousWave
void RegionCN779SetContinuousWave(ContinuousWaveParams_t *continuousWave)
Sets the radio into continuous wave mode.
uVerifyParams
Definition: Region.h:850
sRxConfigParams
Definition: Region.h:948
sAlternateDrParams
Definition: Region.h:1133
sNewChannelReqParams
Definition: Region.h:1084
sContinuousWaveParams
Definition: Region.h:1228
sAdrNextParams
Definition: Region.h:917
RegionCN779RxParamSetupReq
uint8_t RegionCN779RxParamSetupReq(RxParamSetupReqParams_t *rxParamSetupReq)
The function processes a RX Parameter Setup Request.
MaxPayloadOfDatarateCN779
static const uint8_t MaxPayloadOfDatarateCN779[]
Definition: RegionCN779.h:251
sCalcBackOffParams
Definition: Region.h:1144
RegionCN779ChanMaskSet
bool RegionCN779ChanMaskSet(ChanMaskSetParams_t *chanMaskSet)
Sets a channels mask.
sApplyCFListParams
Definition: Region.h:887
sTxParamSetupReqParams
Definition: Region.h:1099
sChanMaskSetParams
Definition: Region.h:902
sLinkAdrReqParams
Definition: Region.h:1030
RegionCN779Verify
bool RegionCN779Verify(VerifyParams_t *verify, PhyAttribute_t phyAttribute)
Verifies a parameter.
BandwidthsCN779
static const uint32_t BandwidthsCN779[]
Definition: RegionCN779.h:246
RegionCN779AdrNext
bool RegionCN779AdrNext(AdrNextParams_t *adrNext, int8_t *drOut, int8_t *txPowOut, uint32_t *adrAckCounter)
Calculates the next datarate to set, when ADR is on or off.
MaxPayloadOfDatarateRepeaterCN779
static const uint8_t MaxPayloadOfDatarateRepeaterCN779[]
Definition: RegionCN779.h:256
DataratesCN779
static const uint8_t DataratesCN779[]
Definition: RegionCN779.h:241
RegionCN779ChannelAdd
LoRaMacStatus_t RegionCN779ChannelAdd(ChannelAddParams_t *channelAdd)
Adds a channel.
RegionCN779ChannelsRemove
bool RegionCN779ChannelsRemove(ChannelRemoveParams_t *channelRemove)
Removes a channel.
RegionCN779SetBandTxDone
void RegionCN779SetBandTxDone(SetBandTxDoneParams_t *txDone)
Updates the last TX done parameters of the current channel.
sNextChanParams
Definition: Region.h:1175
uPhyParam
Definition: Region.h:780
RegionCN779TxParamSetupReq
int8_t RegionCN779TxParamSetupReq(TxParamSetupReqParams_t *txParamSetupReq)
The function processes a TX ParamSetup Request.
RegionCN779TxConfig
bool RegionCN779TxConfig(TxConfigParams_t *txConfig, int8_t *txPower, TimerTime_t *txTimeOnAir)
TX configuration.
RegionCN779GetPhyParam
PhyParam_t RegionCN779GetPhyParam(GetPhyParams_t *getPhy)
The function gets a value of a specific phy attribute.
sChannelAddParams
Definition: Region.h:1202
RegionCN779LinkAdrReq
uint8_t RegionCN779LinkAdrReq(LinkAdrReqParams_t *linkAdrReq, int8_t *drOut, int8_t *txPowOut, uint8_t *nbRepOut, uint8_t *nbBytesParsed)
The function processes a Link ADR Request.
RegionCN779DlChannelReq
uint8_t RegionCN779DlChannelReq(DlChannelReqParams_t *dlChannelReq)
The function processes a DlChannel Request.
RegionCN779NextChannel
bool RegionCN779NextChannel(NextChanParams_t *nextChanParams, uint8_t *channel, TimerTime_t *time, TimerTime_t *aggregatedTimeOff)
Searches and set the next random available channel.
sDlChannelReqParams
Definition: Region.h:1118
sGetPhyParams
Definition: Region.h:803
RegionCN779ComputeRxWindowParameters
void RegionCN779ComputeRxWindowParameters(int8_t datarate, uint8_t minRxSymbols, uint32_t rxError, RxConfigParams_t *rxConfigParams)
RegionCN779AlternateDr
int8_t RegionCN779AlternateDr(AlternateDrParams_t *alternateDr)
Alternates the datarate of the channel for the join request.
RegionCN779InitDefaults
void RegionCN779InitDefaults(InitType_t type)
Initializes the channels masks and the channels.
PhyAttribute_t
enum ePhyAttribute PhyAttribute_t
TimerTime_t
uint32_t TimerTime_t
Timer time variable definition.
Definition: timer.h:69
RegionCN779NewChannelReq
uint8_t RegionCN779NewChannelReq(NewChannelReqParams_t *newChannelReq)
The function processes a Channel Request.
RegionCN779ApplyCFList
void RegionCN779ApplyCFList(ApplyCFListParams_t *applyCFList)
The function parses the input buffer and sets up the channels of the CF list.
RegionCN779CalcBackOff
void RegionCN779CalcBackOff(CalcBackOffParams_t *calcBackOff)
Calculates the back-off time.