| SX126x-Arduino 2.0.1

Data Fields
RadioStatus_u Union Reference

Structure describing the radio status. More...

`#include <sx126x.h>`

## Data Fields
uint8_t | Value
struct {
uint8_t Reserved: 1
| Reserved. More...
uint8_t CmdStatus: 3
| Command status. More...
uint8_t ChipMode: 3
| Chip mode. More...
uint8_t CpuBusy: 1
| Flag for CPU radio busy. More...
} | Fields

## Detailed Description

Structure describing the radio status.

## Field Documentation

## ◆ Value

uint8_t RadioStatus_u::Value

## ◆ Reserved

uint8_t RadioStatus_u::Reserved

Reserved.

## ◆ CmdStatus

uint8_t RadioStatus_u::CmdStatus

Command status.

## ◆ ChipMode

uint8_t RadioStatus_u::ChipMode

Chip mode.

## ◆ CpuBusy

uint8_t RadioStatus_u::CpuBusy

Flag for CPU radio busy.

## ◆ Fields

struct { ... } RadioStatus_u::Fields

The documentation for this union was generated from the following file:

- src/radio/sx126x/sx126x.h