| SX126x-Arduino 2.0.1

Data Fields
LoraMacHelper_ComplianceTest_s Struct Reference

LoRaWAN compliance tests support data. More...

`#include <LoRaMacHelper.h>`

## Data Fields
bool | running
uint8_t | state
bool | is_tx_confirmed
uint8_t | app_port
uint8_t | data_buffer_size
uint8_t | data_buffer [64]
uint16_t | downlink_counter
bool | link_check
uint8_t | demod_margin
uint8_t | nb_gateways

## Detailed Description

LoRaWAN compliance tests support data.

## Field Documentation

## ◆ running

bool LoraMacHelper_ComplianceTest_s::running

## ◆ state

uint8_t LoraMacHelper_ComplianceTest_s::state

## ◆ is_tx_confirmed

bool LoraMacHelper_ComplianceTest_s::is_tx_confirmed

## ◆ app_port

uint8_t LoraMacHelper_ComplianceTest_s::app_port

## ◆ data_buffer_size

uint8_t LoraMacHelper_ComplianceTest_s::data_buffer_size

## ◆ data_buffer

uint8_t LoraMacHelper_ComplianceTest_s::data_buffer[64]

## ◆ downlink_counter

uint16_t LoraMacHelper_ComplianceTest_s::downlink_counter

## ◆ link_check

bool LoraMacHelper_ComplianceTest_s::link_check

## ◆ demod_margin

uint8_t LoraMacHelper_ComplianceTest_s::demod_margin

## ◆ nb_gateways

uint8_t LoraMacHelper_ComplianceTest_s::nb_gateways

The documentation for this struct was generated from the following file:

- src/mac/LoRaMacHelper.h